<?xml version="1.0" encoding="UTF-8" standalone="no" ?>
<device schemaVersion="1.1" xmlns:xs="http://www.w3.org/2001/XMLSchema-instance" xs:noNamespaceSchemaLocation="CMSIS-SVD_Schema_1_1.xsd">
<name>STM32F303xE</name>
<version>1.0</version>
<description>STM32F303xE</description>
<!--Bus Interface Properties-->
<!--Cortex-M4 is byte addressable-->
<addressUnitBits>8</addressUnitBits>
<!--the maximum data bit width accessible within a single transfer-->
<width>32</width>
<!--Register Default Properties-->
<size>0x20</size>
<resetValue>0x0</resetValue>
<resetMask>0xFFFFFFFF</resetMask>
<peripherals>
<peripheral>
<name>GPIOA</name>
<description>General-purpose I/Os</description>
<groupName>GPIO</groupName>
<baseAddress>0x48000000</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<registers>
<register>
<name>MODER</name>
<displayName>MODER</displayName>
<description>GPIO port mode register</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x28000000</resetValue>
<fields>
<field>
<name>MODER15</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>30</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER14</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>28</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER13</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>26</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER12</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>24</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER11</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>22</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER10</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>20</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER9</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>18</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER8</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>16</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER7</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>14</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER6</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER5</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>10</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER4</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER3</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>6</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER2</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>4</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER1</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER0</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
</fields>
</register>
<register>
<name>OTYPER</name>
<displayName>OTYPER</displayName>
<description>GPIO port output type register</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>OT15</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT14</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT13</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT12</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT11</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT10</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT9</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT8</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT7</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT6</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT5</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT4</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT3</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT2</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT1</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT0</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>OSPEEDR</name>
<displayName>OSPEEDR</displayName>
<description>GPIO port output speed           register</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>OSPEEDR15</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>30</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR14</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>28</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR13</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>26</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR12</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>24</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR11</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>22</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR10</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>20</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR9</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>18</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR8</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>16</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR7</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>14</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR6</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR5</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>10</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR4</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR3</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>6</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR2</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>4</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR1</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR0</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
</fields>
</register>
<register>
<name>PUPDR</name>
<displayName>PUPDR</displayName>
<description>GPIO port pull-up/pull-down           register</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x24000000</resetValue>
<fields>
<field>
<name>PUPDR15</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>30</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR14</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>28</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR13</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>26</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR12</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>24</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR11</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>22</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR10</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>20</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR9</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>18</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR8</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>16</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR7</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>14</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR6</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR5</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>10</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR4</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR3</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>6</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR2</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>4</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR1</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR0</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
</fields>
</register>
<register>
<name>IDR</name>
<displayName>IDR</displayName>
<description>GPIO port input data register</description>
<addressOffset>0x10</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IDR15</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR14</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR13</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR12</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR11</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR10</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR9</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR8</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR7</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR6</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR5</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR4</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR3</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR2</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR1</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR0</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>ODR</name>
<displayName>ODR</displayName>
<description>GPIO port output data register</description>
<addressOffset>0x14</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>ODR15</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR14</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR13</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR12</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR11</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR10</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR9</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR8</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR7</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR6</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR5</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR4</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR3</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR2</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR1</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR0</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>BSRR</name>
<displayName>BSRR</displayName>
<description>GPIO port bit set/reset           register</description>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<access>write-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BR15</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR14</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR13</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR12</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR11</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR10</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR9</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR8</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR7</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR6</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR5</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR4</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR3</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR2</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR1</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR0</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS15</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS14</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS13</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS12</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS11</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS10</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS9</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS8</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS7</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS6</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS5</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS4</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS3</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS2</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS1</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS0</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>LCKR</name>
<displayName>LCKR</displayName>
<description>GPIO port configuration lock           register</description>
<addressOffset>0x1C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>LCKK</name>
<description>Lok Key</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK15</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK14</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK13</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK12</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK11</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK10</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK9</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK8</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK7</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK6</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK5</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK4</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK3</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK2</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK1</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK0</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>AFRL</name>
<displayName>AFRL</displayName>
<description>GPIO alternate function low           register</description>
<addressOffset>0x20</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>AFRL7</name>
<description>Alternate function selection for port x               bit y (y = 0..7)</description>
<bitOffset>28</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRL6</name>
<description>Alternate function selection for port x               bit y (y = 0..7)</description>
<bitOffset>24</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRL5</name>
<description>Alternate function selection for port x               bit y (y = 0..7)</description>
<bitOffset>20</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRL4</name>
<description>Alternate function selection for port x               bit y (y = 0..7)</description>
<bitOffset>16</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRL3</name>
<description>Alternate function selection for port x               bit y (y = 0..7)</description>
<bitOffset>12</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRL2</name>
<description>Alternate function selection for port x               bit y (y = 0..7)</description>
<bitOffset>8</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRL1</name>
<description>Alternate function selection for port x               bit y (y = 0..7)</description>
<bitOffset>4</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRL0</name>
<description>Alternate function selection for port x               bit y (y = 0..7)</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>AFRH</name>
<displayName>AFRH</displayName>
<description>GPIO alternate function high           register</description>
<addressOffset>0x24</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>AFRH15</name>
<description>Alternate function selection for port x               bit y (y = 8..15)</description>
<bitOffset>28</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRH14</name>
<description>Alternate function selection for port x               bit y (y = 8..15)</description>
<bitOffset>24</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRH13</name>
<description>Alternate function selection for port x               bit y (y = 8..15)</description>
<bitOffset>20</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRH12</name>
<description>Alternate function selection for port x               bit y (y = 8..15)</description>
<bitOffset>16</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRH11</name>
<description>Alternate function selection for port x               bit y (y = 8..15)</description>
<bitOffset>12</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRH10</name>
<description>Alternate function selection for port x               bit y (y = 8..15)</description>
<bitOffset>8</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRH9</name>
<description>Alternate function selection for port x               bit y (y = 8..15)</description>
<bitOffset>4</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRH8</name>
<description>Alternate function selection for port x               bit y (y = 8..15)</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>BRR</name>
<displayName>BRR</displayName>
<description>Port bit reset register</description>
<addressOffset>0x28</addressOffset>
<size>0x20</size>
<access>write-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BR0</name>
<description>Port x Reset bit y</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR1</name>
<description>Port x Reset bit y</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR2</name>
<description>Port x Reset bit y</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR3</name>
<description>Port x Reset bit y</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR4</name>
<description>Port x Reset bit y</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR5</name>
<description>Port x Reset bit y</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR6</name>
<description>Port x Reset bit y</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR7</name>
<description>Port x Reset bit y</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR8</name>
<description>Port x Reset bit y</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR9</name>
<description>Port x Reset bit y</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR10</name>
<description>Port x Reset bit y</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR11</name>
<description>Port x Reset bit y</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR12</name>
<description>Port x Reset bit y</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR13</name>
<description>Port x Reset bit y</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR14</name>
<description>Port x Reset bit y</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR15</name>
<description>Port x Reset bit y</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral>
<name>GPIOB</name>
<description>General-purpose I/Os</description>
<groupName>GPIO</groupName>
<baseAddress>0x48000400</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<registers>
<register>
<name>MODER</name>
<displayName>MODER</displayName>
<description>GPIO port mode register</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>MODER15</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>30</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER14</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>28</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER13</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>26</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER12</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>24</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER11</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>22</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER10</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>20</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER9</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>18</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER8</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>16</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER7</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>14</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER6</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER5</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>10</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER4</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER3</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>6</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER2</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>4</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER1</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MODER0</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
</fields>
</register>
<register>
<name>OTYPER</name>
<displayName>OTYPER</displayName>
<description>GPIO port output type register</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>OT15</name>
<description>Port x configuration bit               15</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT14</name>
<description>Port x configuration bit               14</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT13</name>
<description>Port x configuration bit               13</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT12</name>
<description>Port x configuration bit               12</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT11</name>
<description>Port x configuration bit               11</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT10</name>
<description>Port x configuration bit               10</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT9</name>
<description>Port x configuration bit 9</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT8</name>
<description>Port x configuration bit 8</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT7</name>
<description>Port x configuration bit 7</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT6</name>
<description>Port x configuration bit 6</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT5</name>
<description>Port x configuration bit 5</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT4</name>
<description>Port x configuration bit 4</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT3</name>
<description>Port x configuration bit 3</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT2</name>
<description>Port x configuration bit 2</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT1</name>
<description>Port x configuration bit 1</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OT0</name>
<description>Port x configuration bit 0</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>OSPEEDR</name>
<displayName>OSPEEDR</displayName>
<description>GPIO port output speed           register</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>OSPEEDR15</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>30</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR14</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>28</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR13</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>26</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR12</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>24</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR11</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>22</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR10</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>20</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR9</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>18</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR8</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>16</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR7</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>14</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR6</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR5</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>10</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR4</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR3</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>6</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR2</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>4</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR1</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSPEEDR0</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
</fields>
</register>
<register>
<name>PUPDR</name>
<displayName>PUPDR</displayName>
<description>GPIO port pull-up/pull-down           register</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>PUPDR15</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>30</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR14</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>28</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR13</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>26</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR12</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>24</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR11</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>22</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR10</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>20</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR9</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>18</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR8</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>16</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR7</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>14</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR6</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR5</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>10</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR4</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR3</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>6</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR2</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>4</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR1</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PUPDR0</name>
<description>Port x configuration bits (y =               0..15)</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
</fields>
</register>
<register>
<name>IDR</name>
<displayName>IDR</displayName>
<description>GPIO port input data register</description>
<addressOffset>0x10</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IDR15</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR14</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR13</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR12</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR11</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR10</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR9</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR8</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR7</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR6</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR5</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR4</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR3</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR2</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR1</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDR0</name>
<description>Port input data (y =               0..15)</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>ODR</name>
<displayName>ODR</displayName>
<description>GPIO port output data register</description>
<addressOffset>0x14</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>ODR15</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR14</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR13</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR12</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR11</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR10</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR9</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR8</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR7</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR6</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR5</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR4</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR3</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR2</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR1</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODR0</name>
<description>Port output data (y =               0..15)</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>BSRR</name>
<displayName>BSRR</displayName>
<description>GPIO port bit set/reset           register</description>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<access>write-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BR15</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR14</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR13</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR12</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR11</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR10</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR9</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR8</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR7</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR6</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR5</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR4</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR3</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR2</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR1</name>
<description>Port x reset bit y (y =               0..15)</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR0</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS15</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS14</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS13</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS12</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS11</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS10</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS9</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS8</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS7</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS6</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS5</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS4</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS3</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS2</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS1</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BS0</name>
<description>Port x set bit y (y=               0..15)</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>LCKR</name>
<displayName>LCKR</displayName>
<description>GPIO port configuration lock           register</description>
<addressOffset>0x1C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>LCKK</name>
<description>Lok Key</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK15</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK14</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK13</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK12</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK11</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK10</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK9</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK8</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK7</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK6</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK5</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK4</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK3</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK2</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK1</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LCK0</name>
<description>Port x lock bit y (y=               0..15)</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>AFRL</name>
<displayName>AFRL</displayName>
<description>GPIO alternate function low           register</description>
<addressOffset>0x20</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>AFRL7</name>
<description>Alternate function selection for port x               bit y (y = 0..7)</description>
<bitOffset>28</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRL6</name>
<description>Alternate function selection for port x               bit y (y = 0..7)</description>
<bitOffset>24</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRL5</name>
<description>Alternate function selection for port x               bit y (y = 0..7)</description>
<bitOffset>20</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRL4</name>
<description>Alternate function selection for port x               bit y (y = 0..7)</description>
<bitOffset>16</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRL3</name>
<description>Alternate function selection for port x               bit y (y = 0..7)</description>
<bitOffset>12</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRL2</name>
<description>Alternate function selection for port x               bit y (y = 0..7)</description>
<bitOffset>8</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRL1</name>
<description>Alternate function selection for port x               bit y (y = 0..7)</description>
<bitOffset>4</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRL0</name>
<description>Alternate function selection for port x               bit y (y = 0..7)</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>AFRH</name>
<displayName>AFRH</displayName>
<description>GPIO alternate function high           register</description>
<addressOffset>0x24</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>AFRH15</name>
<description>Alternate function selection for port x               bit y (y = 8..15)</description>
<bitOffset>28</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRH14</name>
<description>Alternate function selection for port x               bit y (y = 8..15)</description>
<bitOffset>24</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRH13</name>
<description>Alternate function selection for port x               bit y (y = 8..15)</description>
<bitOffset>20</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRH12</name>
<description>Alternate function selection for port x               bit y (y = 8..15)</description>
<bitOffset>16</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRH11</name>
<description>Alternate function selection for port x               bit y (y = 8..15)</description>
<bitOffset>12</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRH10</name>
<description>Alternate function selection for port x               bit y (y = 8..15)</description>
<bitOffset>8</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRH9</name>
<description>Alternate function selection for port x               bit y (y = 8..15)</description>
<bitOffset>4</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>AFRH8</name>
<description>Alternate function selection for port x               bit y (y = 8..15)</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>BRR</name>
<displayName>BRR</displayName>
<description>Port bit reset register</description>
<addressOffset>0x28</addressOffset>
<size>0x20</size>
<access>write-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BR0</name>
<description>Port x Reset bit y</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR1</name>
<description>Port x Reset bit y</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR2</name>
<description>Port x Reset bit y</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR3</name>
<description>Port x Reset bit y</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR4</name>
<description>Port x Reset bit y</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR5</name>
<description>Port x Reset bit y</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR6</name>
<description>Port x Reset bit y</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR7</name>
<description>Port x Reset bit y</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR8</name>
<description>Port x Reset bit y</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR9</name>
<description>Port x Reset bit y</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR10</name>
<description>Port x Reset bit y</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR11</name>
<description>Port x Reset bit y</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR12</name>
<description>Port x Reset bit y</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR13</name>
<description>Port x Reset bit y</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR14</name>
<description>Port x Reset bit y</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR15</name>
<description>Port x Reset bit y</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral derivedFrom="GPIOB">
<name>GPIOC</name>
<baseAddress>0x48000800</baseAddress>
</peripheral>
<peripheral derivedFrom="GPIOB">
<name>GPIOD</name>
<baseAddress>0x48000C00</baseAddress>
</peripheral>
<peripheral derivedFrom="GPIOB">
<name>GPIOE</name>
<baseAddress>0x48001000</baseAddress>
</peripheral>
<peripheral derivedFrom="GPIOB">
<name>GPIOF</name>
<baseAddress>0x48001400</baseAddress>
</peripheral>
<peripheral derivedFrom="GPIOB">
<name>GPIOG</name>
<baseAddress>0x48001800</baseAddress>
</peripheral>
<peripheral derivedFrom="GPIOB">
<name>GPIOH</name>
<baseAddress>0x48001C00</baseAddress>
</peripheral>
<peripheral>
<name>TSC</name>
<description>Touch sensing controller</description>
<groupName>TSC</groupName>
<baseAddress>0x40024000</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<interrupt>
<name>EXTI2_TSC</name>
<description>EXTI Line2 and Touch sensing
        interrupts</description>
<value>8</value>
</interrupt>
<registers>
<register>
<name>CR</name>
<displayName>CR</displayName>
<description>control register</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CTPH</name>
<description>Charge transfer pulse high</description>
<bitOffset>28</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>CTPL</name>
<description>Charge transfer pulse low</description>
<bitOffset>24</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>SSD</name>
<description>Spread spectrum deviation</description>
<bitOffset>17</bitOffset>
<bitWidth>7</bitWidth>
</field>
<field>
<name>SSE</name>
<description>Spread spectrum enable</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SSPSC</name>
<description>Spread spectrum prescaler</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PGPSC</name>
<description>pulse generator prescaler</description>
<bitOffset>12</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>MCV</name>
<description>Max count value</description>
<bitOffset>5</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>IODEF</name>
<description>I/O Default mode</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SYNCPOL</name>
<description>Synchronization pin               polarity</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>AM</name>
<description>Acquisition mode</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>START</name>
<description>Start a new acquisition</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TSCE</name>
<description>Touch sensing controller               enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>IER</name>
<displayName>IER</displayName>
<description>interrupt enable register</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>MCEIE</name>
<description>Max count error interrupt               enable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>EOAIE</name>
<description>End of acquisition interrupt               enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>ICR</name>
<displayName>ICR</displayName>
<description>interrupt clear register</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>MCEIC</name>
<description>Max count error interrupt               clear</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>EOAIC</name>
<description>End of acquisition interrupt               clear</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>ISR</name>
<displayName>ISR</displayName>
<description>interrupt status register</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>MCEF</name>
<description>Max count error flag</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>EOAF</name>
<description>End of acquisition flag</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>IOHCR</name>
<displayName>IOHCR</displayName>
<description>I/O hysteresis control           register</description>
<addressOffset>0x10</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0xFFFFFFFF</resetValue>
<fields>
<field>
<name>G1_IO1</name>
<description>G1_IO1 Schmitt trigger hysteresis               mode</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G1_IO2</name>
<description>G1_IO2 Schmitt trigger hysteresis               mode</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G1_IO3</name>
<description>G1_IO3 Schmitt trigger hysteresis               mode</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G1_IO4</name>
<description>G1_IO4 Schmitt trigger hysteresis               mode</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G2_IO1</name>
<description>G2_IO1 Schmitt trigger hysteresis               mode</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G2_IO2</name>
<description>G2_IO2 Schmitt trigger hysteresis               mode</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G2_IO3</name>
<description>G2_IO3 Schmitt trigger hysteresis               mode</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G2_IO4</name>
<description>G2_IO4 Schmitt trigger hysteresis               mode</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G3_IO1</name>
<description>G3_IO1 Schmitt trigger hysteresis               mode</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G3_IO2</name>
<description>G3_IO2 Schmitt trigger hysteresis               mode</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G3_IO3</name>
<description>G3_IO3 Schmitt trigger hysteresis               mode</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G3_IO4</name>
<description>G3_IO4 Schmitt trigger hysteresis               mode</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G4_IO1</name>
<description>G4_IO1 Schmitt trigger hysteresis               mode</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G4_IO2</name>
<description>G4_IO2 Schmitt trigger hysteresis               mode</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G4_IO3</name>
<description>G4_IO3 Schmitt trigger hysteresis               mode</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G4_IO4</name>
<description>G4_IO4 Schmitt trigger hysteresis               mode</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G5_IO1</name>
<description>G5_IO1 Schmitt trigger hysteresis               mode</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G5_IO2</name>
<description>G5_IO2 Schmitt trigger hysteresis               mode</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G5_IO3</name>
<description>G5_IO3 Schmitt trigger hysteresis               mode</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G5_IO4</name>
<description>G5_IO4 Schmitt trigger hysteresis               mode</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G6_IO1</name>
<description>G6_IO1 Schmitt trigger hysteresis               mode</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G6_IO2</name>
<description>G6_IO2 Schmitt trigger hysteresis               mode</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G6_IO3</name>
<description>G6_IO3 Schmitt trigger hysteresis               mode</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G6_IO4</name>
<description>G6_IO4 Schmitt trigger hysteresis               mode</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G7_IO1</name>
<description>G7_IO1 Schmitt trigger hysteresis               mode</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G7_IO2</name>
<description>G7_IO2 Schmitt trigger hysteresis               mode</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G7_IO3</name>
<description>G7_IO3 Schmitt trigger hysteresis               mode</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G7_IO4</name>
<description>G7_IO4 Schmitt trigger hysteresis               mode</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G8_IO1</name>
<description>G8_IO1 Schmitt trigger hysteresis               mode</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G8_IO2</name>
<description>G8_IO2 Schmitt trigger hysteresis               mode</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G8_IO3</name>
<description>G8_IO3 Schmitt trigger hysteresis               mode</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G8_IO4</name>
<description>G8_IO4 Schmitt trigger hysteresis               mode</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>IOASCR</name>
<displayName>IOASCR</displayName>
<description>I/O analog switch control           register</description>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>G1_IO1</name>
<description>G1_IO1 analog switch               enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G1_IO2</name>
<description>G1_IO2 analog switch               enable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G1_IO3</name>
<description>G1_IO3 analog switch               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G1_IO4</name>
<description>G1_IO4 analog switch               enable</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G2_IO1</name>
<description>G2_IO1 analog switch               enable</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G2_IO2</name>
<description>G2_IO2 analog switch               enable</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G2_IO3</name>
<description>G2_IO3 analog switch               enable</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G2_IO4</name>
<description>G2_IO4 analog switch               enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G3_IO1</name>
<description>G3_IO1 analog switch               enable</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G3_IO2</name>
<description>G3_IO2 analog switch               enable</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G3_IO3</name>
<description>G3_IO3 analog switch               enable</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G3_IO4</name>
<description>G3_IO4 analog switch               enable</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G4_IO1</name>
<description>G4_IO1 analog switch               enable</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G4_IO2</name>
<description>G4_IO2 analog switch               enable</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G4_IO3</name>
<description>G4_IO3 analog switch               enable</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G4_IO4</name>
<description>G4_IO4 analog switch               enable</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G5_IO1</name>
<description>G5_IO1 analog switch               enable</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G5_IO2</name>
<description>G5_IO2 analog switch               enable</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G5_IO3</name>
<description>G5_IO3 analog switch               enable</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G5_IO4</name>
<description>G5_IO4 analog switch               enable</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G6_IO1</name>
<description>G6_IO1 analog switch               enable</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G6_IO2</name>
<description>G6_IO2 analog switch               enable</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G6_IO3</name>
<description>G6_IO3 analog switch               enable</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G6_IO4</name>
<description>G6_IO4 analog switch               enable</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G7_IO1</name>
<description>G7_IO1 analog switch               enable</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G7_IO2</name>
<description>G7_IO2 analog switch               enable</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G7_IO3</name>
<description>G7_IO3 analog switch               enable</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G7_IO4</name>
<description>G7_IO4 analog switch               enable</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G8_IO1</name>
<description>G8_IO1 analog switch               enable</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G8_IO2</name>
<description>G8_IO2 analog switch               enable</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G8_IO3</name>
<description>G8_IO3 analog switch               enable</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G8_IO4</name>
<description>G8_IO4 analog switch               enable</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>IOSCR</name>
<displayName>IOSCR</displayName>
<description>I/O sampling control register</description>
<addressOffset>0x20</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>G1_IO1</name>
<description>G1_IO1 sampling mode</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G1_IO2</name>
<description>G1_IO2 sampling mode</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G1_IO3</name>
<description>G1_IO3 sampling mode</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G1_IO4</name>
<description>G1_IO4 sampling mode</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G2_IO1</name>
<description>G2_IO1 sampling mode</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G2_IO2</name>
<description>G2_IO2 sampling mode</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G2_IO3</name>
<description>G2_IO3 sampling mode</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G2_IO4</name>
<description>G2_IO4 sampling mode</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G3_IO1</name>
<description>G3_IO1 sampling mode</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G3_IO2</name>
<description>G3_IO2 sampling mode</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G3_IO3</name>
<description>G3_IO3 sampling mode</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G3_IO4</name>
<description>G3_IO4 sampling mode</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G4_IO1</name>
<description>G4_IO1 sampling mode</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G4_IO2</name>
<description>G4_IO2 sampling mode</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G4_IO3</name>
<description>G4_IO3 sampling mode</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G4_IO4</name>
<description>G4_IO4 sampling mode</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G5_IO1</name>
<description>G5_IO1 sampling mode</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G5_IO2</name>
<description>G5_IO2 sampling mode</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G5_IO3</name>
<description>G5_IO3 sampling mode</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G5_IO4</name>
<description>G5_IO4 sampling mode</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G6_IO1</name>
<description>G6_IO1 sampling mode</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G6_IO2</name>
<description>G6_IO2 sampling mode</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G6_IO3</name>
<description>G6_IO3 sampling mode</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G6_IO4</name>
<description>G6_IO4 sampling mode</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G7_IO1</name>
<description>G7_IO1 sampling mode</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G7_IO2</name>
<description>G7_IO2 sampling mode</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G7_IO3</name>
<description>G7_IO3 sampling mode</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G7_IO4</name>
<description>G7_IO4 sampling mode</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G8_IO1</name>
<description>G8_IO1 sampling mode</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G8_IO2</name>
<description>G8_IO2 sampling mode</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G8_IO3</name>
<description>G8_IO3 sampling mode</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G8_IO4</name>
<description>G8_IO4 sampling mode</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>IOCCR</name>
<displayName>IOCCR</displayName>
<description>I/O channel control register</description>
<addressOffset>0x28</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>G1_IO1</name>
<description>G1_IO1 channel mode</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G1_IO2</name>
<description>G1_IO2 channel mode</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G1_IO3</name>
<description>G1_IO3 channel mode</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G1_IO4</name>
<description>G1_IO4 channel mode</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G2_IO1</name>
<description>G2_IO1 channel mode</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G2_IO2</name>
<description>G2_IO2 channel mode</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G2_IO3</name>
<description>G2_IO3 channel mode</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G2_IO4</name>
<description>G2_IO4 channel mode</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G3_IO1</name>
<description>G3_IO1 channel mode</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G3_IO2</name>
<description>G3_IO2 channel mode</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G3_IO3</name>
<description>G3_IO3 channel mode</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G3_IO4</name>
<description>G3_IO4 channel mode</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G4_IO1</name>
<description>G4_IO1 channel mode</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G4_IO2</name>
<description>G4_IO2 channel mode</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G4_IO3</name>
<description>G4_IO3 channel mode</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G4_IO4</name>
<description>G4_IO4 channel mode</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G5_IO1</name>
<description>G5_IO1 channel mode</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G5_IO2</name>
<description>G5_IO2 channel mode</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G5_IO3</name>
<description>G5_IO3 channel mode</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G5_IO4</name>
<description>G5_IO4 channel mode</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G6_IO1</name>
<description>G6_IO1 channel mode</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G6_IO2</name>
<description>G6_IO2 channel mode</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G6_IO3</name>
<description>G6_IO3 channel mode</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G6_IO4</name>
<description>G6_IO4 channel mode</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G7_IO1</name>
<description>G7_IO1 channel mode</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G7_IO2</name>
<description>G7_IO2 channel mode</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G7_IO3</name>
<description>G7_IO3 channel mode</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G7_IO4</name>
<description>G7_IO4 channel mode</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G8_IO1</name>
<description>G8_IO1 channel mode</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G8_IO2</name>
<description>G8_IO2 channel mode</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G8_IO3</name>
<description>G8_IO3 channel mode</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>G8_IO4</name>
<description>G8_IO4 channel mode</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>IOGCSR</name>
<displayName>IOGCSR</displayName>
<description>I/O group control status           register</description>
<addressOffset>0x30</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>G8S</name>
<description>Analog I/O group x status</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>G7S</name>
<description>Analog I/O group x status</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>G6S</name>
<description>Analog I/O group x status</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>G5S</name>
<description>Analog I/O group x status</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>G4S</name>
<description>Analog I/O group x status</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>G3S</name>
<description>Analog I/O group x status</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>G2S</name>
<description>Analog I/O group x status</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>G1S</name>
<description>Analog I/O group x status</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>G8E</name>
<description>Analog I/O group x enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>G7E</name>
<description>Analog I/O group x enable</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>G6E</name>
<description>Analog I/O group x enable</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>G5E</name>
<description>Analog I/O group x enable</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>G4E</name>
<description>Analog I/O group x enable</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>G3E</name>
<description>Analog I/O group x enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>G2E</name>
<description>Analog I/O group x enable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>G1E</name>
<description>Analog I/O group x enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
<register>
<name>IOG1CR</name>
<displayName>IOG1CR</displayName>
<description>I/O group x counter register</description>
<addressOffset>0x34</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CNT</name>
<description>Counter value</description>
<bitOffset>0</bitOffset>
<bitWidth>14</bitWidth>
</field>
</fields>
</register>
<register>
<name>IOG2CR</name>
<displayName>IOG2CR</displayName>
<description>I/O group x counter register</description>
<addressOffset>0x38</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CNT</name>
<description>Counter value</description>
<bitOffset>0</bitOffset>
<bitWidth>14</bitWidth>
</field>
</fields>
</register>
<register>
<name>IOG3CR</name>
<displayName>IOG3CR</displayName>
<description>I/O group x counter register</description>
<addressOffset>0x3C</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CNT</name>
<description>Counter value</description>
<bitOffset>0</bitOffset>
<bitWidth>14</bitWidth>
</field>
</fields>
</register>
<register>
<name>IOG4CR</name>
<displayName>IOG4CR</displayName>
<description>I/O group x counter register</description>
<addressOffset>0x40</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CNT</name>
<description>Counter value</description>
<bitOffset>0</bitOffset>
<bitWidth>14</bitWidth>
</field>
</fields>
</register>
<register>
<name>IOG5CR</name>
<displayName>IOG5CR</displayName>
<description>I/O group x counter register</description>
<addressOffset>0x44</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CNT</name>
<description>Counter value</description>
<bitOffset>0</bitOffset>
<bitWidth>14</bitWidth>
</field>
</fields>
</register>
<register>
<name>IOG6CR</name>
<displayName>IOG6CR</displayName>
<description>I/O group x counter register</description>
<addressOffset>0x48</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CNT</name>
<description>Counter value</description>
<bitOffset>0</bitOffset>
<bitWidth>14</bitWidth>
</field>
</fields>
</register>
<register>
<name>IOG7CR</name>
<displayName>IOG7CR</displayName>
<description>I/O group x counter register</description>
<addressOffset>0x4C</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CNT</name>
<description>Counter value</description>
<bitOffset>0</bitOffset>
<bitWidth>14</bitWidth>
</field>
</fields>
</register>
<register>
<name>IOG8CR</name>
<displayName>IOG8CR</displayName>
<description>I/O group x counter register</description>
<addressOffset>0x50</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CNT</name>
<description>Counter value</description>
<bitOffset>0</bitOffset>
<bitWidth>14</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral>
<name>CRC</name>
<description>cyclic redundancy check calculation       unit</description>
<groupName>CRC</groupName>
<baseAddress>0x40023000</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<registers>
<register>
<name>DR</name>
<displayName>DR</displayName>
<description>Data register</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0xFFFFFFFF</resetValue>
<fields>
<field>
<name>DR</name>
<description>Data register bits</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>IDR</name>
<displayName>IDR</displayName>
<description>Independent data register</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IDR</name>
<description>General-purpose 8-bit data register               bits</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>CR</name>
<displayName>CR</displayName>
<description>Control register</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>RESET</name>
<description>reset bit</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>POLYSIZE</name>
<description>Polynomial size</description>
<bitOffset>3</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>REV_IN</name>
<description>Reverse input data</description>
<bitOffset>5</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>REV_OUT</name>
<description>Reverse output data</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>INIT</name>
<displayName>INIT</displayName>
<description>Initial CRC value</description>
<addressOffset>0x10</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0xFFFFFFFF</resetValue>
<fields>
<field>
<name>INIT</name>
<description>Programmable initial CRC               value</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>POL</name>
<displayName>POL</displayName>
<description>CRC polynomial</description>
<addressOffset>0x14</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x04C11DB7</resetValue>
<fields>
<field>
<name>POL</name>
<description>Programmable polynomial</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral>
<name>Flash</name>
<description>Flash</description>
<groupName>Flash</groupName>
<baseAddress>0x40022000</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<interrupt>
<name>FLASH</name>
<description>Flash global interrupt</description>
<value>4</value>
</interrupt>
<registers>
<register>
<name>ACR</name>
<displayName>ACR</displayName>
<description>Flash access control register</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<resetValue>0x00000030</resetValue>
<fields>
<field>
<name>LATENCY</name>
<description>LATENCY</description>
<bitOffset>0</bitOffset>
<bitWidth>3</bitWidth>
<access>read-write</access>
</field>
<field>
<name>PRFTBE</name>
<description>PRFTBE</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>PRFTBS</name>
<description>PRFTBS</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
</fields>
</register>
<register>
<name>KEYR</name>
<displayName>KEYR</displayName>
<description>Flash key register</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>write-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FKEYR</name>
<description>Flash Key</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>OPTKEYR</name>
<displayName>OPTKEYR</displayName>
<description>Flash option key register</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<access>write-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>OPTKEYR</name>
<description>Option byte key</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>SR</name>
<displayName>SR</displayName>
<description>Flash status register</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>EOP</name>
<description>End of operation</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>WRPRT</name>
<description>Write protection error</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>PGERR</name>
<description>Programming error</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>BSY</name>
<description>Busy</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
</fields>
</register>
<register>
<name>CR</name>
<displayName>CR</displayName>
<description>Flash control register</description>
<addressOffset>0x10</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000080</resetValue>
<fields>
<field>
<name>FORCE_OPTLOAD</name>
<description>Force option byte loading</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>EOPIE</name>
<description>End of operation interrupt               enable</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ERRIE</name>
<description>Error interrupt enable</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OPTWRE</name>
<description>Option bytes write enable</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LOCK</name>
<description>Lock</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>STRT</name>
<description>Start</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OPTER</name>
<description>Option byte erase</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OPTPG</name>
<description>Option byte programming</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MER</name>
<description>Mass erase</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PER</name>
<description>Page erase</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PG</name>
<description>Programming</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>AR</name>
<displayName>AR</displayName>
<description>Flash address register</description>
<addressOffset>0x14</addressOffset>
<size>0x20</size>
<access>write-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FAR</name>
<description>Flash address</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>OBR</name>
<displayName>OBR</displayName>
<description>Option byte register</description>
<addressOffset>0x1C</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0xFFFFFF02</resetValue>
<fields>
<field>
<name>OPTERR</name>
<description>Option byte error</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LEVEL1_PROT</name>
<description>Level 1 protection status</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LEVEL2_PROT</name>
<description>Level 2 protection status</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>WDG_SW</name>
<description>WDG_SW</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>nRST_STOP</name>
<description>nRST_STOP</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>nRST_STDBY</name>
<description>nRST_STDBY</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BOOT1</name>
<description>BOOT1</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>VDDA_MONITOR</name>
<description>VDDA_MONITOR</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SRAM_PARITY_CHECK</name>
<description>SRAM_PARITY_CHECK</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>Data0</name>
<description>Data0</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>Data1</name>
<description>Data1</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>WRPR</name>
<displayName>WRPR</displayName>
<description>Write protection register</description>
<addressOffset>0x20</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0xFFFFFFFF</resetValue>
<fields>
<field>
<name>WRP</name>
<description>Write protect</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral>
<name>RCC</name>
<description>Reset and clock control</description>
<groupName>RCC</groupName>
<baseAddress>0x40021000</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<interrupt>
<name>RCC</name>
<description>RCC global interrupt</description>
<value>5</value>
</interrupt>
<registers>
<register>
<name>CR</name>
<displayName>CR</displayName>
<description>Clock control register</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<resetValue>0x00000083</resetValue>
<fields>
<field>
<name>HSION</name>
<description>Internal High Speed clock               enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>HSIRDY</name>
<description>Internal High Speed clock ready               flag</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>HSITRIM</name>
<description>Internal High Speed clock               trimming</description>
<bitOffset>3</bitOffset>
<bitWidth>5</bitWidth>
<access>read-write</access>
</field>
<field>
<name>HSICAL</name>
<description>Internal High Speed clock               Calibration</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
<access>read-only</access>
</field>
<field>
<name>HSEON</name>
<description>External High Speed clock               enable</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>HSERDY</name>
<description>External High Speed clock ready               flag</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>HSEBYP</name>
<description>External High Speed clock               Bypass</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CSSON</name>
<description>Clock Security System               enable</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>PLLON</name>
<description>PLL enable</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>PLLRDY</name>
<description>PLL clock ready flag</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
</fields>
</register>
<register>
<name>CFGR</name>
<displayName>CFGR</displayName>
<description>Clock configuration register           (RCC_CFGR)</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>SW</name>
<description>System clock Switch</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>SWS</name>
<description>System Clock Switch Status</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
<access>read-only</access>
</field>
<field>
<name>HPRE</name>
<description>AHB prescaler</description>
<bitOffset>4</bitOffset>
<bitWidth>4</bitWidth>
<access>read-write</access>
</field>
<field>
<name>PPRE1</name>
<description>APB Low speed prescaler               (APB1)</description>
<bitOffset>8</bitOffset>
<bitWidth>3</bitWidth>
<access>read-write</access>
</field>
<field>
<name>PPRE2</name>
<description>APB high speed prescaler               (APB2)</description>
<bitOffset>11</bitOffset>
<bitWidth>3</bitWidth>
<access>read-write</access>
</field>
<field>
<name>PLLSRC</name>
<description>PLL entry clock source</description>
<bitOffset>15</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>PLLXTPRE</name>
<description>HSE divider for PLL entry</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>PLLMUL</name>
<description>PLL Multiplication Factor</description>
<bitOffset>18</bitOffset>
<bitWidth>4</bitWidth>
<access>read-write</access>
</field>
<field>
<name>USBPRES</name>
<description>USB prescaler</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>MCO</name>
<description>Microcontroller clock               output</description>
<bitOffset>24</bitOffset>
<bitWidth>3</bitWidth>
<access>read-write</access>
</field>
<field>
<name>MCOF</name>
<description>Microcontroller Clock Output               Flag</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>I2SSRC</name>
<description>I2S external clock source               selection</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
<register>
<name>CIR</name>
<displayName>CIR</displayName>
<description>Clock interrupt register           (RCC_CIR)</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>LSIRDYF</name>
<description>LSI Ready Interrupt flag</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>LSERDYF</name>
<description>LSE Ready Interrupt flag</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>HSIRDYF</name>
<description>HSI Ready Interrupt flag</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>HSERDYF</name>
<description>HSE Ready Interrupt flag</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>PLLRDYF</name>
<description>PLL Ready Interrupt flag</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>CSSF</name>
<description>Clock Security System Interrupt               flag</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>LSIRDYIE</name>
<description>LSI Ready Interrupt Enable</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>LSERDYIE</name>
<description>LSE Ready Interrupt Enable</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>HSIRDYIE</name>
<description>HSI Ready Interrupt Enable</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>HSERDYIE</name>
<description>HSE Ready Interrupt Enable</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>PLLRDYIE</name>
<description>PLL Ready Interrupt Enable</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>LSIRDYC</name>
<description>LSI Ready Interrupt Clear</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
<access>write-only</access>
</field>
<field>
<name>LSERDYC</name>
<description>LSE Ready Interrupt Clear</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
<access>write-only</access>
</field>
<field>
<name>HSIRDYC</name>
<description>HSI Ready Interrupt Clear</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
<access>write-only</access>
</field>
<field>
<name>HSERDYC</name>
<description>HSE Ready Interrupt Clear</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
<access>write-only</access>
</field>
<field>
<name>PLLRDYC</name>
<description>PLL Ready Interrupt Clear</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
<access>write-only</access>
</field>
<field>
<name>CSSC</name>
<description>Clock security system interrupt               clear</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
<access>write-only</access>
</field>
</fields>
</register>
<register>
<name>APB2RSTR</name>
<displayName>APB2RSTR</displayName>
<description>APB2 peripheral reset register           (RCC_APB2RSTR)</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>SYSCFGRST</name>
<description>SYSCFG and COMP reset</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIM1RST</name>
<description>TIM1 timer reset</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SPI1RST</name>
<description>SPI 1 reset</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIM8RST</name>
<description>TIM8 timer reset</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>USART1RST</name>
<description>USART1 reset</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIM15RST</name>
<description>TIM15 timer reset</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIM16RST</name>
<description>TIM16 timer reset</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIM17RST</name>
<description>TIM17 timer reset</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>APB1RSTR</name>
<displayName>APB1RSTR</displayName>
<description>APB1 peripheral reset register           (RCC_APB1RSTR)</description>
<addressOffset>0x10</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>TIM2RST</name>
<description>Timer 2 reset</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIM3RST</name>
<description>Timer 3 reset</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIM4RST</name>
<description>Timer 14 reset</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIM6RST</name>
<description>Timer 6 reset</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIM7RST</name>
<description>Timer 7 reset</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>WWDGRST</name>
<description>Window watchdog reset</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SPI2RST</name>
<description>SPI2 reset</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SPI3RST</name>
<description>SPI3 reset</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>USART2RST</name>
<description>USART 2 reset</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>USART3RST</name>
<description>USART3 reset</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UART4RST</name>
<description>UART 4 reset</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UART5RST</name>
<description>UART 5 reset</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>I2C1RST</name>
<description>I2C1 reset</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>I2C2RST</name>
<description>I2C2 reset</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>USBRST</name>
<description>USB reset</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CANRST</name>
<description>CAN reset</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PWRRST</name>
<description>Power interface reset</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DACRST</name>
<description>DAC interface reset</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>I2C3RST</name>
<description>I2C3 reset</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>AHBENR</name>
<displayName>AHBENR</displayName>
<description>AHB Peripheral Clock enable register           (RCC_AHBENR)</description>
<addressOffset>0x14</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000014</resetValue>
<fields>
<field>
<name>DMAEN</name>
<description>DMA1 clock enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DMA2EN</name>
<description>DMA2 clock enable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SRAMEN</name>
<description>SRAM interface clock               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FLITFEN</name>
<description>FLITF clock enable</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CRCEN</name>
<description>CRC clock enable</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IOPHEN</name>
<description>I/O port H clock enable</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IOPAEN</name>
<description>I/O port A clock enable</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IOPBEN</name>
<description>I/O port B clock enable</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IOPCEN</name>
<description>I/O port C clock enable</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IOPDEN</name>
<description>I/O port D clock enable</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IOPEEN</name>
<description>I/O port E clock enable</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IOPFEN</name>
<description>I/O port F clock enable</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IOPGEN</name>
<description>I/O port G clock enable</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TSCEN</name>
<description>Touch sensing controller clock               enable</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ADC12EN</name>
<description>ADC1 and ADC2 clock enable</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ADC34EN</name>
<description>ADC3 and ADC4 clock enable</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>APB2ENR</name>
<displayName>APB2ENR</displayName>
<description>APB2 peripheral clock enable register           (RCC_APB2ENR)</description>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>SYSCFGEN</name>
<description>SYSCFG clock enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIM1EN</name>
<description>TIM1 Timer clock enable</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SPI1EN</name>
<description>SPI 1 clock enable</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIM8EN</name>
<description>TIM8 Timer clock enable</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>USART1EN</name>
<description>USART1 clock enable</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIM15EN</name>
<description>TIM15 timer clock enable</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIM16EN</name>
<description>TIM16 timer clock enable</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIM17EN</name>
<description>TIM17 timer clock enable</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>APB1ENR</name>
<displayName>APB1ENR</displayName>
<description>APB1 peripheral clock enable register           (RCC_APB1ENR)</description>
<addressOffset>0x1C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>TIM2EN</name>
<description>Timer 2 clock enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIM3EN</name>
<description>Timer 3 clock enable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIM4EN</name>
<description>Timer 4 clock enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIM6EN</name>
<description>Timer 6 clock enable</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIM7EN</name>
<description>Timer 7 clock enable</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>WWDGEN</name>
<description>Window watchdog clock               enable</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SPI2EN</name>
<description>SPI 2 clock enable</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SPI3EN</name>
<description>SPI 3 clock enable</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>USART2EN</name>
<description>USART 2 clock enable</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>USART3EN</name>
<description>USART 3 clock enable</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UART4EN</name>
<description>UART 4 clock enable</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UART5EN</name>
<description>UART 5 clock enable</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>I2C1EN</name>
<description>I2C 1 clock enable</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>I2C2EN</name>
<description>I2C 2 clock enable</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>USBEN</name>
<description>USB clock enable</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CANEN</name>
<description>CAN clock enable</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PWREN</name>
<description>Power interface clock               enable</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DACEN</name>
<description>DAC interface clock enable</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>I2C3EN</name>
<description>I2C 3 clock enable</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>BDCR</name>
<displayName>BDCR</displayName>
<description>Backup domain control register           (RCC_BDCR)</description>
<addressOffset>0x20</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>LSEON</name>
<description>External Low Speed oscillator               enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>LSERDY</name>
<description>External Low Speed oscillator               ready</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>LSEBYP</name>
<description>External Low Speed oscillator               bypass</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>LSEDRV</name>
<description>LSE oscillator drive               capability</description>
<bitOffset>3</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>RTCSEL</name>
<description>RTC clock source selection</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>RTCEN</name>
<description>RTC clock enable</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>BDRST</name>
<description>Backup domain software               reset</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
<register>
<name>CSR</name>
<displayName>CSR</displayName>
<description>Control/status register           (RCC_CSR)</description>
<addressOffset>0x24</addressOffset>
<size>0x20</size>
<resetValue>0x0C000000</resetValue>
<fields>
<field>
<name>LSION</name>
<description>Internal low speed oscillator               enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>LSIRDY</name>
<description>Internal low speed oscillator               ready</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>RMVF</name>
<description>Remove reset flag</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>OBLRSTF</name>
<description>Option byte loader reset               flag</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>PINRSTF</name>
<description>PIN reset flag</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>PORRSTF</name>
<description>POR/PDR reset flag</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>SFTRSTF</name>
<description>Software reset flag</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>IWDGRSTF</name>
<description>Independent watchdog reset               flag</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>WWDGRSTF</name>
<description>Window watchdog reset flag</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>LPWRRSTF</name>
<description>Low-power reset flag</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
<register>
<name>AHBRSTR</name>
<displayName>AHBRSTR</displayName>
<description>AHB peripheral reset register</description>
<addressOffset>0x28</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IOPHRST</name>
<description>I/O port H reset</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IOPARST</name>
<description>I/O port A reset</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IOPBRST</name>
<description>I/O port B reset</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IOPCRST</name>
<description>I/O port C reset</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IOPDRST</name>
<description>I/O port D reset</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IOPERST</name>
<description>I/O port E reset</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IOPFRST</name>
<description>I/O port F reset</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IOPGRST</name>
<description>I/O port G reset</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TSCRST</name>
<description>Touch sensing controller               reset</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ADC12RST</name>
<description>ADC1 and ADC2 reset</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ADC34RST</name>
<description>ADC3 and ADC4 reset</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CFGR2</name>
<displayName>CFGR2</displayName>
<description>Clock configuration register 2</description>
<addressOffset>0x2C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>PREDIV</name>
<description>PREDIV division factor</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>ADC12PRES</name>
<description>ADC1 and ADC2 prescaler</description>
<bitOffset>4</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>ADC34PRES</name>
<description>ADC3 and ADC4 prescaler</description>
<bitOffset>9</bitOffset>
<bitWidth>5</bitWidth>
</field>
</fields>
</register>
<register>
<name>CFGR3</name>
<displayName>CFGR3</displayName>
<description>Clock configuration register 3</description>
<addressOffset>0x30</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>USART1SW</name>
<description>USART1 clock source               selection</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>I2C1SW</name>
<description>I2C1 clock source               selection</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>I2C2SW</name>
<description>I2C2 clock source               selection</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>I2C3SW</name>
<description>I2C3 clock source               selection</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>USART2SW</name>
<description>USART2 clock source               selection</description>
<bitOffset>16</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>USART3SW</name>
<description>USART3 clock source               selection</description>
<bitOffset>18</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>TIM1SW</name>
<description>Timer1 clock source               selection</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIM8SW</name>
<description>Timer8 clock source               selection</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UART4SW</name>
<description>UART4 clock source               selection</description>
<bitOffset>20</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>UART5SW</name>
<description>UART5 clock source               selection</description>
<bitOffset>22</bitOffset>
<bitWidth>2</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral>
<name>DMA1</name>
<description>DMA controller 1</description>
<groupName>DMA</groupName>
<baseAddress>0x40020000</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<interrupt>
<name>DMA1_CH1</name>
<description>DMA1 channel 1 interrupt</description>
<value>11</value>
</interrupt>
<interrupt>
<name>DMA1_CH2</name>
<description>DMA1 channel 2 interrupt</description>
<value>12</value>
</interrupt>
<interrupt>
<name>DMA1_CH3</name>
<description>DMA1 channel 3 interrupt</description>
<value>13</value>
</interrupt>
<interrupt>
<name>DMA1_CH4</name>
<description>DMA1 channel 4 interrupt</description>
<value>14</value>
</interrupt>
<interrupt>
<name>DMA1_CH5</name>
<description>DMA1 channel 5 interrupt</description>
<value>15</value>
</interrupt>
<interrupt>
<name>DMA1_CH6</name>
<description>DMA1 channel 6 interrupt</description>
<value>16</value>
</interrupt>
<interrupt>
<name>DMA1_CH7</name>
<description>DMA1 channel 7interrupt</description>
<value>17</value>
</interrupt>
<registers>
<register>
<name>ISR</name>
<displayName>ISR</displayName>
<description>DMA interrupt status register           (DMA_ISR)</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>GIF1</name>
<description>Channel 1 Global interrupt               flag</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TCIF1</name>
<description>Channel 1 Transfer Complete               flag</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>HTIF1</name>
<description>Channel 1 Half Transfer Complete               flag</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TEIF1</name>
<description>Channel 1 Transfer Error               flag</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>GIF2</name>
<description>Channel 2 Global interrupt               flag</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TCIF2</name>
<description>Channel 2 Transfer Complete               flag</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>HTIF2</name>
<description>Channel 2 Half Transfer Complete               flag</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TEIF2</name>
<description>Channel 2 Transfer Error               flag</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>GIF3</name>
<description>Channel 3 Global interrupt               flag</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TCIF3</name>
<description>Channel 3 Transfer Complete               flag</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>HTIF3</name>
<description>Channel 3 Half Transfer Complete               flag</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TEIF3</name>
<description>Channel 3 Transfer Error               flag</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>GIF4</name>
<description>Channel 4 Global interrupt               flag</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TCIF4</name>
<description>Channel 4 Transfer Complete               flag</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>HTIF4</name>
<description>Channel 4 Half Transfer Complete               flag</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TEIF4</name>
<description>Channel 4 Transfer Error               flag</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>GIF5</name>
<description>Channel 5 Global interrupt               flag</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TCIF5</name>
<description>Channel 5 Transfer Complete               flag</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>HTIF5</name>
<description>Channel 5 Half Transfer Complete               flag</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TEIF5</name>
<description>Channel 5 Transfer Error               flag</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>GIF6</name>
<description>Channel 6 Global interrupt               flag</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TCIF6</name>
<description>Channel 6 Transfer Complete               flag</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>HTIF6</name>
<description>Channel 6 Half Transfer Complete               flag</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TEIF6</name>
<description>Channel 6 Transfer Error               flag</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>GIF7</name>
<description>Channel 7 Global interrupt               flag</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TCIF7</name>
<description>Channel 7 Transfer Complete               flag</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>HTIF7</name>
<description>Channel 7 Half Transfer Complete               flag</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TEIF7</name>
<description>Channel 7 Transfer Error               flag</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>IFCR</name>
<displayName>IFCR</displayName>
<description>DMA interrupt flag clear register           (DMA_IFCR)</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>write-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CGIF1</name>
<description>Channel 1 Global interrupt               clear</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CTCIF1</name>
<description>Channel 1 Transfer Complete               clear</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CHTIF1</name>
<description>Channel 1 Half Transfer               clear</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CTEIF1</name>
<description>Channel 1 Transfer Error               clear</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CGIF2</name>
<description>Channel 2 Global interrupt               clear</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CTCIF2</name>
<description>Channel 2 Transfer Complete               clear</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CHTIF2</name>
<description>Channel 2 Half Transfer               clear</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CTEIF2</name>
<description>Channel 2 Transfer Error               clear</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CGIF3</name>
<description>Channel 3 Global interrupt               clear</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CTCIF3</name>
<description>Channel 3 Transfer Complete               clear</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CHTIF3</name>
<description>Channel 3 Half Transfer               clear</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CTEIF3</name>
<description>Channel 3 Transfer Error               clear</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CGIF4</name>
<description>Channel 4 Global interrupt               clear</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CTCIF4</name>
<description>Channel 4 Transfer Complete               clear</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CHTIF4</name>
<description>Channel 4 Half Transfer               clear</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CTEIF4</name>
<description>Channel 4 Transfer Error               clear</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CGIF5</name>
<description>Channel 5 Global interrupt               clear</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CTCIF5</name>
<description>Channel 5 Transfer Complete               clear</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CHTIF5</name>
<description>Channel 5 Half Transfer               clear</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CTEIF5</name>
<description>Channel 5 Transfer Error               clear</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CGIF6</name>
<description>Channel 6 Global interrupt               clear</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CTCIF6</name>
<description>Channel 6 Transfer Complete               clear</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CHTIF6</name>
<description>Channel 6 Half Transfer               clear</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CTEIF6</name>
<description>Channel 6 Transfer Error               clear</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CGIF7</name>
<description>Channel 7 Global interrupt               clear</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CTCIF7</name>
<description>Channel 7 Transfer Complete               clear</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CHTIF7</name>
<description>Channel 7 Half Transfer               clear</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CTEIF7</name>
<description>Channel 7 Transfer Error               clear</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR1</name>
<displayName>CCR1</displayName>
<description>DMA channel configuration register           (DMA_CCR)</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>EN</name>
<description>Channel enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TCIE</name>
<description>Transfer complete interrupt               enable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>HTIE</name>
<description>Half Transfer interrupt               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TEIE</name>
<description>Transfer error interrupt               enable</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DIR</name>
<description>Data transfer direction</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CIRC</name>
<description>Circular mode</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PINC</name>
<description>Peripheral increment mode</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MINC</name>
<description>Memory increment mode</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PSIZE</name>
<description>Peripheral size</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MSIZE</name>
<description>Memory size</description>
<bitOffset>10</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PL</name>
<description>Channel Priority level</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MEM2MEM</name>
<description>Memory to memory mode</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CNDTR1</name>
<displayName>CNDTR1</displayName>
<description>DMA channel 1 number of data           register</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>NDT</name>
<description>Number of data to transfer</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>CPAR1</name>
<displayName>CPAR1</displayName>
<description>DMA channel 1 peripheral address           register</description>
<addressOffset>0x10</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>PA</name>
<description>Peripheral address</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>CMAR1</name>
<displayName>CMAR1</displayName>
<description>DMA channel 1 memory address           register</description>
<addressOffset>0x14</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>MA</name>
<description>Memory address</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR2</name>
<displayName>CCR2</displayName>
<description>DMA channel configuration register           (DMA_CCR)</description>
<addressOffset>0x1C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>EN</name>
<description>Channel enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TCIE</name>
<description>Transfer complete interrupt               enable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>HTIE</name>
<description>Half Transfer interrupt               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TEIE</name>
<description>Transfer error interrupt               enable</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DIR</name>
<description>Data transfer direction</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CIRC</name>
<description>Circular mode</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PINC</name>
<description>Peripheral increment mode</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MINC</name>
<description>Memory increment mode</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PSIZE</name>
<description>Peripheral size</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MSIZE</name>
<description>Memory size</description>
<bitOffset>10</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PL</name>
<description>Channel Priority level</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MEM2MEM</name>
<description>Memory to memory mode</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CNDTR2</name>
<displayName>CNDTR2</displayName>
<description>DMA channel 2 number of data           register</description>
<addressOffset>0x20</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>NDT</name>
<description>Number of data to transfer</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>CPAR2</name>
<displayName>CPAR2</displayName>
<description>DMA channel 2 peripheral address           register</description>
<addressOffset>0x24</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>PA</name>
<description>Peripheral address</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>CMAR2</name>
<displayName>CMAR2</displayName>
<description>DMA channel 2 memory address           register</description>
<addressOffset>0x28</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>MA</name>
<description>Memory address</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR3</name>
<displayName>CCR3</displayName>
<description>DMA channel configuration register           (DMA_CCR)</description>
<addressOffset>0x30</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>EN</name>
<description>Channel enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TCIE</name>
<description>Transfer complete interrupt               enable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>HTIE</name>
<description>Half Transfer interrupt               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TEIE</name>
<description>Transfer error interrupt               enable</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DIR</name>
<description>Data transfer direction</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CIRC</name>
<description>Circular mode</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PINC</name>
<description>Peripheral increment mode</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MINC</name>
<description>Memory increment mode</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PSIZE</name>
<description>Peripheral size</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MSIZE</name>
<description>Memory size</description>
<bitOffset>10</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PL</name>
<description>Channel Priority level</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MEM2MEM</name>
<description>Memory to memory mode</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CNDTR3</name>
<displayName>CNDTR3</displayName>
<description>DMA channel 3 number of data           register</description>
<addressOffset>0x34</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>NDT</name>
<description>Number of data to transfer</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>CPAR3</name>
<displayName>CPAR3</displayName>
<description>DMA channel 3 peripheral address           register</description>
<addressOffset>0x38</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>PA</name>
<description>Peripheral address</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>CMAR3</name>
<displayName>CMAR3</displayName>
<description>DMA channel 3 memory address           register</description>
<addressOffset>0x3C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>MA</name>
<description>Memory address</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR4</name>
<displayName>CCR4</displayName>
<description>DMA channel configuration register           (DMA_CCR)</description>
<addressOffset>0x44</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>EN</name>
<description>Channel enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TCIE</name>
<description>Transfer complete interrupt               enable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>HTIE</name>
<description>Half Transfer interrupt               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TEIE</name>
<description>Transfer error interrupt               enable</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DIR</name>
<description>Data transfer direction</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CIRC</name>
<description>Circular mode</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PINC</name>
<description>Peripheral increment mode</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MINC</name>
<description>Memory increment mode</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PSIZE</name>
<description>Peripheral size</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MSIZE</name>
<description>Memory size</description>
<bitOffset>10</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PL</name>
<description>Channel Priority level</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MEM2MEM</name>
<description>Memory to memory mode</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CNDTR4</name>
<displayName>CNDTR4</displayName>
<description>DMA channel 4 number of data           register</description>
<addressOffset>0x48</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>NDT</name>
<description>Number of data to transfer</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>CPAR4</name>
<displayName>CPAR4</displayName>
<description>DMA channel 4 peripheral address           register</description>
<addressOffset>0x4C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>PA</name>
<description>Peripheral address</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>CMAR4</name>
<displayName>CMAR4</displayName>
<description>DMA channel 4 memory address           register</description>
<addressOffset>0x50</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>MA</name>
<description>Memory address</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR5</name>
<displayName>CCR5</displayName>
<description>DMA channel configuration register           (DMA_CCR)</description>
<addressOffset>0x58</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>EN</name>
<description>Channel enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TCIE</name>
<description>Transfer complete interrupt               enable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>HTIE</name>
<description>Half Transfer interrupt               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TEIE</name>
<description>Transfer error interrupt               enable</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DIR</name>
<description>Data transfer direction</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CIRC</name>
<description>Circular mode</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PINC</name>
<description>Peripheral increment mode</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MINC</name>
<description>Memory increment mode</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PSIZE</name>
<description>Peripheral size</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MSIZE</name>
<description>Memory size</description>
<bitOffset>10</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PL</name>
<description>Channel Priority level</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MEM2MEM</name>
<description>Memory to memory mode</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CNDTR5</name>
<displayName>CNDTR5</displayName>
<description>DMA channel 5 number of data           register</description>
<addressOffset>0x5C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>NDT</name>
<description>Number of data to transfer</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>CPAR5</name>
<displayName>CPAR5</displayName>
<description>DMA channel 5 peripheral address           register</description>
<addressOffset>0x60</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>PA</name>
<description>Peripheral address</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>CMAR5</name>
<displayName>CMAR5</displayName>
<description>DMA channel 5 memory address           register</description>
<addressOffset>0x64</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>MA</name>
<description>Memory address</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR6</name>
<displayName>CCR6</displayName>
<description>DMA channel configuration register           (DMA_CCR)</description>
<addressOffset>0x6C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>EN</name>
<description>Channel enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TCIE</name>
<description>Transfer complete interrupt               enable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>HTIE</name>
<description>Half Transfer interrupt               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TEIE</name>
<description>Transfer error interrupt               enable</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DIR</name>
<description>Data transfer direction</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CIRC</name>
<description>Circular mode</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PINC</name>
<description>Peripheral increment mode</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MINC</name>
<description>Memory increment mode</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PSIZE</name>
<description>Peripheral size</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MSIZE</name>
<description>Memory size</description>
<bitOffset>10</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PL</name>
<description>Channel Priority level</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MEM2MEM</name>
<description>Memory to memory mode</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CNDTR6</name>
<displayName>CNDTR6</displayName>
<description>DMA channel 6 number of data           register</description>
<addressOffset>0x70</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>NDT</name>
<description>Number of data to transfer</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>CPAR6</name>
<displayName>CPAR6</displayName>
<description>DMA channel 6 peripheral address           register</description>
<addressOffset>0x74</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>PA</name>
<description>Peripheral address</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>CMAR6</name>
<displayName>CMAR6</displayName>
<description>DMA channel 6 memory address           register</description>
<addressOffset>0x78</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>MA</name>
<description>Memory address</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR7</name>
<displayName>CCR7</displayName>
<description>DMA channel configuration register           (DMA_CCR)</description>
<addressOffset>0x80</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>EN</name>
<description>Channel enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TCIE</name>
<description>Transfer complete interrupt               enable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>HTIE</name>
<description>Half Transfer interrupt               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TEIE</name>
<description>Transfer error interrupt               enable</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DIR</name>
<description>Data transfer direction</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CIRC</name>
<description>Circular mode</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PINC</name>
<description>Peripheral increment mode</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MINC</name>
<description>Memory increment mode</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PSIZE</name>
<description>Peripheral size</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MSIZE</name>
<description>Memory size</description>
<bitOffset>10</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PL</name>
<description>Channel Priority level</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>MEM2MEM</name>
<description>Memory to memory mode</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CNDTR7</name>
<displayName>CNDTR7</displayName>
<description>DMA channel 7 number of data           register</description>
<addressOffset>0x84</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>NDT</name>
<description>Number of data to transfer</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>CPAR7</name>
<displayName>CPAR7</displayName>
<description>DMA channel 7 peripheral address           register</description>
<addressOffset>0x88</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>PA</name>
<description>Peripheral address</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>CMAR7</name>
<displayName>CMAR7</displayName>
<description>DMA channel 7 memory address           register</description>
<addressOffset>0x8C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>MA</name>
<description>Memory address</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral derivedFrom="DMA1">
<name>DMA2</name>
<baseAddress>0x40020400</baseAddress>
<interrupt>
<name>DMA2_CH1</name>
<description>DMA2 channel1 global interrupt</description>
<value>56</value>
</interrupt>
<interrupt>
<name>DMA2_CH2</name>
<description>DMA2 channel2 global interrupt</description>
<value>57</value>
</interrupt>
<interrupt>
<name>DMA2_CH3</name>
<description>DMA2 channel3 global interrupt</description>
<value>58</value>
</interrupt>
<interrupt>
<name>DMA2_CH4</name>
<description>DMA2 channel4 global interrupt</description>
<value>59</value>
</interrupt>
<interrupt>
<name>DMA2_CH5</name>
<description>DMA2 channel5 global interrupt</description>
<value>60</value>
</interrupt>
</peripheral>
<peripheral>
<name>TIM2</name>
<description>General purpose timer</description>
<groupName>TIMs</groupName>
<baseAddress>0x40000000</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<interrupt>
<name>TIM2</name>
<description>TIM2 global interrupt</description>
<value>28</value>
</interrupt>
<registers>
<register>
<name>CR1</name>
<displayName>CR1</displayName>
<description>control register 1</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>CEN</name>
<description>Counter enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UDIS</name>
<description>Update disable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>URS</name>
<description>Update request source</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OPM</name>
<description>One-pulse mode</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DIR</name>
<description>Direction</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CMS</name>
<description>Center-aligned mode               selection</description>
<bitOffset>5</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>ARPE</name>
<description>Auto-reload preload enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CKD</name>
<description>Clock division</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>UIFREMAP</name>
<description>UIF status bit remapping</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CR2</name>
<displayName>CR2</displayName>
<description>control register 2</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>TI1S</name>
<description>TI1 selection</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MMS</name>
<description>Master mode selection</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>CCDS</name>
<description>Capture/compare DMA               selection</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>SMCR</name>
<displayName>SMCR</displayName>
<description>slave mode control register</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>SMS</name>
<description>Slave mode selection</description>
<bitOffset>0</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>OCCS</name>
<description>OCREF clear selection</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TS</name>
<description>Trigger selection</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>MSM</name>
<description>Master/Slave mode</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ETF</name>
<description>External trigger filter</description>
<bitOffset>8</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>ETPS</name>
<description>External trigger prescaler</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>ECE</name>
<description>External clock enable</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ETP</name>
<description>External trigger polarity</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SMS_3</name>
<description>Slave mode selection bit3</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>DIER</name>
<displayName>DIER</displayName>
<description>DMA/Interrupt enable register</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>TDE</name>
<description>Trigger DMA request enable</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4DE</name>
<description>Capture/Compare 4 DMA request               enable</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3DE</name>
<description>Capture/Compare 3 DMA request               enable</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2DE</name>
<description>Capture/Compare 2 DMA request               enable</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1DE</name>
<description>Capture/Compare 1 DMA request               enable</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UDE</name>
<description>Update DMA request enable</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIE</name>
<description>Trigger interrupt enable</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4IE</name>
<description>Capture/Compare 4 interrupt               enable</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3IE</name>
<description>Capture/Compare 3 interrupt               enable</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2IE</name>
<description>Capture/Compare 2 interrupt               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1IE</name>
<description>Capture/Compare 1 interrupt               enable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UIE</name>
<description>Update interrupt enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>SR</name>
<displayName>SR</displayName>
<description>status register</description>
<addressOffset>0x10</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>CC4OF</name>
<description>Capture/Compare 4 overcapture               flag</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3OF</name>
<description>Capture/Compare 3 overcapture               flag</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2OF</name>
<description>Capture/compare 2 overcapture               flag</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1OF</name>
<description>Capture/Compare 1 overcapture               flag</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIF</name>
<description>Trigger interrupt flag</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4IF</name>
<description>Capture/Compare 4 interrupt               flag</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3IF</name>
<description>Capture/Compare 3 interrupt               flag</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2IF</name>
<description>Capture/Compare 2 interrupt               flag</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1IF</name>
<description>Capture/compare 1 interrupt               flag</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UIF</name>
<description>Update interrupt flag</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>EGR</name>
<displayName>EGR</displayName>
<description>event generation register</description>
<addressOffset>0x14</addressOffset>
<size>0x20</size>
<access>write-only</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>TG</name>
<description>Trigger generation</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4G</name>
<description>Capture/compare 4               generation</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3G</name>
<description>Capture/compare 3               generation</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2G</name>
<description>Capture/compare 2               generation</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1G</name>
<description>Capture/compare 1               generation</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UG</name>
<description>Update generation</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCMR1_Output</name>
<displayName>CCMR1_Output</displayName>
<description>capture/compare mode register 1 (output           mode)</description>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CC1S</name>
<description>Capture/Compare 1               selection</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OC1FE</name>
<description>Output compare 1 fast               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC1PE</name>
<description>Output compare 1 preload               enable</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC1M</name>
<description>Output compare 1 mode</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>OC1CE</name>
<description>Output compare 1 clear               enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2S</name>
<description>Capture/Compare 2               selection</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OC2FE</name>
<description>Output compare 2 fast               enable</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC2PE</name>
<description>Output compare 2 preload               enable</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC2M</name>
<description>Output compare 2 mode</description>
<bitOffset>12</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>OC2CE</name>
<description>Output compare 2 clear               enable</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC1M_3</name>
<description>Output compare 1 mode bit               3</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC2M_3</name>
<description>Output compare 2 mode bit               3</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCMR1_Input</name>
<displayName>CCMR1_Input</displayName>
<description>capture/compare mode register 1 (input           mode)</description>
<alternateRegister>CCMR1_Output</alternateRegister>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IC2F</name>
<description>Input capture 2 filter</description>
<bitOffset>12</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>IC2PSC</name>
<description>Input capture 2 prescaler</description>
<bitOffset>10</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>CC2S</name>
<description>Capture/compare 2               selection</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>IC1F</name>
<description>Input capture 1 filter</description>
<bitOffset>4</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>IC1PSC</name>
<description>Input capture 1 prescaler</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>CC1S</name>
<description>Capture/Compare 1               selection</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCMR2_Output</name>
<displayName>CCMR2_Output</displayName>
<description>capture/compare mode register 2 (output           mode)</description>
<addressOffset>0x1C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CC3S</name>
<description>Capture/Compare 3               selection</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OC3FE</name>
<description>Output compare 3 fast               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC3PE</name>
<description>Output compare 3 preload               enable</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC3M</name>
<description>Output compare 3 mode</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>OC3CE</name>
<description>Output compare 3 clear               enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4S</name>
<description>Capture/Compare 4               selection</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OC4FE</name>
<description>Output compare 4 fast               enable</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC4PE</name>
<description>Output compare 4 preload               enable</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC4M</name>
<description>Output compare 4 mode</description>
<bitOffset>12</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>O24CE</name>
<description>Output compare 4 clear               enable</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC3M_3</name>
<description>Output compare 3 mode bit3</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC4M_3</name>
<description>Output compare 4 mode bit3</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCMR2_Input</name>
<displayName>CCMR2_Input</displayName>
<description>capture/compare mode register 2 (input           mode)</description>
<alternateRegister>CCMR2_Output</alternateRegister>
<addressOffset>0x1C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IC4F</name>
<description>Input capture 4 filter</description>
<bitOffset>12</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>IC4PSC</name>
<description>Input capture 4 prescaler</description>
<bitOffset>10</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>CC4S</name>
<description>Capture/Compare 4               selection</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>IC3F</name>
<description>Input capture 3 filter</description>
<bitOffset>4</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>IC3PSC</name>
<description>Input capture 3 prescaler</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>CC3S</name>
<description>Capture/Compare 3               selection</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCER</name>
<displayName>CCER</displayName>
<description>capture/compare enable           register</description>
<addressOffset>0x20</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>CC1E</name>
<description>Capture/Compare 1 output               enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1P</name>
<description>Capture/Compare 1 output               Polarity</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1NP</name>
<description>Capture/Compare 1 output               Polarity</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2E</name>
<description>Capture/Compare 2 output               enable</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2P</name>
<description>Capture/Compare 2 output               Polarity</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2NP</name>
<description>Capture/Compare 2 output               Polarity</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3E</name>
<description>Capture/Compare 3 output               enable</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3P</name>
<description>Capture/Compare 3 output               Polarity</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3NP</name>
<description>Capture/Compare 3 output               Polarity</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4E</name>
<description>Capture/Compare 4 output               enable</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4P</name>
<description>Capture/Compare 3 output               Polarity</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4NP</name>
<description>Capture/Compare 3 output               Polarity</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CNT</name>
<displayName>CNT</displayName>
<description>counter</description>
<addressOffset>0x24</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CNTL</name>
<description>Low counter value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
<field>
<name>CNTH</name>
<description>High counter value</description>
<bitOffset>16</bitOffset>
<bitWidth>15</bitWidth>
</field>
<field>
<name>CNT_or_UIFCPY</name>
<description>if IUFREMAP=0 than CNT with read write               access else UIFCPY with read only               access</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>PSC</name>
<displayName>PSC</displayName>
<description>prescaler</description>
<addressOffset>0x28</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>PSC</name>
<description>Prescaler value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>ARR</name>
<displayName>ARR</displayName>
<description>auto-reload register</description>
<addressOffset>0x2C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>ARRL</name>
<description>Low Auto-reload value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
<field>
<name>ARRH</name>
<description>High Auto-reload value</description>
<bitOffset>16</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR1</name>
<displayName>CCR1</displayName>
<description>capture/compare register 1</description>
<addressOffset>0x34</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CCR1L</name>
<description>Low Capture/Compare 1               value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
<field>
<name>CCR1H</name>
<description>High Capture/Compare 1 value (on               TIM2)</description>
<bitOffset>16</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR2</name>
<displayName>CCR2</displayName>
<description>capture/compare register 2</description>
<addressOffset>0x38</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CCR2L</name>
<description>Low Capture/Compare 2               value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
<field>
<name>CCR2H</name>
<description>High Capture/Compare 2 value (on               TIM2)</description>
<bitOffset>16</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR3</name>
<displayName>CCR3</displayName>
<description>capture/compare register 3</description>
<addressOffset>0x3C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CCR3L</name>
<description>Low Capture/Compare value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
<field>
<name>CCR3H</name>
<description>High Capture/Compare value (on               TIM2)</description>
<bitOffset>16</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR4</name>
<displayName>CCR4</displayName>
<description>capture/compare register 4</description>
<addressOffset>0x40</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CCR4L</name>
<description>Low Capture/Compare value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
<field>
<name>CCR4H</name>
<description>High Capture/Compare value (on               TIM2)</description>
<bitOffset>16</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>DCR</name>
<displayName>DCR</displayName>
<description>DMA control register</description>
<addressOffset>0x48</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>DBL</name>
<description>DMA burst length</description>
<bitOffset>8</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>DBA</name>
<description>DMA base address</description>
<bitOffset>0</bitOffset>
<bitWidth>5</bitWidth>
</field>
</fields>
</register>
<register>
<name>DMAR</name>
<displayName>DMAR</displayName>
<description>DMA address for full transfer</description>
<addressOffset>0x4C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>DMAB</name>
<description>DMA register for burst               accesses</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral derivedFrom="TIM2">
<name>TIM3</name>
<baseAddress>0x40000400</baseAddress>
<interrupt>
<name>TIM3</name>
<description>TIM3 global interrupt</description>
<value>29</value>
</interrupt>
</peripheral>
<peripheral derivedFrom="TIM2">
<name>TIM4</name>
<baseAddress>0x40000800</baseAddress>
<interrupt>
<name>TIM4</name>
<description>TIM4 global interrupt</description>
<value>30</value>
</interrupt>
</peripheral>
<peripheral>
<name>TIM15</name>
<description>General purpose timers</description>
<groupName>TIMs</groupName>
<baseAddress>0x40014000</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<interrupt>
<name>TIM1_BRK_TIM15</name>
<description>TIM1 Break/TIM15 global
        interruts</description>
<value>24</value>
</interrupt>
<registers>
<register>
<name>CR1</name>
<displayName>CR1</displayName>
<description>control register 1</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>CEN</name>
<description>Counter enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UDIS</name>
<description>Update disable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>URS</name>
<description>Update request source</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OPM</name>
<description>One-pulse mode</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ARPE</name>
<description>Auto-reload preload enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CKD</name>
<description>Clock division</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>UIFREMAP</name>
<description>UIF status bit remapping</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CR2</name>
<displayName>CR2</displayName>
<description>control register 2</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>CCPC</name>
<description>Capture/compare preloaded               control</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CCUS</name>
<description>Capture/compare control update               selection</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CCDS</name>
<description>Capture/compare DMA               selection</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MMS</name>
<description>Master mode selection</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>TI1S</name>
<description>TI1 selection</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OIS1</name>
<description>Output Idle state 1</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OIS1N</name>
<description>Output Idle state 1</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OIS2</name>
<description>Output Idle state 2</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>SMCR</name>
<displayName>SMCR</displayName>
<description>slave mode control register</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>SMS</name>
<description>Slave mode selection</description>
<bitOffset>0</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>TS</name>
<description>Trigger selection</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>MSM</name>
<description>Master/Slave mode</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SMS_3</name>
<description>Slave mode selection bit 3</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>DIER</name>
<displayName>DIER</displayName>
<description>DMA/Interrupt enable register</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>UIE</name>
<description>Update interrupt enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1IE</name>
<description>Capture/Compare 1 interrupt               enable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2IE</name>
<description>Capture/Compare 2 interrupt               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>COMIE</name>
<description>COM interrupt enable</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIE</name>
<description>Trigger interrupt enable</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BIE</name>
<description>Break interrupt enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UDE</name>
<description>Update DMA request enable</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1DE</name>
<description>Capture/Compare 1 DMA request               enable</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2DE</name>
<description>Capture/Compare 2 DMA request               enable</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>COMDE</name>
<description>COM DMA request enable</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TDE</name>
<description>Trigger DMA request enable</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>SR</name>
<displayName>SR</displayName>
<description>status register</description>
<addressOffset>0x10</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>CC2OF</name>
<description>Capture/compare 2 overcapture               flag</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1OF</name>
<description>Capture/Compare 1 overcapture               flag</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BIF</name>
<description>Break interrupt flag</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIF</name>
<description>Trigger interrupt flag</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>COMIF</name>
<description>COM interrupt flag</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2IF</name>
<description>Capture/Compare 2 interrupt               flag</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1IF</name>
<description>Capture/compare 1 interrupt               flag</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UIF</name>
<description>Update interrupt flag</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>EGR</name>
<displayName>EGR</displayName>
<description>event generation register</description>
<addressOffset>0x14</addressOffset>
<size>0x20</size>
<access>write-only</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>BG</name>
<description>Break generation</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TG</name>
<description>Trigger generation</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>COMG</name>
<description>Capture/Compare control update               generation</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2G</name>
<description>Capture/compare 2               generation</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1G</name>
<description>Capture/compare 1               generation</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UG</name>
<description>Update generation</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCMR1_Output</name>
<displayName>CCMR1_Output</displayName>
<description>capture/compare mode register (output           mode)</description>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CC1S</name>
<description>Capture/Compare 1               selection</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OC1FE</name>
<description>Output Compare 1 fast               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC1PE</name>
<description>Output Compare 1 preload               enable</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC1M</name>
<description>Output Compare 1 mode</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>CC2S</name>
<description>Capture/Compare 2               selection</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OC2FE</name>
<description>Output Compare 2 fast               enable</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC2PE</name>
<description>Output Compare 2 preload               enable</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC2M</name>
<description>Output Compare 2 mode</description>
<bitOffset>12</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>OC1M_3</name>
<description>Output Compare 1 mode bit               3</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC2M_3</name>
<description>Output Compare 2 mode bit               3</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCMR1_Input</name>
<displayName>CCMR1_Input</displayName>
<description>capture/compare mode register 1 (input           mode)</description>
<alternateRegister>CCMR1_Output</alternateRegister>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IC2F</name>
<description>Input capture 2 filter</description>
<bitOffset>12</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>IC2PSC</name>
<description>Input capture 2 prescaler</description>
<bitOffset>10</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>CC2S</name>
<description>Capture/Compare 2               selection</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>IC1F</name>
<description>Input capture 1 filter</description>
<bitOffset>4</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>IC1PSC</name>
<description>Input capture 1 prescaler</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>CC1S</name>
<description>Capture/Compare 1               selection</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCER</name>
<displayName>CCER</displayName>
<description>capture/compare enable           register</description>
<addressOffset>0x20</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>CC2NP</name>
<description>Capture/Compare 2 output               Polarity</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2P</name>
<description>Capture/Compare 2 output               Polarity</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2E</name>
<description>Capture/Compare 2 output               enable</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1NP</name>
<description>Capture/Compare 1 output               Polarity</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1NE</name>
<description>Capture/Compare 1 complementary output               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1P</name>
<description>Capture/Compare 1 output               Polarity</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1E</name>
<description>Capture/Compare 1 output               enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CNT</name>
<displayName>CNT</displayName>
<description>counter</description>
<addressOffset>0x24</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CNT</name>
<description>counter value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
<access>read-write</access>
</field>
<field>
<name>UIFCPY</name>
<description>UIF copy</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
</fields>
</register>
<register>
<name>PSC</name>
<displayName>PSC</displayName>
<description>prescaler</description>
<addressOffset>0x28</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>PSC</name>
<description>Prescaler value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>ARR</name>
<displayName>ARR</displayName>
<description>auto-reload register</description>
<addressOffset>0x2C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>ARR</name>
<description>Auto-reload value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>RCR</name>
<displayName>RCR</displayName>
<description>repetition counter register</description>
<addressOffset>0x30</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>REP</name>
<description>Repetition counter value</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR1</name>
<displayName>CCR1</displayName>
<description>capture/compare register 1</description>
<addressOffset>0x34</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CCR1</name>
<description>Capture/Compare 1 value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR2</name>
<displayName>CCR2</displayName>
<description>capture/compare register 2</description>
<addressOffset>0x38</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CCR2</name>
<description>Capture/Compare 2 value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>BDTR</name>
<displayName>BDTR</displayName>
<description>break and dead-time register</description>
<addressOffset>0x44</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>MOE</name>
<description>Main output enable</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>AOE</name>
<description>Automatic output enable</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BKP</name>
<description>Break polarity</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BKE</name>
<description>Break enable</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OSSR</name>
<description>Off-state selection for Run               mode</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OSSI</name>
<description>Off-state selection for Idle               mode</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LOCK</name>
<description>Lock configuration</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>DTG</name>
<description>Dead-time generator setup</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>BKF</name>
<description>Break filter</description>
<bitOffset>16</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>DCR</name>
<displayName>DCR</displayName>
<description>DMA control register</description>
<addressOffset>0x48</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>DBL</name>
<description>DMA burst length</description>
<bitOffset>8</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>DBA</name>
<description>DMA base address</description>
<bitOffset>0</bitOffset>
<bitWidth>5</bitWidth>
</field>
</fields>
</register>
<register>
<name>DMAR</name>
<displayName>DMAR</displayName>
<description>DMA address for full transfer</description>
<addressOffset>0x4C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>DMAB</name>
<description>DMA register for burst               accesses</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral>
<name>TIM16</name>
<description>General-purpose-timers</description>
<groupName>TIMs</groupName>
<baseAddress>0x40014400</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<interrupt>
<name>TIM1_UP_TIM16</name>
<description>TIM1 Update/TIM16 global
        interrupts</description>
<value>25</value>
</interrupt>
<registers>
<register>
<name>CR1</name>
<displayName>CR1</displayName>
<description>control register 1</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>CEN</name>
<description>Counter enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UDIS</name>
<description>Update disable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>URS</name>
<description>Update request source</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OPM</name>
<description>One-pulse mode</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ARPE</name>
<description>Auto-reload preload enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CKD</name>
<description>Clock division</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>UIFREMAP</name>
<description>UIF status bit remapping</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CR2</name>
<displayName>CR2</displayName>
<description>control register 2</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>OIS1N</name>
<description>Output Idle state 1</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OIS1</name>
<description>Output Idle state 1</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CCDS</name>
<description>Capture/compare DMA               selection</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CCUS</name>
<description>Capture/compare control update               selection</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CCPC</name>
<description>Capture/compare preloaded               control</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>DIER</name>
<displayName>DIER</displayName>
<description>DMA/Interrupt enable register</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>UIE</name>
<description>Update interrupt enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1IE</name>
<description>Capture/Compare 1 interrupt               enable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>COMIE</name>
<description>COM interrupt enable</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIE</name>
<description>Trigger interrupt enable</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BIE</name>
<description>Break interrupt enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UDE</name>
<description>Update DMA request enable</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1DE</name>
<description>Capture/Compare 1 DMA request               enable</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>COMDE</name>
<description>COM DMA request enable</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TDE</name>
<description>Trigger DMA request enable</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>SR</name>
<displayName>SR</displayName>
<description>status register</description>
<addressOffset>0x10</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>CC1OF</name>
<description>Capture/Compare 1 overcapture               flag</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BIF</name>
<description>Break interrupt flag</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIF</name>
<description>Trigger interrupt flag</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>COMIF</name>
<description>COM interrupt flag</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1IF</name>
<description>Capture/compare 1 interrupt               flag</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UIF</name>
<description>Update interrupt flag</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>EGR</name>
<displayName>EGR</displayName>
<description>event generation register</description>
<addressOffset>0x14</addressOffset>
<size>0x20</size>
<access>write-only</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>BG</name>
<description>Break generation</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TG</name>
<description>Trigger generation</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>COMG</name>
<description>Capture/Compare control update               generation</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1G</name>
<description>Capture/compare 1               generation</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UG</name>
<description>Update generation</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCMR1_Output</name>
<displayName>CCMR1_Output</displayName>
<description>capture/compare mode register (output           mode)</description>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CC1S</name>
<description>Capture/Compare 1               selection</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OC1FE</name>
<description>Output Compare 1 fast               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC1PE</name>
<description>Output Compare 1 preload               enable</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC1M</name>
<description>Output Compare 1 mode</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>OC1M_3</name>
<description>Output Compare 1 mode</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCMR1_Input</name>
<displayName>CCMR1_Input</displayName>
<description>capture/compare mode register 1 (input           mode)</description>
<alternateRegister>CCMR1_Output</alternateRegister>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IC1F</name>
<description>Input capture 1 filter</description>
<bitOffset>4</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>IC1PSC</name>
<description>Input capture 1 prescaler</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>CC1S</name>
<description>Capture/Compare 1               selection</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCER</name>
<displayName>CCER</displayName>
<description>capture/compare enable           register</description>
<addressOffset>0x20</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>CC1NP</name>
<description>Capture/Compare 1 output               Polarity</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1NE</name>
<description>Capture/Compare 1 complementary output               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1P</name>
<description>Capture/Compare 1 output               Polarity</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1E</name>
<description>Capture/Compare 1 output               enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CNT</name>
<displayName>CNT</displayName>
<description>counter</description>
<addressOffset>0x24</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CNT</name>
<description>counter value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
<access>read-write</access>
</field>
<field>
<name>UIFCPY</name>
<description>UIF Copy</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
</fields>
</register>
<register>
<name>PSC</name>
<displayName>PSC</displayName>
<description>prescaler</description>
<addressOffset>0x28</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>PSC</name>
<description>Prescaler value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>ARR</name>
<displayName>ARR</displayName>
<description>auto-reload register</description>
<addressOffset>0x2C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>ARR</name>
<description>Auto-reload value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>RCR</name>
<displayName>RCR</displayName>
<description>repetition counter register</description>
<addressOffset>0x30</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>REP</name>
<description>Repetition counter value</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR1</name>
<displayName>CCR1</displayName>
<description>capture/compare register 1</description>
<addressOffset>0x34</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CCR1</name>
<description>Capture/Compare 1 value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>BDTR</name>
<displayName>BDTR</displayName>
<description>break and dead-time register</description>
<addressOffset>0x44</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>DTG</name>
<description>Dead-time generator setup</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>LOCK</name>
<description>Lock configuration</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSSI</name>
<description>Off-state selection for Idle               mode</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OSSR</name>
<description>Off-state selection for Run               mode</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BKE</name>
<description>Break enable</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BKP</name>
<description>Break polarity</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>AOE</name>
<description>Automatic output enable</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MOE</name>
<description>Main output enable</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BKF</name>
<description>Break filter</description>
<bitOffset>16</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>DCR</name>
<displayName>DCR</displayName>
<description>DMA control register</description>
<addressOffset>0x48</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>DBL</name>
<description>DMA burst length</description>
<bitOffset>8</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>DBA</name>
<description>DMA base address</description>
<bitOffset>0</bitOffset>
<bitWidth>5</bitWidth>
</field>
</fields>
</register>
<register>
<name>DMAR</name>
<displayName>DMAR</displayName>
<description>DMA address for full transfer</description>
<addressOffset>0x4C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>DMAB</name>
<description>DMA register for burst               accesses</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>OR</name>
<displayName>OR</displayName>
<description>option register</description>
<addressOffset>0x50</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
</register>
</registers>
</peripheral>
<peripheral>
<name>TIM17</name>
<description>General purpose timer</description>
<groupName>TIMs</groupName>
<baseAddress>0x40014800</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<interrupt>
<name>TIM1_TRG_COM_TIM17</name>
<description>TIM1 trigger and commutation/TIM17
        interrupts</description>
<value>26</value>
</interrupt>
<registers>
<register>
<name>CR1</name>
<displayName>CR1</displayName>
<description>control register 1</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>CEN</name>
<description>Counter enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UDIS</name>
<description>Update disable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>URS</name>
<description>Update request source</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OPM</name>
<description>One-pulse mode</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ARPE</name>
<description>Auto-reload preload enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CKD</name>
<description>Clock division</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>UIFREMAP</name>
<description>UIF status bit remapping</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CR2</name>
<displayName>CR2</displayName>
<description>control register 2</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>OIS1N</name>
<description>Output Idle state 1</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OIS1</name>
<description>Output Idle state 1</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CCDS</name>
<description>Capture/compare DMA               selection</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CCUS</name>
<description>Capture/compare control update               selection</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CCPC</name>
<description>Capture/compare preloaded               control</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>DIER</name>
<displayName>DIER</displayName>
<description>DMA/Interrupt enable register</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>UIE</name>
<description>Update interrupt enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1IE</name>
<description>Capture/Compare 1 interrupt               enable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>COMIE</name>
<description>COM interrupt enable</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIE</name>
<description>Trigger interrupt enable</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BIE</name>
<description>Break interrupt enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UDE</name>
<description>Update DMA request enable</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1DE</name>
<description>Capture/Compare 1 DMA request               enable</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>COMDE</name>
<description>COM DMA request enable</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TDE</name>
<description>Trigger DMA request enable</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>SR</name>
<displayName>SR</displayName>
<description>status register</description>
<addressOffset>0x10</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>CC1OF</name>
<description>Capture/Compare 1 overcapture               flag</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BIF</name>
<description>Break interrupt flag</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIF</name>
<description>Trigger interrupt flag</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>COMIF</name>
<description>COM interrupt flag</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1IF</name>
<description>Capture/compare 1 interrupt               flag</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UIF</name>
<description>Update interrupt flag</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>EGR</name>
<displayName>EGR</displayName>
<description>event generation register</description>
<addressOffset>0x14</addressOffset>
<size>0x20</size>
<access>write-only</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>BG</name>
<description>Break generation</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TG</name>
<description>Trigger generation</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>COMG</name>
<description>Capture/Compare control update               generation</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1G</name>
<description>Capture/compare 1               generation</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UG</name>
<description>Update generation</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCMR1_Output</name>
<displayName>CCMR1_Output</displayName>
<description>capture/compare mode register (output           mode)</description>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CC1S</name>
<description>Capture/Compare 1               selection</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OC1FE</name>
<description>Output Compare 1 fast               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC1PE</name>
<description>Output Compare 1 preload               enable</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC1M</name>
<description>Output Compare 1 mode</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>OC1M_3</name>
<description>Output Compare 1 mode</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCMR1_Input</name>
<displayName>CCMR1_Input</displayName>
<description>capture/compare mode register 1 (input           mode)</description>
<alternateRegister>CCMR1_Output</alternateRegister>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IC1F</name>
<description>Input capture 1 filter</description>
<bitOffset>4</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>IC1PSC</name>
<description>Input capture 1 prescaler</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>CC1S</name>
<description>Capture/Compare 1               selection</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCER</name>
<displayName>CCER</displayName>
<description>capture/compare enable           register</description>
<addressOffset>0x20</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>CC1NP</name>
<description>Capture/Compare 1 output               Polarity</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1NE</name>
<description>Capture/Compare 1 complementary output               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1P</name>
<description>Capture/Compare 1 output               Polarity</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1E</name>
<description>Capture/Compare 1 output               enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CNT</name>
<displayName>CNT</displayName>
<description>counter</description>
<addressOffset>0x24</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CNT</name>
<description>counter value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
<access>read-write</access>
</field>
<field>
<name>UIFCPY</name>
<description>UIF Copy</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
</fields>
</register>
<register>
<name>PSC</name>
<displayName>PSC</displayName>
<description>prescaler</description>
<addressOffset>0x28</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>PSC</name>
<description>Prescaler value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>ARR</name>
<displayName>ARR</displayName>
<description>auto-reload register</description>
<addressOffset>0x2C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>ARR</name>
<description>Auto-reload value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>RCR</name>
<displayName>RCR</displayName>
<description>repetition counter register</description>
<addressOffset>0x30</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>REP</name>
<description>Repetition counter value</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR1</name>
<displayName>CCR1</displayName>
<description>capture/compare register 1</description>
<addressOffset>0x34</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CCR1</name>
<description>Capture/Compare 1 value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>BDTR</name>
<displayName>BDTR</displayName>
<description>break and dead-time register</description>
<addressOffset>0x44</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>DTG</name>
<description>Dead-time generator setup</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>LOCK</name>
<description>Lock configuration</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSSI</name>
<description>Off-state selection for Idle               mode</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OSSR</name>
<description>Off-state selection for Run               mode</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BKE</name>
<description>Break enable</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BKP</name>
<description>Break polarity</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>AOE</name>
<description>Automatic output enable</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MOE</name>
<description>Main output enable</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BKF</name>
<description>Break filter</description>
<bitOffset>16</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>DCR</name>
<displayName>DCR</displayName>
<description>DMA control register</description>
<addressOffset>0x48</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>DBL</name>
<description>DMA burst length</description>
<bitOffset>8</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>DBA</name>
<description>DMA base address</description>
<bitOffset>0</bitOffset>
<bitWidth>5</bitWidth>
</field>
</fields>
</register>
<register>
<name>DMAR</name>
<displayName>DMAR</displayName>
<description>DMA address for full transfer</description>
<addressOffset>0x4C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>DMAB</name>
<description>DMA register for burst               accesses</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral>
<name>USART1</name>
<description>Universal synchronous asynchronous receiver       transmitter</description>
<groupName>USART</groupName>
<baseAddress>0x40013800</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<interrupt>
<name>USART1_EXTI25</name>
<description>USART1 global interrupt and EXTI Line 25
        interrupt</description>
<value>37</value>
</interrupt>
<registers>
<register>
<name>CR1</name>
<displayName>CR1</displayName>
<description>Control register 1</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>EOBIE</name>
<description>End of Block interrupt               enable</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RTOIE</name>
<description>Receiver timeout interrupt               enable</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DEAT</name>
<description>Driver Enable assertion               time</description>
<bitOffset>21</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>DEDT</name>
<description>Driver Enable deassertion               time</description>
<bitOffset>16</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>OVER8</name>
<description>Oversampling mode</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CMIE</name>
<description>Character match interrupt               enable</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MME</name>
<description>Mute mode enable</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>M</name>
<description>Word length</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>WAKE</name>
<description>Receiver wakeup method</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PCE</name>
<description>Parity control enable</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PS</name>
<description>Parity selection</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PEIE</name>
<description>PE interrupt enable</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TXEIE</name>
<description>interrupt enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TCIE</name>
<description>Transmission complete interrupt               enable</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RXNEIE</name>
<description>RXNE interrupt enable</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDLEIE</name>
<description>IDLE interrupt enable</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TE</name>
<description>Transmitter enable</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RE</name>
<description>Receiver enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UESM</name>
<description>USART enable in Stop mode</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UE</name>
<description>USART enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CR2</name>
<displayName>CR2</displayName>
<description>Control register 2</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>ADD4</name>
<description>Address of the USART node</description>
<bitOffset>28</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>ADD0</name>
<description>Address of the USART node</description>
<bitOffset>24</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>RTOEN</name>
<description>Receiver timeout enable</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ABRMOD</name>
<description>Auto baud rate mode</description>
<bitOffset>21</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>ABREN</name>
<description>Auto baud rate enable</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MSBFIRST</name>
<description>Most significant bit first</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DATAINV</name>
<description>Binary data inversion</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TXINV</name>
<description>TX pin active level               inversion</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RXINV</name>
<description>RX pin active level               inversion</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWAP</name>
<description>Swap TX/RX pins</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LINEN</name>
<description>LIN mode enable</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>STOP</name>
<description>STOP bits</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>CLKEN</name>
<description>Clock enable</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CPOL</name>
<description>Clock polarity</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CPHA</name>
<description>Clock phase</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LBCL</name>
<description>Last bit clock pulse</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LBDIE</name>
<description>LIN break detection interrupt               enable</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LBDL</name>
<description>LIN break detection length</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ADDM7</name>
<description>7-bit Address Detection/4-bit Address               Detection</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CR3</name>
<displayName>CR3</displayName>
<description>Control register 3</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>WUFIE</name>
<description>Wakeup from Stop mode interrupt               enable</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>WUS</name>
<description>Wakeup from Stop mode interrupt flag               selection</description>
<bitOffset>20</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>SCARCNT</name>
<description>Smartcard auto-retry count</description>
<bitOffset>17</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>DEP</name>
<description>Driver enable polarity               selection</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DEM</name>
<description>Driver enable mode</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DDRE</name>
<description>DMA Disable on Reception               Error</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OVRDIS</name>
<description>Overrun Disable</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ONEBIT</name>
<description>One sample bit method               enable</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CTSIE</name>
<description>CTS interrupt enable</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CTSE</name>
<description>CTS enable</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RTSE</name>
<description>RTS enable</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DMAT</name>
<description>DMA enable transmitter</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DMAR</name>
<description>DMA enable receiver</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SCEN</name>
<description>Smartcard mode enable</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>NACK</name>
<description>Smartcard NACK enable</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>HDSEL</name>
<description>Half-duplex selection</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IRLP</name>
<description>IrDA low-power</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IREN</name>
<description>IrDA mode enable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>EIE</name>
<description>Error interrupt enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>BRR</name>
<displayName>BRR</displayName>
<description>Baud rate register</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>DIV_Mantissa</name>
<description>mantissa of USARTDIV</description>
<bitOffset>4</bitOffset>
<bitWidth>12</bitWidth>
</field>
<field>
<name>DIV_Fraction</name>
<description>fraction of USARTDIV</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>GTPR</name>
<displayName>GTPR</displayName>
<description>Guard time and prescaler           register</description>
<addressOffset>0x10</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>GT</name>
<description>Guard time value</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>PSC</name>
<description>Prescaler value</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>RTOR</name>
<displayName>RTOR</displayName>
<description>Receiver timeout register</description>
<addressOffset>0x14</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>BLEN</name>
<description>Block Length</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>RTO</name>
<description>Receiver timeout value</description>
<bitOffset>0</bitOffset>
<bitWidth>24</bitWidth>
</field>
</fields>
</register>
<register>
<name>RQR</name>
<displayName>RQR</displayName>
<description>Request register</description>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>TXFRQ</name>
<description>Transmit data flush               request</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RXFRQ</name>
<description>Receive data flush request</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MMRQ</name>
<description>Mute mode request</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SBKRQ</name>
<description>Send break request</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ABRRQ</name>
<description>Auto baud rate request</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>ISR</name>
<displayName>ISR</displayName>
<description>Interrupt &amp; status           register</description>
<addressOffset>0x1C</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00C0</resetValue>
<fields>
<field>
<name>REACK</name>
<description>Receive enable acknowledge               flag</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TEACK</name>
<description>Transmit enable acknowledge               flag</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>WUF</name>
<description>Wakeup from Stop mode flag</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RWU</name>
<description>Receiver wakeup from Mute               mode</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SBKF</name>
<description>Send break flag</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CMF</name>
<description>character match flag</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BUSY</name>
<description>Busy flag</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ABRF</name>
<description>Auto baud rate flag</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ABRE</name>
<description>Auto baud rate error</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>EOBF</name>
<description>End of block flag</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RTOF</name>
<description>Receiver timeout</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CTS</name>
<description>CTS flag</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CTSIF</name>
<description>CTS interrupt flag</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LBDF</name>
<description>LIN break detection flag</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TXE</name>
<description>Transmit data register               empty</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TC</name>
<description>Transmission complete</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RXNE</name>
<description>Read data register not               empty</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDLE</name>
<description>Idle line detected</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ORE</name>
<description>Overrun error</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>NF</name>
<description>Noise detected flag</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FE</name>
<description>Framing error</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PE</name>
<description>Parity error</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>ICR</name>
<displayName>ICR</displayName>
<description>Interrupt flag clear register</description>
<addressOffset>0x20</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>WUCF</name>
<description>Wakeup from Stop mode clear               flag</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CMCF</name>
<description>Character match clear flag</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>EOBCF</name>
<description>End of timeout clear flag</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RTOCF</name>
<description>Receiver timeout clear               flag</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CTSCF</name>
<description>CTS clear flag</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LBDCF</name>
<description>LIN break detection clear               flag</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TCCF</name>
<description>Transmission complete clear               flag</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>IDLECF</name>
<description>Idle line detected clear               flag</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ORECF</name>
<description>Overrun error clear flag</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>NCF</name>
<description>Noise detected clear flag</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FECF</name>
<description>Framing error clear flag</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PECF</name>
<description>Parity error clear flag</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>RDR</name>
<displayName>RDR</displayName>
<description>Receive data register</description>
<addressOffset>0x24</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>RDR</name>
<description>Receive data value</description>
<bitOffset>0</bitOffset>
<bitWidth>9</bitWidth>
</field>
</fields>
</register>
<register>
<name>TDR</name>
<displayName>TDR</displayName>
<description>Transmit data register</description>
<addressOffset>0x28</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>TDR</name>
<description>Transmit data value</description>
<bitOffset>0</bitOffset>
<bitWidth>9</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral derivedFrom="USART1">
<name>USART2</name>
<baseAddress>0x40004400</baseAddress>
<interrupt>
<name>USART2_EXTI26</name>
<description>USART2 global interrupt and EXTI Line 26
        interrupt</description>
<value>38</value>
</interrupt>
</peripheral>
<peripheral derivedFrom="USART1">
<name>USART3</name>
<baseAddress>0x40004800</baseAddress>
<interrupt>
<name>USART3_EXTI28</name>
<description>USART3 global interrupt and EXTI Line 28
        interrupt</description>
<value>39</value>
</interrupt>
</peripheral>
<peripheral derivedFrom="USART1">
<name>UART4</name>
<baseAddress>0x40004C00</baseAddress>
<interrupt>
<name>UART4_EXTI34</name>
<description>UART4 global and EXTI Line 34
        interrupts</description>
<value>52</value>
</interrupt>
</peripheral>
<peripheral derivedFrom="USART1">
<name>UART5</name>
<baseAddress>0x40005000</baseAddress>
<interrupt>
<name>UART5_EXTI35</name>
<description>UART5 global and EXTI Line 35
        interrupts</description>
<value>53</value>
</interrupt>
</peripheral>
<peripheral>
<name>SPI1</name>
<description>Serial peripheral interface/Inter-IC       sound</description>
<groupName>SPI</groupName>
<baseAddress>0x40013000</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<interrupt>
<name>SPI1</name>
<description>SPI1 global interrupt</description>
<value>35</value>
</interrupt>
<registers>
<register>
<name>CR1</name>
<displayName>CR1</displayName>
<description>control register 1</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>BIDIMODE</name>
<description>Bidirectional data mode               enable</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BIDIOE</name>
<description>Output enable in bidirectional               mode</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CRCEN</name>
<description>Hardware CRC calculation               enable</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CRCNEXT</name>
<description>CRC transfer next</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DFF</name>
<description>Data frame format</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RXONLY</name>
<description>Receive only</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SSM</name>
<description>Software slave management</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SSI</name>
<description>Internal slave select</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LSBFIRST</name>
<description>Frame format</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SPE</name>
<description>SPI enable</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BR</name>
<description>Baud rate control</description>
<bitOffset>3</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>MSTR</name>
<description>Master selection</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CPOL</name>
<description>Clock polarity</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CPHA</name>
<description>Clock phase</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CR2</name>
<displayName>CR2</displayName>
<description>control register 2</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>RXDMAEN</name>
<description>Rx buffer DMA enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TXDMAEN</name>
<description>Tx buffer DMA enable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SSOE</name>
<description>SS output enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>NSSP</name>
<description>NSS pulse management</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FRF</name>
<description>Frame format</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ERRIE</name>
<description>Error interrupt enable</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RXNEIE</name>
<description>RX buffer not empty interrupt               enable</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TXEIE</name>
<description>Tx buffer empty interrupt               enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DS</name>
<description>Data size</description>
<bitOffset>8</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>FRXTH</name>
<description>FIFO reception threshold</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LDMA_RX</name>
<description>Last DMA transfer for               reception</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LDMA_TX</name>
<description>Last DMA transfer for               transmission</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>SR</name>
<displayName>SR</displayName>
<description>status register</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<resetValue>0x0002</resetValue>
<fields>
<field>
<name>RXNE</name>
<description>Receive buffer not empty</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>TXE</name>
<description>Transmit buffer empty</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>CHSIDE</name>
<description>Channel side</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>UDR</name>
<description>Underrun flag</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>CRCERR</name>
<description>CRC error flag</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>MODF</name>
<description>Mode fault</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>OVR</name>
<description>Overrun flag</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>BSY</name>
<description>Busy flag</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>TIFRFE</name>
<description>TI frame format error</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>FRLVL</name>
<description>FIFO reception level</description>
<bitOffset>9</bitOffset>
<bitWidth>2</bitWidth>
<access>read-only</access>
</field>
<field>
<name>FTLVL</name>
<description>FIFO transmission level</description>
<bitOffset>11</bitOffset>
<bitWidth>2</bitWidth>
<access>read-only</access>
</field>
</fields>
</register>
<register>
<name>DR</name>
<displayName>DR</displayName>
<description>data register</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>DR</name>
<description>Data register</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>CRCPR</name>
<displayName>CRCPR</displayName>
<description>CRC polynomial register</description>
<addressOffset>0x10</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0007</resetValue>
<fields>
<field>
<name>CRCPOLY</name>
<description>CRC polynomial register</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>RXCRCR</name>
<displayName>RXCRCR</displayName>
<description>RX CRC register</description>
<addressOffset>0x14</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>RxCRC</name>
<description>Rx CRC register</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>TXCRCR</name>
<displayName>TXCRCR</displayName>
<description>TX CRC register</description>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>TxCRC</name>
<description>Tx CRC register</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>I2SCFGR</name>
<displayName>I2SCFGR</displayName>
<description>I2S configuration register</description>
<addressOffset>0x1C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>I2SMOD</name>
<description>I2S mode selection</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>I2SE</name>
<description>I2S Enable</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>I2SCFG</name>
<description>I2S configuration mode</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PCMSYNC</name>
<description>PCM frame synchronization</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>I2SSTD</name>
<description>I2S standard selection</description>
<bitOffset>4</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>CKPOL</name>
<description>Steady state clock               polarity</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DATLEN</name>
<description>Data length to be               transferred</description>
<bitOffset>1</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>CHLEN</name>
<description>Channel length (number of bits per audio               channel)</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>I2SPR</name>
<displayName>I2SPR</displayName>
<description>I2S prescaler register</description>
<addressOffset>0x20</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000010</resetValue>
<fields>
<field>
<name>MCKOE</name>
<description>Master clock output enable</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ODD</name>
<description>Odd factor for the               prescaler</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>I2SDIV</name>
<description>I2S Linear prescaler</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral derivedFrom="SPI1">
<name>SPI2</name>
<baseAddress>0x40003800</baseAddress>
<interrupt>
<name>SPI2</name>
<description>SPI2 global interrupt</description>
<value>36</value>
</interrupt>
</peripheral>
<peripheral derivedFrom="SPI1">
<name>SPI3</name>
<baseAddress>0x40003C00</baseAddress>
<interrupt>
<name>SPI3</name>
<description>SPI3 global interrupt</description>
<value>51</value>
</interrupt>
</peripheral>
<peripheral derivedFrom="SPI1">
<name>I2S2ext</name>
<baseAddress>0x40003400</baseAddress>
</peripheral>
<peripheral derivedFrom="SPI1">
<name>I2S3ext</name>
<baseAddress>0x40004000</baseAddress>
</peripheral>
<peripheral derivedFrom="SPI1">
<name>SPI4</name>
<baseAddress>0x40013C00</baseAddress>
<interrupt>
<name>SPI3</name>
<description>SPI3 global interrupt</description>
<value>51</value>
</interrupt>
</peripheral>
<peripheral>
<name>EXTI</name>
<description>External interrupt/event       controller</description>
<groupName>EXTI</groupName>
<baseAddress>0x40010400</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<interrupt>
<name>TAMP_STAMP</name>
<description>Tamper and TimeStamp interrupts</description>
<value>2</value>
</interrupt>
<interrupt>
<name>EXTI0</name>
<description>EXTI Line0 interrupt</description>
<value>6</value>
</interrupt>
<interrupt>
<name>EXTI1</name>
<description>EXTI Line3 interrupt</description>
<value>7</value>
</interrupt>
<interrupt>
<name>EXTI2_TSC</name>
<description>EXTI Line2 and Touch sensing
        interrupts</description>
<value>8</value>
</interrupt>
<interrupt>
<name>EXTI3</name>
<description>EXTI Line3 interrupt</description>
<value>9</value>
</interrupt>
<interrupt>
<name>EXTI4</name>
<description>EXTI Line4 interrupt</description>
<value>10</value>
</interrupt>
<interrupt>
<name>EXTI9_5</name>
<description>EXTI Line5 to Line9 interrupts</description>
<value>23</value>
</interrupt>
<interrupt>
<name>I2C1_EV_EXTI23</name>
<description>I2C1 event interrupt and EXTI Line23
        interrupt</description>
<value>31</value>
</interrupt>
<interrupt>
<name>USART1_EXTI25</name>
<description>USART1 global interrupt and EXTI Line 25
        interrupt</description>
<value>37</value>
</interrupt>
<interrupt>
<name>USART2_EXTI26</name>
<description>USART2 global interrupt and EXTI Line 26
        interrupt</description>
<value>38</value>
</interrupt>
<interrupt>
<name>USART3_EXTI28</name>
<description>USART3 global interrupt and EXTI Line 28
        interrupt</description>
<value>39</value>
</interrupt>
<interrupt>
<name>EXTI15_10</name>
<description>EXTI Line15 to Line10 interrupts</description>
<value>40</value>
</interrupt>
<interrupt>
<name>UART4_EXTI34</name>
<description>UART4 global and EXTI Line 34
        interrupts</description>
<value>52</value>
</interrupt>
<interrupt>
<name>UART5_EXTI35</name>
<description>UART5 global and EXTI Line 35
        interrupts</description>
<value>53</value>
</interrupt>
<interrupt>
<name>USB_WKUP_EXTI</name>
<description>USB wakeup from Suspend and EXTI Line
        18</description>
<value>76</value>
</interrupt>
<registers>
<register>
<name>IMR1</name>
<displayName>IMR1</displayName>
<description>Interrupt mask register</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x1F800000</resetValue>
<fields>
<field>
<name>MR0</name>
<description>Interrupt Mask on line 0</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR1</name>
<description>Interrupt Mask on line 1</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR2</name>
<description>Interrupt Mask on line 2</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR3</name>
<description>Interrupt Mask on line 3</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR4</name>
<description>Interrupt Mask on line 4</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR5</name>
<description>Interrupt Mask on line 5</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR6</name>
<description>Interrupt Mask on line 6</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR7</name>
<description>Interrupt Mask on line 7</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR8</name>
<description>Interrupt Mask on line 8</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR9</name>
<description>Interrupt Mask on line 9</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR10</name>
<description>Interrupt Mask on line 10</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR11</name>
<description>Interrupt Mask on line 11</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR12</name>
<description>Interrupt Mask on line 12</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR13</name>
<description>Interrupt Mask on line 13</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR14</name>
<description>Interrupt Mask on line 14</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR15</name>
<description>Interrupt Mask on line 15</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR16</name>
<description>Interrupt Mask on line 16</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR17</name>
<description>Interrupt Mask on line 17</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR18</name>
<description>Interrupt Mask on line 18</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR19</name>
<description>Interrupt Mask on line 19</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR20</name>
<description>Interrupt Mask on line 20</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR21</name>
<description>Interrupt Mask on line 21</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR22</name>
<description>Interrupt Mask on line 22</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR23</name>
<description>Interrupt Mask on line 23</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR24</name>
<description>Interrupt Mask on line 24</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR25</name>
<description>Interrupt Mask on line 25</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR26</name>
<description>Interrupt Mask on line 26</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR27</name>
<description>Interrupt Mask on line 27</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR28</name>
<description>Interrupt Mask on line 28</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR29</name>
<description>Interrupt Mask on line 29</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR30</name>
<description>Interrupt Mask on line 30</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR31</name>
<description>Interrupt Mask on line 31</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>EMR1</name>
<displayName>EMR1</displayName>
<description>Event mask register</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>MR0</name>
<description>Event Mask on line 0</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR1</name>
<description>Event Mask on line 1</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR2</name>
<description>Event Mask on line 2</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR3</name>
<description>Event Mask on line 3</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR4</name>
<description>Event Mask on line 4</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR5</name>
<description>Event Mask on line 5</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR6</name>
<description>Event Mask on line 6</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR7</name>
<description>Event Mask on line 7</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR8</name>
<description>Event Mask on line 8</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR9</name>
<description>Event Mask on line 9</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR10</name>
<description>Event Mask on line 10</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR11</name>
<description>Event Mask on line 11</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR12</name>
<description>Event Mask on line 12</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR13</name>
<description>Event Mask on line 13</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR14</name>
<description>Event Mask on line 14</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR15</name>
<description>Event Mask on line 15</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR16</name>
<description>Event Mask on line 16</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR17</name>
<description>Event Mask on line 17</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR18</name>
<description>Event Mask on line 18</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR19</name>
<description>Event Mask on line 19</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR20</name>
<description>Event Mask on line 20</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR21</name>
<description>Event Mask on line 21</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR22</name>
<description>Event Mask on line 22</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR23</name>
<description>Event Mask on line 23</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR24</name>
<description>Event Mask on line 24</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR25</name>
<description>Event Mask on line 25</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR26</name>
<description>Event Mask on line 26</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR27</name>
<description>Event Mask on line 27</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR28</name>
<description>Event Mask on line 28</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR29</name>
<description>Event Mask on line 29</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR30</name>
<description>Event Mask on line 30</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR31</name>
<description>Event Mask on line 31</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>RTSR1</name>
<displayName>RTSR1</displayName>
<description>Rising Trigger selection           register</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>TR0</name>
<description>Rising trigger event configuration of               line 0</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR1</name>
<description>Rising trigger event configuration of               line 1</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR2</name>
<description>Rising trigger event configuration of               line 2</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR3</name>
<description>Rising trigger event configuration of               line 3</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR4</name>
<description>Rising trigger event configuration of               line 4</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR5</name>
<description>Rising trigger event configuration of               line 5</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR6</name>
<description>Rising trigger event configuration of               line 6</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR7</name>
<description>Rising trigger event configuration of               line 7</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR8</name>
<description>Rising trigger event configuration of               line 8</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR9</name>
<description>Rising trigger event configuration of               line 9</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR10</name>
<description>Rising trigger event configuration of               line 10</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR11</name>
<description>Rising trigger event configuration of               line 11</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR12</name>
<description>Rising trigger event configuration of               line 12</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR13</name>
<description>Rising trigger event configuration of               line 13</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR14</name>
<description>Rising trigger event configuration of               line 14</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR15</name>
<description>Rising trigger event configuration of               line 15</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR16</name>
<description>Rising trigger event configuration of               line 16</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR17</name>
<description>Rising trigger event configuration of               line 17</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR18</name>
<description>Rising trigger event configuration of               line 18</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR19</name>
<description>Rising trigger event configuration of               line 19</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR20</name>
<description>Rising trigger event configuration of               line 20</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR21</name>
<description>Rising trigger event configuration of               line 21</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR22</name>
<description>Rising trigger event configuration of               line 22</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR29</name>
<description>Rising trigger event configuration of               line 29</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR30</name>
<description>Rising trigger event configuration of               line 30</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR31</name>
<description>Rising trigger event configuration of               line 31</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>FTSR1</name>
<displayName>FTSR1</displayName>
<description>Falling Trigger selection           register</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>TR0</name>
<description>Falling trigger event configuration of               line 0</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR1</name>
<description>Falling trigger event configuration of               line 1</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR2</name>
<description>Falling trigger event configuration of               line 2</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR3</name>
<description>Falling trigger event configuration of               line 3</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR4</name>
<description>Falling trigger event configuration of               line 4</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR5</name>
<description>Falling trigger event configuration of               line 5</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR6</name>
<description>Falling trigger event configuration of               line 6</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR7</name>
<description>Falling trigger event configuration of               line 7</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR8</name>
<description>Falling trigger event configuration of               line 8</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR9</name>
<description>Falling trigger event configuration of               line 9</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR10</name>
<description>Falling trigger event configuration of               line 10</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR11</name>
<description>Falling trigger event configuration of               line 11</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR12</name>
<description>Falling trigger event configuration of               line 12</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR13</name>
<description>Falling trigger event configuration of               line 13</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR14</name>
<description>Falling trigger event configuration of               line 14</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR15</name>
<description>Falling trigger event configuration of               line 15</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR16</name>
<description>Falling trigger event configuration of               line 16</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR17</name>
<description>Falling trigger event configuration of               line 17</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR18</name>
<description>Falling trigger event configuration of               line 18</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR19</name>
<description>Falling trigger event configuration of               line 19</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR20</name>
<description>Falling trigger event configuration of               line 20</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR21</name>
<description>Falling trigger event configuration of               line 21</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR22</name>
<description>Falling trigger event configuration of               line 22</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR29</name>
<description>Falling trigger event configuration of               line 29</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR30</name>
<description>Falling trigger event configuration of               line 30.</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR31</name>
<description>Falling trigger event configuration of               line 31</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>SWIER1</name>
<displayName>SWIER1</displayName>
<description>Software interrupt event           register</description>
<addressOffset>0x10</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>SWIER0</name>
<description>Software Interrupt on line               0</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER1</name>
<description>Software Interrupt on line               1</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER2</name>
<description>Software Interrupt on line               2</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER3</name>
<description>Software Interrupt on line               3</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER4</name>
<description>Software Interrupt on line               4</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER5</name>
<description>Software Interrupt on line               5</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER6</name>
<description>Software Interrupt on line               6</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER7</name>
<description>Software Interrupt on line               7</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER8</name>
<description>Software Interrupt on line               8</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER9</name>
<description>Software Interrupt on line               9</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER10</name>
<description>Software Interrupt on line               10</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER11</name>
<description>Software Interrupt on line               11</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER12</name>
<description>Software Interrupt on line               12</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER13</name>
<description>Software Interrupt on line               13</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER14</name>
<description>Software Interrupt on line               14</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER15</name>
<description>Software Interrupt on line               15</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER16</name>
<description>Software Interrupt on line               16</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER17</name>
<description>Software Interrupt on line               17</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER18</name>
<description>Software Interrupt on line               18</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER19</name>
<description>Software Interrupt on line               19</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER20</name>
<description>Software Interrupt on line               20</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER21</name>
<description>Software Interrupt on line               21</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER22</name>
<description>Software Interrupt on line               22</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER29</name>
<description>Software Interrupt on line               29</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER30</name>
<description>Software Interrupt on line               309</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER31</name>
<description>Software Interrupt on line               319</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>PR1</name>
<displayName>PR1</displayName>
<description>Pending register</description>
<addressOffset>0x14</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>PR0</name>
<description>Pending bit 0</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR1</name>
<description>Pending bit 1</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR2</name>
<description>Pending bit 2</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR3</name>
<description>Pending bit 3</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR4</name>
<description>Pending bit 4</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR5</name>
<description>Pending bit 5</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR6</name>
<description>Pending bit 6</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR7</name>
<description>Pending bit 7</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR8</name>
<description>Pending bit 8</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR9</name>
<description>Pending bit 9</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR10</name>
<description>Pending bit 10</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR11</name>
<description>Pending bit 11</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR12</name>
<description>Pending bit 12</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR13</name>
<description>Pending bit 13</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR14</name>
<description>Pending bit 14</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR15</name>
<description>Pending bit 15</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR16</name>
<description>Pending bit 16</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR17</name>
<description>Pending bit 17</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR18</name>
<description>Pending bit 18</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR19</name>
<description>Pending bit 19</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR20</name>
<description>Pending bit 20</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR21</name>
<description>Pending bit 21</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR22</name>
<description>Pending bit 22</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR29</name>
<description>Pending bit 29</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR30</name>
<description>Pending bit 30</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR31</name>
<description>Pending bit 31</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>IMR2</name>
<displayName>IMR2</displayName>
<description>Interrupt mask register</description>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0xFFFFFFFC</resetValue>
<fields>
<field>
<name>MR32</name>
<description>Interrupt Mask on external/internal line               32</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR33</name>
<description>Interrupt Mask on external/internal line               33</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR34</name>
<description>Interrupt Mask on external/internal line               34</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR35</name>
<description>Interrupt Mask on external/internal line               35</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>EMR2</name>
<displayName>EMR2</displayName>
<description>Event mask register</description>
<addressOffset>0x1C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>MR32</name>
<description>Event mask on external/internal line               32</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR33</name>
<description>Event mask on external/internal line               33</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR34</name>
<description>Event mask on external/internal line               34</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MR35</name>
<description>Event mask on external/internal line               35</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>RTSR2</name>
<displayName>RTSR2</displayName>
<description>Rising Trigger selection           register</description>
<addressOffset>0x20</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>TR32</name>
<description>Rising trigger event configuration bit               of line 32</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR33</name>
<description>Rising trigger event configuration bit               of line 33</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>FTSR2</name>
<displayName>FTSR2</displayName>
<description>Falling Trigger selection           register</description>
<addressOffset>0x24</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>TR32</name>
<description>Falling trigger event configuration bit               of line 32</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TR33</name>
<description>Falling trigger event configuration bit               of line 33</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>SWIER2</name>
<displayName>SWIER2</displayName>
<description>Software interrupt event           register</description>
<addressOffset>0x28</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>SWIER32</name>
<description>Software interrupt on line               32</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWIER33</name>
<description>Software interrupt on line               33</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>PR2</name>
<displayName>PR2</displayName>
<description>Pending register</description>
<addressOffset>0x2C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>PR32</name>
<description>Pending bit on line 32</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PR33</name>
<description>Pending bit on line 33</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral>
<name>COMP</name>
<description>Comparator</description>
<groupName>COMP</groupName>
<baseAddress>0x4001001C</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x19</size>
<usage>registers</usage>
</addressBlock>
<interrupt>
<name>COMP123</name>
<description>COMP1 &amp; COMP2 &amp; COMP3 interrupts
        combined with EXTI Lines 21, 22 and 29
        interrupts</description>
<value>64</value>
</interrupt>
<interrupt>
<name>COMP456</name>
<description>COMP4 &amp; COMP5 &amp; COMP6 interrupts
        combined with EXTI Lines 30, 31 and 32
        interrupts</description>
<value>65</value>
</interrupt>
<interrupt>
<name>COMP7</name>
<description>COMP7 interrupt combined with EXTI Line 33
        interrupt</description>
<value>66</value>
</interrupt>
<registers>
<register>
<name>COMP1_CSR</name>
<displayName>COMP1_CSR</displayName>
<description>control and status register</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>COMP1EN</name>
<description>Comparator 1 enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP1_INP_DAC</name>
<description>COMP1_INP_DAC</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP1MODE</name>
<description>Comparator 1 mode</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP1INSEL</name>
<description>Comparator 1 inverting input               selection</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP1_OUT_SEL</name>
<description>Comparator 1 output               selection</description>
<bitOffset>10</bitOffset>
<bitWidth>4</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP1POL</name>
<description>Comparator 1 output               polarity</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP1HYST</name>
<description>Comparator 1 hysteresis</description>
<bitOffset>16</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP1_BLANKING</name>
<description>Comparator 1 blanking               source</description>
<bitOffset>18</bitOffset>
<bitWidth>3</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP1OUT</name>
<description>Comparator 1 output</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>COMP1LOCK</name>
<description>Comparator 1 lock</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
<register>
<name>COMP2_CSR</name>
<displayName>COMP2_CSR</displayName>
<description>control and status register</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>COMP2EN</name>
<description>Comparator 2 enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>COMP2MODE</name>
<description>Comparator 2 mode</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>COMP2INSEL</name>
<description>Comparator 2 inverting input               selection</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>COMP2INPSEL</name>
<description>Comparator 2 non inverted input               selection</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>COMP2INMSEL</name>
<description>Comparator 1inverting input               selection</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>COMP2_OUT_SEL</name>
<description>Comparator 2 output               selection</description>
<bitOffset>10</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>COMP2POL</name>
<description>Comparator 2 output               polarity</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>COMP2HYST</name>
<description>Comparator 2 hysteresis</description>
<bitOffset>16</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>COMP2_BLANKING</name>
<description>Comparator 2 blanking               source</description>
<bitOffset>18</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>COMP2LOCK</name>
<description>Comparator 2 lock</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>COMP3_CSR</name>
<displayName>COMP3_CSR</displayName>
<description>control and status register</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>COMP3EN</name>
<description>Comparator 3 enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP3MODE</name>
<description>Comparator 3 mode</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP3INSEL</name>
<description>Comparator 3 inverting input               selection</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP3INPSEL</name>
<description>Comparator 3 non inverted input               selection</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP3_OUT_SEL</name>
<description>Comparator 3 output               selection</description>
<bitOffset>10</bitOffset>
<bitWidth>4</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP3POL</name>
<description>Comparator 3 output               polarity</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP3HYST</name>
<description>Comparator 3 hysteresis</description>
<bitOffset>16</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP3_BLANKING</name>
<description>Comparator 3 blanking               source</description>
<bitOffset>18</bitOffset>
<bitWidth>3</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP3OUT</name>
<description>Comparator 3 output</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>COMP3LOCK</name>
<description>Comparator 3 lock</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
<register>
<name>COMP4_CSR</name>
<displayName>COMP4_CSR</displayName>
<description>control and status register</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>COMP4EN</name>
<description>Comparator 4 enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP4MODE</name>
<description>Comparator 4 mode</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP4INSEL</name>
<description>Comparator 4 inverting input               selection</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP4INPSEL</name>
<description>Comparator 4 non inverted input               selection</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COM4WINMODE</name>
<description>Comparator 4 window mode</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP4_OUT_SEL</name>
<description>Comparator 4 output               selection</description>
<bitOffset>10</bitOffset>
<bitWidth>4</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP4POL</name>
<description>Comparator 4 output               polarity</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP4HYST</name>
<description>Comparator 4 hysteresis</description>
<bitOffset>16</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP4_BLANKING</name>
<description>Comparator 4 blanking               source</description>
<bitOffset>18</bitOffset>
<bitWidth>3</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP4OUT</name>
<description>Comparator 4 output</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>COMP4LOCK</name>
<description>Comparator 4 lock</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
<register>
<name>COMP5_CSR</name>
<displayName>COMP5_CSR</displayName>
<description>control and status register</description>
<addressOffset>0x10</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>COMP5EN</name>
<description>Comparator 5 enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP5MODE</name>
<description>Comparator 5 mode</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP5INSEL</name>
<description>Comparator 5 inverting input               selection</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP5INPSEL</name>
<description>Comparator 5 non inverted input               selection</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP5_OUT_SEL</name>
<description>Comparator 5 output               selection</description>
<bitOffset>10</bitOffset>
<bitWidth>4</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP5POL</name>
<description>Comparator 5 output               polarity</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP5HYST</name>
<description>Comparator 5 hysteresis</description>
<bitOffset>16</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP5_BLANKING</name>
<description>Comparator 5 blanking               source</description>
<bitOffset>18</bitOffset>
<bitWidth>3</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP5OUT</name>
<description>Comparator51 output</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>COMP5LOCK</name>
<description>Comparator 5 lock</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
<register>
<name>COMP6_CSR</name>
<displayName>COMP6_CSR</displayName>
<description>control and status register</description>
<addressOffset>0x14</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>COMP6EN</name>
<description>Comparator 6 enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP6MODE</name>
<description>Comparator 6 mode</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP6INSEL</name>
<description>Comparator 6 inverting input               selection</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP6INPSEL</name>
<description>Comparator 6 non inverted input               selection</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COM6WINMODE</name>
<description>Comparator 6 window mode</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP6_OUT_SEL</name>
<description>Comparator 6 output               selection</description>
<bitOffset>10</bitOffset>
<bitWidth>4</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP6POL</name>
<description>Comparator 6 output               polarity</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP6HYST</name>
<description>Comparator 6 hysteresis</description>
<bitOffset>16</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP6_BLANKING</name>
<description>Comparator 6 blanking               source</description>
<bitOffset>18</bitOffset>
<bitWidth>3</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP6OUT</name>
<description>Comparator 6 output</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>COMP6LOCK</name>
<description>Comparator 6 lock</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
<register>
<name>COMP7_CSR</name>
<displayName>COMP7_CSR</displayName>
<description>control and status register</description>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>COMP7EN</name>
<description>Comparator 7 enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP7MODE</name>
<description>Comparator 7 mode</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP7INSEL</name>
<description>Comparator 7 inverting input               selection</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP7INPSEL</name>
<description>Comparator 7 non inverted input               selection</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP7_OUT_SEL</name>
<description>Comparator 7 output               selection</description>
<bitOffset>10</bitOffset>
<bitWidth>4</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP7POL</name>
<description>Comparator 7 output               polarity</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP7HYST</name>
<description>Comparator 7 hysteresis</description>
<bitOffset>16</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP7_BLANKING</name>
<description>Comparator 7 blanking               source</description>
<bitOffset>18</bitOffset>
<bitWidth>3</bitWidth>
<access>read-write</access>
</field>
<field>
<name>COMP7OUT</name>
<description>Comparator 7 output</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>COMP7LOCK</name>
<description>Comparator 7 lock</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral>
<name>PWR</name>
<description>Power control</description>
<groupName>PWR</groupName>
<baseAddress>0x40007000</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<interrupt>
<name>PVD</name>
<description>PVD through EXTI line detection
        interrupt</description>
<value>1</value>
</interrupt>
<registers>
<register>
<name>CR</name>
<displayName>CR</displayName>
<description>power control register</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>LPDS</name>
<description>Low-power deep sleep</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PDDS</name>
<description>Power down deepsleep</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CWUF</name>
<description>Clear wakeup flag</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CSBF</name>
<description>Clear standby flag</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PVDE</name>
<description>Power voltage detector               enable</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PLS</name>
<description>PVD level selection</description>
<bitOffset>5</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>DBP</name>
<description>Disable backup domain write               protection</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CSR</name>
<displayName>CSR</displayName>
<description>power control/status register</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>WUF</name>
<description>Wakeup flag</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>SBF</name>
<description>Standby flag</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>PVDO</name>
<description>PVD output</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>EWUP1</name>
<description>Enable WKUP1 pin</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>EWUP2</name>
<description>Enable WKUP2 pin</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral>
<name>CAN</name>
<description>Controller area network</description>
<groupName>CAN</groupName>
<baseAddress>0x40006400</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<interrupt>
<name>USB_HP_CAN_TX</name>
<description>USB High Priority/CAN_TX
        interrupts</description>
<value>19</value>
</interrupt>
<interrupt>
<name>USB_LP_CAN_RX0</name>
<description>USB Low Priority/CAN_RX0
        interrupts</description>
<value>20</value>
</interrupt>
<interrupt>
<name>CAN_RX1</name>
<description>CAN_RX1 interrupt</description>
<value>21</value>
</interrupt>
<interrupt>
<name>CAN_SCE</name>
<description>CAN_SCE interrupt</description>
<value>22</value>
</interrupt>
<registers>
<register>
<name>MCR</name>
<displayName>MCR</displayName>
<description>master control register</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00010002</resetValue>
<fields>
<field>
<name>DBF</name>
<description>DBF</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RESET</name>
<description>RESET</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TTCM</name>
<description>TTCM</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ABOM</name>
<description>ABOM</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>AWUM</name>
<description>AWUM</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>NART</name>
<description>NART</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RFLM</name>
<description>RFLM</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TXFP</name>
<description>TXFP</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SLEEP</name>
<description>SLEEP</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>INRQ</name>
<description>INRQ</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>MSR</name>
<displayName>MSR</displayName>
<description>master status register</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<resetValue>0x00000C02</resetValue>
<fields>
<field>
<name>RX</name>
<description>RX</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>SAMP</name>
<description>SAMP</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>RXM</name>
<description>RXM</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>TXM</name>
<description>TXM</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>SLAKI</name>
<description>SLAKI</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>WKUI</name>
<description>WKUI</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>ERRI</name>
<description>ERRI</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>SLAK</name>
<description>SLAK</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>INAK</name>
<description>INAK</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
</fields>
</register>
<register>
<name>TSR</name>
<displayName>TSR</displayName>
<description>transmit status register</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<resetValue>0x1C000000</resetValue>
<fields>
<field>
<name>LOW2</name>
<description>Lowest priority flag for mailbox               2</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>LOW1</name>
<description>Lowest priority flag for mailbox               1</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>LOW0</name>
<description>Lowest priority flag for mailbox               0</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>TME2</name>
<description>Lowest priority flag for mailbox               2</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>TME1</name>
<description>Lowest priority flag for mailbox               1</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>TME0</name>
<description>Lowest priority flag for mailbox               0</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>CODE</name>
<description>CODE</description>
<bitOffset>24</bitOffset>
<bitWidth>2</bitWidth>
<access>read-only</access>
</field>
<field>
<name>ABRQ2</name>
<description>ABRQ2</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TERR2</name>
<description>TERR2</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>ALST2</name>
<description>ALST2</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TXOK2</name>
<description>TXOK2</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>RQCP2</name>
<description>RQCP2</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>ABRQ1</name>
<description>ABRQ1</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TERR1</name>
<description>TERR1</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>ALST1</name>
<description>ALST1</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TXOK1</name>
<description>TXOK1</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>RQCP1</name>
<description>RQCP1</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>ABRQ0</name>
<description>ABRQ0</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TERR0</name>
<description>TERR0</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>ALST0</name>
<description>ALST0</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TXOK0</name>
<description>TXOK0</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>RQCP0</name>
<description>RQCP0</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
<register>
<name>RF0R</name>
<displayName>RF0R</displayName>
<description>receive FIFO 0 register</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>RFOM0</name>
<description>RFOM0</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>FOVR0</name>
<description>FOVR0</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>FULL0</name>
<description>FULL0</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>FMP0</name>
<description>FMP0</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
<access>read-only</access>
</field>
</fields>
</register>
<register>
<name>RF1R</name>
<displayName>RF1R</displayName>
<description>receive FIFO 1 register</description>
<addressOffset>0x10</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>RFOM1</name>
<description>RFOM1</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>FOVR1</name>
<description>FOVR1</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>FULL1</name>
<description>FULL1</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>FMP1</name>
<description>FMP1</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
<access>read-only</access>
</field>
</fields>
</register>
<register>
<name>IER</name>
<displayName>IER</displayName>
<description>interrupt enable register</description>
<addressOffset>0x14</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>SLKIE</name>
<description>SLKIE</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>WKUIE</name>
<description>WKUIE</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ERRIE</name>
<description>ERRIE</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LECIE</name>
<description>LECIE</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BOFIE</name>
<description>BOFIE</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>EPVIE</name>
<description>EPVIE</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>EWGIE</name>
<description>EWGIE</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FOVIE1</name>
<description>FOVIE1</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFIE1</name>
<description>FFIE1</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FMPIE1</name>
<description>FMPIE1</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FOVIE0</name>
<description>FOVIE0</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFIE0</name>
<description>FFIE0</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FMPIE0</name>
<description>FMPIE0</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TMEIE</name>
<description>TMEIE</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>ESR</name>
<displayName>ESR</displayName>
<description>error status register</description>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>REC</name>
<description>REC</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
<access>read-only</access>
</field>
<field>
<name>TEC</name>
<description>TEC</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
<access>read-only</access>
</field>
<field>
<name>LEC</name>
<description>LEC</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
<access>read-write</access>
</field>
<field>
<name>BOFF</name>
<description>BOFF</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>EPVF</name>
<description>EPVF</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>EWGF</name>
<description>EWGF</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
</fields>
</register>
<register>
<name>BTR</name>
<displayName>BTR</displayName>
<description>bit timing register</description>
<addressOffset>0x1C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x01230000</resetValue>
<fields>
<field>
<name>SILM</name>
<description>SILM</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LBKM</name>
<description>LBKM</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SJW</name>
<description>SJW</description>
<bitOffset>24</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>TS2</name>
<description>TS2</description>
<bitOffset>20</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>TS1</name>
<description>TS1</description>
<bitOffset>16</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>BRP</name>
<description>BRP</description>
<bitOffset>0</bitOffset>
<bitWidth>10</bitWidth>
</field>
</fields>
</register>
<register>
<name>TI0R</name>
<displayName>TI0R</displayName>
<description>TX mailbox identifier register</description>
<addressOffset>0x180</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>STID</name>
<description>STID</description>
<bitOffset>21</bitOffset>
<bitWidth>11</bitWidth>
</field>
<field>
<name>EXID</name>
<description>EXID</description>
<bitOffset>3</bitOffset>
<bitWidth>18</bitWidth>
</field>
<field>
<name>IDE</name>
<description>IDE</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RTR</name>
<description>RTR</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TXRQ</name>
<description>TXRQ</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>TDT0R</name>
<displayName>TDT0R</displayName>
<description>mailbox data length control and time stamp           register</description>
<addressOffset>0x184</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>TIME</name>
<description>TIME</description>
<bitOffset>16</bitOffset>
<bitWidth>16</bitWidth>
</field>
<field>
<name>TGT</name>
<description>TGT</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DLC</name>
<description>DLC</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>TDL0R</name>
<displayName>TDL0R</displayName>
<description>mailbox data low register</description>
<addressOffset>0x188</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DATA3</name>
<description>DATA3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA2</name>
<description>DATA2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA1</name>
<description>DATA1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA0</name>
<description>DATA0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>TDH0R</name>
<displayName>TDH0R</displayName>
<description>mailbox data high register</description>
<addressOffset>0x18C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DATA7</name>
<description>DATA7</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA6</name>
<description>DATA6</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA5</name>
<description>DATA5</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA4</name>
<description>DATA4</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>TI1R</name>
<displayName>TI1R</displayName>
<description>TX mailbox identifier register</description>
<addressOffset>0x190</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>STID</name>
<description>STID</description>
<bitOffset>21</bitOffset>
<bitWidth>11</bitWidth>
</field>
<field>
<name>EXID</name>
<description>EXID</description>
<bitOffset>3</bitOffset>
<bitWidth>18</bitWidth>
</field>
<field>
<name>IDE</name>
<description>IDE</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RTR</name>
<description>RTR</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TXRQ</name>
<description>TXRQ</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>TDT1R</name>
<displayName>TDT1R</displayName>
<description>mailbox data length control and time stamp           register</description>
<addressOffset>0x194</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>TIME</name>
<description>TIME</description>
<bitOffset>16</bitOffset>
<bitWidth>16</bitWidth>
</field>
<field>
<name>TGT</name>
<description>TGT</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DLC</name>
<description>DLC</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>TDL1R</name>
<displayName>TDL1R</displayName>
<description>mailbox data low register</description>
<addressOffset>0x198</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DATA3</name>
<description>DATA3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA2</name>
<description>DATA2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA1</name>
<description>DATA1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA0</name>
<description>DATA0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>TDH1R</name>
<displayName>TDH1R</displayName>
<description>mailbox data high register</description>
<addressOffset>0x19C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DATA7</name>
<description>DATA7</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA6</name>
<description>DATA6</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA5</name>
<description>DATA5</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA4</name>
<description>DATA4</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>TI2R</name>
<displayName>TI2R</displayName>
<description>TX mailbox identifier register</description>
<addressOffset>0x1A0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>STID</name>
<description>STID</description>
<bitOffset>21</bitOffset>
<bitWidth>11</bitWidth>
</field>
<field>
<name>EXID</name>
<description>EXID</description>
<bitOffset>3</bitOffset>
<bitWidth>18</bitWidth>
</field>
<field>
<name>IDE</name>
<description>IDE</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RTR</name>
<description>RTR</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TXRQ</name>
<description>TXRQ</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>TDT2R</name>
<displayName>TDT2R</displayName>
<description>mailbox data length control and time stamp           register</description>
<addressOffset>0x1A4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>TIME</name>
<description>TIME</description>
<bitOffset>16</bitOffset>
<bitWidth>16</bitWidth>
</field>
<field>
<name>TGT</name>
<description>TGT</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DLC</name>
<description>DLC</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>TDL2R</name>
<displayName>TDL2R</displayName>
<description>mailbox data low register</description>
<addressOffset>0x1A8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DATA3</name>
<description>DATA3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA2</name>
<description>DATA2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA1</name>
<description>DATA1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA0</name>
<description>DATA0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>TDH2R</name>
<displayName>TDH2R</displayName>
<description>mailbox data high register</description>
<addressOffset>0x1AC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DATA7</name>
<description>DATA7</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA6</name>
<description>DATA6</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA5</name>
<description>DATA5</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA4</name>
<description>DATA4</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>RI0R</name>
<displayName>RI0R</displayName>
<description>receive FIFO mailbox identifier           register</description>
<addressOffset>0x1B0</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>STID</name>
<description>STID</description>
<bitOffset>21</bitOffset>
<bitWidth>11</bitWidth>
</field>
<field>
<name>EXID</name>
<description>EXID</description>
<bitOffset>3</bitOffset>
<bitWidth>18</bitWidth>
</field>
<field>
<name>IDE</name>
<description>IDE</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RTR</name>
<description>RTR</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>RDT0R</name>
<displayName>RDT0R</displayName>
<description>receive FIFO mailbox data length control and           time stamp register</description>
<addressOffset>0x1B4</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>TIME</name>
<description>TIME</description>
<bitOffset>16</bitOffset>
<bitWidth>16</bitWidth>
</field>
<field>
<name>FMI</name>
<description>FMI</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DLC</name>
<description>DLC</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>RDL0R</name>
<displayName>RDL0R</displayName>
<description>receive FIFO mailbox data low           register</description>
<addressOffset>0x1B8</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DATA3</name>
<description>DATA3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA2</name>
<description>DATA2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA1</name>
<description>DATA1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA0</name>
<description>DATA0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>RDH0R</name>
<displayName>RDH0R</displayName>
<description>receive FIFO mailbox data high           register</description>
<addressOffset>0x1BC</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DATA7</name>
<description>DATA7</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA6</name>
<description>DATA6</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA5</name>
<description>DATA5</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA4</name>
<description>DATA4</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>RI1R</name>
<displayName>RI1R</displayName>
<description>receive FIFO mailbox identifier           register</description>
<addressOffset>0x1C0</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>STID</name>
<description>STID</description>
<bitOffset>21</bitOffset>
<bitWidth>11</bitWidth>
</field>
<field>
<name>EXID</name>
<description>EXID</description>
<bitOffset>3</bitOffset>
<bitWidth>18</bitWidth>
</field>
<field>
<name>IDE</name>
<description>IDE</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RTR</name>
<description>RTR</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>RDT1R</name>
<displayName>RDT1R</displayName>
<description>receive FIFO mailbox data length control and           time stamp register</description>
<addressOffset>0x1C4</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>TIME</name>
<description>TIME</description>
<bitOffset>16</bitOffset>
<bitWidth>16</bitWidth>
</field>
<field>
<name>FMI</name>
<description>FMI</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DLC</name>
<description>DLC</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>RDL1R</name>
<displayName>RDL1R</displayName>
<description>receive FIFO mailbox data low           register</description>
<addressOffset>0x1C8</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DATA3</name>
<description>DATA3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA2</name>
<description>DATA2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA1</name>
<description>DATA1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA0</name>
<description>DATA0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>RDH1R</name>
<displayName>RDH1R</displayName>
<description>receive FIFO mailbox data high           register</description>
<addressOffset>0x1CC</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DATA7</name>
<description>DATA7</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA6</name>
<description>DATA6</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA5</name>
<description>DATA5</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DATA4</name>
<description>DATA4</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>FMR</name>
<displayName>FMR</displayName>
<description>filter master register</description>
<addressOffset>0x200</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x2A1C0E01</resetValue>
<fields>
<field>
<name>CAN2SB</name>
<description>CAN2 start bank</description>
<bitOffset>8</bitOffset>
<bitWidth>6</bitWidth>
</field>
<field>
<name>FINIT</name>
<description>Filter init mode</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>FM1R</name>
<displayName>FM1R</displayName>
<description>filter mode register</description>
<addressOffset>0x204</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FBM0</name>
<description>Filter mode</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM1</name>
<description>Filter mode</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM2</name>
<description>Filter mode</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM3</name>
<description>Filter mode</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM4</name>
<description>Filter mode</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM5</name>
<description>Filter mode</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM6</name>
<description>Filter mode</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM7</name>
<description>Filter mode</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM8</name>
<description>Filter mode</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM9</name>
<description>Filter mode</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM10</name>
<description>Filter mode</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM11</name>
<description>Filter mode</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM12</name>
<description>Filter mode</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM13</name>
<description>Filter mode</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM14</name>
<description>Filter mode</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM15</name>
<description>Filter mode</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM16</name>
<description>Filter mode</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM17</name>
<description>Filter mode</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM18</name>
<description>Filter mode</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM19</name>
<description>Filter mode</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM20</name>
<description>Filter mode</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM21</name>
<description>Filter mode</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM22</name>
<description>Filter mode</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM23</name>
<description>Filter mode</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM24</name>
<description>Filter mode</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM25</name>
<description>Filter mode</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM26</name>
<description>Filter mode</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FBM27</name>
<description>Filter mode</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>FS1R</name>
<displayName>FS1R</displayName>
<description>filter scale register</description>
<addressOffset>0x20C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FSC0</name>
<description>Filter scale configuration</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC1</name>
<description>Filter scale configuration</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC2</name>
<description>Filter scale configuration</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC3</name>
<description>Filter scale configuration</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC4</name>
<description>Filter scale configuration</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC5</name>
<description>Filter scale configuration</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC6</name>
<description>Filter scale configuration</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC7</name>
<description>Filter scale configuration</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC8</name>
<description>Filter scale configuration</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC9</name>
<description>Filter scale configuration</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC10</name>
<description>Filter scale configuration</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC11</name>
<description>Filter scale configuration</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC12</name>
<description>Filter scale configuration</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC13</name>
<description>Filter scale configuration</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC14</name>
<description>Filter scale configuration</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC15</name>
<description>Filter scale configuration</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC16</name>
<description>Filter scale configuration</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC17</name>
<description>Filter scale configuration</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC18</name>
<description>Filter scale configuration</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC19</name>
<description>Filter scale configuration</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC20</name>
<description>Filter scale configuration</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC21</name>
<description>Filter scale configuration</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC22</name>
<description>Filter scale configuration</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC23</name>
<description>Filter scale configuration</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC24</name>
<description>Filter scale configuration</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC25</name>
<description>Filter scale configuration</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC26</name>
<description>Filter scale configuration</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSC27</name>
<description>Filter scale configuration</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>FFA1R</name>
<displayName>FFA1R</displayName>
<description>filter FIFO assignment           register</description>
<addressOffset>0x214</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FFA0</name>
<description>Filter FIFO assignment for filter               0</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA1</name>
<description>Filter FIFO assignment for filter               1</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA2</name>
<description>Filter FIFO assignment for filter               2</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA3</name>
<description>Filter FIFO assignment for filter               3</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA4</name>
<description>Filter FIFO assignment for filter               4</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA5</name>
<description>Filter FIFO assignment for filter               5</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA6</name>
<description>Filter FIFO assignment for filter               6</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA7</name>
<description>Filter FIFO assignment for filter               7</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA8</name>
<description>Filter FIFO assignment for filter               8</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA9</name>
<description>Filter FIFO assignment for filter               9</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA10</name>
<description>Filter FIFO assignment for filter               10</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA11</name>
<description>Filter FIFO assignment for filter               11</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA12</name>
<description>Filter FIFO assignment for filter               12</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA13</name>
<description>Filter FIFO assignment for filter               13</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA14</name>
<description>Filter FIFO assignment for filter               14</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA15</name>
<description>Filter FIFO assignment for filter               15</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA16</name>
<description>Filter FIFO assignment for filter               16</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA17</name>
<description>Filter FIFO assignment for filter               17</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA18</name>
<description>Filter FIFO assignment for filter               18</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA19</name>
<description>Filter FIFO assignment for filter               19</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA20</name>
<description>Filter FIFO assignment for filter               20</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA21</name>
<description>Filter FIFO assignment for filter               21</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA22</name>
<description>Filter FIFO assignment for filter               22</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA23</name>
<description>Filter FIFO assignment for filter               23</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA24</name>
<description>Filter FIFO assignment for filter               24</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA25</name>
<description>Filter FIFO assignment for filter               25</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA26</name>
<description>Filter FIFO assignment for filter               26</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FFA27</name>
<description>Filter FIFO assignment for filter               27</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>FA1R</name>
<displayName>FA1R</displayName>
<description>CAN filter activation register</description>
<addressOffset>0x21C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FACT0</name>
<description>Filter active</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT1</name>
<description>Filter active</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT2</name>
<description>Filter active</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT3</name>
<description>Filter active</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT4</name>
<description>Filter active</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT5</name>
<description>Filter active</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT6</name>
<description>Filter active</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT7</name>
<description>Filter active</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT8</name>
<description>Filter active</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT9</name>
<description>Filter active</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT10</name>
<description>Filter active</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT11</name>
<description>Filter active</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT12</name>
<description>Filter active</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT13</name>
<description>Filter active</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT14</name>
<description>Filter active</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT15</name>
<description>Filter active</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT16</name>
<description>Filter active</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT17</name>
<description>Filter active</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT18</name>
<description>Filter active</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT19</name>
<description>Filter active</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT20</name>
<description>Filter active</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT21</name>
<description>Filter active</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT22</name>
<description>Filter active</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT23</name>
<description>Filter active</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT24</name>
<description>Filter active</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT25</name>
<description>Filter active</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT26</name>
<description>Filter active</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FACT27</name>
<description>Filter active</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F0R1</name>
<displayName>F0R1</displayName>
<description>Filter bank 0 register 1</description>
<addressOffset>0x240</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F0R2</name>
<displayName>F0R2</displayName>
<description>Filter bank 0 register 2</description>
<addressOffset>0x244</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F1R1</name>
<displayName>F1R1</displayName>
<description>Filter bank 1 register 1</description>
<addressOffset>0x248</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F1R2</name>
<displayName>F1R2</displayName>
<description>Filter bank 1 register 2</description>
<addressOffset>0x24C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F2R1</name>
<displayName>F2R1</displayName>
<description>Filter bank 2 register 1</description>
<addressOffset>0x250</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F2R2</name>
<displayName>F2R2</displayName>
<description>Filter bank 2 register 2</description>
<addressOffset>0x254</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F3R1</name>
<displayName>F3R1</displayName>
<description>Filter bank 3 register 1</description>
<addressOffset>0x258</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F3R2</name>
<displayName>F3R2</displayName>
<description>Filter bank 3 register 2</description>
<addressOffset>0x25C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F4R1</name>
<displayName>F4R1</displayName>
<description>Filter bank 4 register 1</description>
<addressOffset>0x260</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F4R2</name>
<displayName>F4R2</displayName>
<description>Filter bank 4 register 2</description>
<addressOffset>0x264</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F5R1</name>
<displayName>F5R1</displayName>
<description>Filter bank 5 register 1</description>
<addressOffset>0x268</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F5R2</name>
<displayName>F5R2</displayName>
<description>Filter bank 5 register 2</description>
<addressOffset>0x26C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F6R1</name>
<displayName>F6R1</displayName>
<description>Filter bank 6 register 1</description>
<addressOffset>0x270</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F6R2</name>
<displayName>F6R2</displayName>
<description>Filter bank 6 register 2</description>
<addressOffset>0x274</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F7R1</name>
<displayName>F7R1</displayName>
<description>Filter bank 7 register 1</description>
<addressOffset>0x278</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F7R2</name>
<displayName>F7R2</displayName>
<description>Filter bank 7 register 2</description>
<addressOffset>0x27C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F8R1</name>
<displayName>F8R1</displayName>
<description>Filter bank 8 register 1</description>
<addressOffset>0x280</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F8R2</name>
<displayName>F8R2</displayName>
<description>Filter bank 8 register 2</description>
<addressOffset>0x284</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F9R1</name>
<displayName>F9R1</displayName>
<description>Filter bank 9 register 1</description>
<addressOffset>0x288</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F9R2</name>
<displayName>F9R2</displayName>
<description>Filter bank 9 register 2</description>
<addressOffset>0x28C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F10R1</name>
<displayName>F10R1</displayName>
<description>Filter bank 10 register 1</description>
<addressOffset>0x290</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F10R2</name>
<displayName>F10R2</displayName>
<description>Filter bank 10 register 2</description>
<addressOffset>0x294</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F11R1</name>
<displayName>F11R1</displayName>
<description>Filter bank 11 register 1</description>
<addressOffset>0x298</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F11R2</name>
<displayName>F11R2</displayName>
<description>Filter bank 11 register 2</description>
<addressOffset>0x29C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F12R1</name>
<displayName>F12R1</displayName>
<description>Filter bank 4 register 1</description>
<addressOffset>0x2A0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F12R2</name>
<displayName>F12R2</displayName>
<description>Filter bank 12 register 2</description>
<addressOffset>0x2A4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F13R1</name>
<displayName>F13R1</displayName>
<description>Filter bank 13 register 1</description>
<addressOffset>0x2A8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F13R2</name>
<displayName>F13R2</displayName>
<description>Filter bank 13 register 2</description>
<addressOffset>0x2AC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F14R1</name>
<displayName>F14R1</displayName>
<description>Filter bank 14 register 1</description>
<addressOffset>0x2B0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F14R2</name>
<displayName>F14R2</displayName>
<description>Filter bank 14 register 2</description>
<addressOffset>0x2B4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F15R1</name>
<displayName>F15R1</displayName>
<description>Filter bank 15 register 1</description>
<addressOffset>0x2B8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F15R2</name>
<displayName>F15R2</displayName>
<description>Filter bank 15 register 2</description>
<addressOffset>0x2BC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F16R1</name>
<displayName>F16R1</displayName>
<description>Filter bank 16 register 1</description>
<addressOffset>0x2C0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F16R2</name>
<displayName>F16R2</displayName>
<description>Filter bank 16 register 2</description>
<addressOffset>0x2C4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F17R1</name>
<displayName>F17R1</displayName>
<description>Filter bank 17 register 1</description>
<addressOffset>0x2C8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F17R2</name>
<displayName>F17R2</displayName>
<description>Filter bank 17 register 2</description>
<addressOffset>0x2CC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F18R1</name>
<displayName>F18R1</displayName>
<description>Filter bank 18 register 1</description>
<addressOffset>0x2D0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F18R2</name>
<displayName>F18R2</displayName>
<description>Filter bank 18 register 2</description>
<addressOffset>0x2D4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F19R1</name>
<displayName>F19R1</displayName>
<description>Filter bank 19 register 1</description>
<addressOffset>0x2D8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F19R2</name>
<displayName>F19R2</displayName>
<description>Filter bank 19 register 2</description>
<addressOffset>0x2DC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F20R1</name>
<displayName>F20R1</displayName>
<description>Filter bank 20 register 1</description>
<addressOffset>0x2E0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F20R2</name>
<displayName>F20R2</displayName>
<description>Filter bank 20 register 2</description>
<addressOffset>0x2E4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F21R1</name>
<displayName>F21R1</displayName>
<description>Filter bank 21 register 1</description>
<addressOffset>0x2E8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F21R2</name>
<displayName>F21R2</displayName>
<description>Filter bank 21 register 2</description>
<addressOffset>0x2EC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F22R1</name>
<displayName>F22R1</displayName>
<description>Filter bank 22 register 1</description>
<addressOffset>0x2F0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F22R2</name>
<displayName>F22R2</displayName>
<description>Filter bank 22 register 2</description>
<addressOffset>0x2F4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F23R1</name>
<displayName>F23R1</displayName>
<description>Filter bank 23 register 1</description>
<addressOffset>0x2F8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F23R2</name>
<displayName>F23R2</displayName>
<description>Filter bank 23 register 2</description>
<addressOffset>0x2FC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F24R1</name>
<displayName>F24R1</displayName>
<description>Filter bank 24 register 1</description>
<addressOffset>0x300</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F24R2</name>
<displayName>F24R2</displayName>
<description>Filter bank 24 register 2</description>
<addressOffset>0x304</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F25R1</name>
<displayName>F25R1</displayName>
<description>Filter bank 25 register 1</description>
<addressOffset>0x308</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F25R2</name>
<displayName>F25R2</displayName>
<description>Filter bank 25 register 2</description>
<addressOffset>0x30C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F26R1</name>
<displayName>F26R1</displayName>
<description>Filter bank 26 register 1</description>
<addressOffset>0x310</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F26R2</name>
<displayName>F26R2</displayName>
<description>Filter bank 26 register 2</description>
<addressOffset>0x314</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F27R1</name>
<displayName>F27R1</displayName>
<description>Filter bank 27 register 1</description>
<addressOffset>0x318</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>F27R2</name>
<displayName>F27R2</displayName>
<description>Filter bank 27 register 2</description>
<addressOffset>0x31C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>FB0</name>
<description>Filter bits</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB1</name>
<description>Filter bits</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB2</name>
<description>Filter bits</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB3</name>
<description>Filter bits</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB4</name>
<description>Filter bits</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB5</name>
<description>Filter bits</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB6</name>
<description>Filter bits</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB7</name>
<description>Filter bits</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB8</name>
<description>Filter bits</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB9</name>
<description>Filter bits</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB10</name>
<description>Filter bits</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB11</name>
<description>Filter bits</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB12</name>
<description>Filter bits</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB13</name>
<description>Filter bits</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB14</name>
<description>Filter bits</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB15</name>
<description>Filter bits</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB16</name>
<description>Filter bits</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB17</name>
<description>Filter bits</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB18</name>
<description>Filter bits</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB19</name>
<description>Filter bits</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB20</name>
<description>Filter bits</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB21</name>
<description>Filter bits</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB22</name>
<description>Filter bits</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB23</name>
<description>Filter bits</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB24</name>
<description>Filter bits</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB25</name>
<description>Filter bits</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB26</name>
<description>Filter bits</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB27</name>
<description>Filter bits</description>
<bitOffset>27</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB28</name>
<description>Filter bits</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB29</name>
<description>Filter bits</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB30</name>
<description>Filter bits</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FB31</name>
<description>Filter bits</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral>
<name>USB_FS</name>
<description>Universal serial bus full-speed device       interface</description>
<groupName>USB_FS</groupName>
<baseAddress>0x40005C00</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<interrupt>
<name>USB_WKUP</name>
<description>USB wakeup from Suspend</description>
<value>42</value>
</interrupt>
<interrupt>
<name>USB_HP</name>
<description>USB High priority interrupt</description>
<value>74</value>
</interrupt>
<interrupt>
<name>USB_LP</name>
<description>USB Low priority interrupt</description>
<value>75</value>
</interrupt>
<registers>
<register>
<name>USB_EP0R</name>
<displayName>USB_EP0R</displayName>
<description>endpoint 0 register</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>EA</name>
<description>Endpoint address</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
<access>read-write</access>
</field>
<field>
<name>STAT_TX</name>
<description>Status bits, for transmission               transfers</description>
<bitOffset>4</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>DTOG_TX</name>
<description>Data Toggle, for transmission               transfers</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CTR_TX</name>
<description>Correct Transfer for               transmission</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>EP_KIND</name>
<description>Endpoint kind</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>EP_TYPE</name>
<description>Endpoint type</description>
<bitOffset>9</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>SETUP</name>
<description>Setup transaction               completed</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>STAT_RX</name>
<description>Status bits, for reception               transfers</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>DTOG_RX</name>
<description>Data Toggle, for reception               transfers</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CTR_RX</name>
<description>Correct transfer for               reception</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
<register>
<name>USB_EP1R</name>
<displayName>USB_EP1R</displayName>
<description>endpoint 1 register</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>EA</name>
<description>Endpoint address</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
<access>read-write</access>
</field>
<field>
<name>STAT_TX</name>
<description>Status bits, for transmission               transfers</description>
<bitOffset>4</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>DTOG_TX</name>
<description>Data Toggle, for transmission               transfers</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CTR_TX</name>
<description>Correct Transfer for               transmission</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>EP_KIND</name>
<description>Endpoint kind</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>EP_TYPE</name>
<description>Endpoint type</description>
<bitOffset>9</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>SETUP</name>
<description>Setup transaction               completed</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>STAT_RX</name>
<description>Status bits, for reception               transfers</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>DTOG_RX</name>
<description>Data Toggle, for reception               transfers</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CTR_RX</name>
<description>Correct transfer for               reception</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
<register>
<name>USB_EP2R</name>
<displayName>USB_EP2R</displayName>
<description>endpoint 2 register</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>EA</name>
<description>Endpoint address</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
<access>read-write</access>
</field>
<field>
<name>STAT_TX</name>
<description>Status bits, for transmission               transfers</description>
<bitOffset>4</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>DTOG_TX</name>
<description>Data Toggle, for transmission               transfers</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CTR_TX</name>
<description>Correct Transfer for               transmission</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>EP_KIND</name>
<description>Endpoint kind</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>EP_TYPE</name>
<description>Endpoint type</description>
<bitOffset>9</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>SETUP</name>
<description>Setup transaction               completed</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>STAT_RX</name>
<description>Status bits, for reception               transfers</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>DTOG_RX</name>
<description>Data Toggle, for reception               transfers</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CTR_RX</name>
<description>Correct transfer for               reception</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
<register>
<name>USB_EP3R</name>
<displayName>USB_EP3R</displayName>
<description>endpoint 3 register</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>EA</name>
<description>Endpoint address</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
<access>read-write</access>
</field>
<field>
<name>STAT_TX</name>
<description>Status bits, for transmission               transfers</description>
<bitOffset>4</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>DTOG_TX</name>
<description>Data Toggle, for transmission               transfers</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CTR_TX</name>
<description>Correct Transfer for               transmission</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>EP_KIND</name>
<description>Endpoint kind</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>EP_TYPE</name>
<description>Endpoint type</description>
<bitOffset>9</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>SETUP</name>
<description>Setup transaction               completed</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>STAT_RX</name>
<description>Status bits, for reception               transfers</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>DTOG_RX</name>
<description>Data Toggle, for reception               transfers</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CTR_RX</name>
<description>Correct transfer for               reception</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
<register>
<name>USB_EP4R</name>
<displayName>USB_EP4R</displayName>
<description>endpoint 4 register</description>
<addressOffset>0x10</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>EA</name>
<description>Endpoint address</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
<access>read-write</access>
</field>
<field>
<name>STAT_TX</name>
<description>Status bits, for transmission               transfers</description>
<bitOffset>4</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>DTOG_TX</name>
<description>Data Toggle, for transmission               transfers</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CTR_TX</name>
<description>Correct Transfer for               transmission</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>EP_KIND</name>
<description>Endpoint kind</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>EP_TYPE</name>
<description>Endpoint type</description>
<bitOffset>9</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>SETUP</name>
<description>Setup transaction               completed</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>STAT_RX</name>
<description>Status bits, for reception               transfers</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>DTOG_RX</name>
<description>Data Toggle, for reception               transfers</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CTR_RX</name>
<description>Correct transfer for               reception</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
<register>
<name>USB_EP5R</name>
<displayName>USB_EP5R</displayName>
<description>endpoint 5 register</description>
<addressOffset>0x14</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>EA</name>
<description>Endpoint address</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
<access>read-write</access>
</field>
<field>
<name>STAT_TX</name>
<description>Status bits, for transmission               transfers</description>
<bitOffset>4</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>DTOG_TX</name>
<description>Data Toggle, for transmission               transfers</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CTR_TX</name>
<description>Correct Transfer for               transmission</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>EP_KIND</name>
<description>Endpoint kind</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>EP_TYPE</name>
<description>Endpoint type</description>
<bitOffset>9</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>SETUP</name>
<description>Setup transaction               completed</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>STAT_RX</name>
<description>Status bits, for reception               transfers</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>DTOG_RX</name>
<description>Data Toggle, for reception               transfers</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CTR_RX</name>
<description>Correct transfer for               reception</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
<register>
<name>USB_EP6R</name>
<displayName>USB_EP6R</displayName>
<description>endpoint 6 register</description>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>EA</name>
<description>Endpoint address</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
<access>read-write</access>
</field>
<field>
<name>STAT_TX</name>
<description>Status bits, for transmission               transfers</description>
<bitOffset>4</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>DTOG_TX</name>
<description>Data Toggle, for transmission               transfers</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CTR_TX</name>
<description>Correct Transfer for               transmission</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>EP_KIND</name>
<description>Endpoint kind</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>EP_TYPE</name>
<description>Endpoint type</description>
<bitOffset>9</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>SETUP</name>
<description>Setup transaction               completed</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>STAT_RX</name>
<description>Status bits, for reception               transfers</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>DTOG_RX</name>
<description>Data Toggle, for reception               transfers</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CTR_RX</name>
<description>Correct transfer for               reception</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
<register>
<name>USB_EP7R</name>
<displayName>USB_EP7R</displayName>
<description>endpoint 7 register</description>
<addressOffset>0x1C</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>EA</name>
<description>Endpoint address</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
<access>read-write</access>
</field>
<field>
<name>STAT_TX</name>
<description>Status bits, for transmission               transfers</description>
<bitOffset>4</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>DTOG_TX</name>
<description>Data Toggle, for transmission               transfers</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CTR_TX</name>
<description>Correct Transfer for               transmission</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>EP_KIND</name>
<description>Endpoint kind</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>EP_TYPE</name>
<description>Endpoint type</description>
<bitOffset>9</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>SETUP</name>
<description>Setup transaction               completed</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>STAT_RX</name>
<description>Status bits, for reception               transfers</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>DTOG_RX</name>
<description>Data Toggle, for reception               transfers</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CTR_RX</name>
<description>Correct transfer for               reception</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
<register>
<name>USB_CNTR</name>
<displayName>USB_CNTR</displayName>
<description>control register</description>
<addressOffset>0x40</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000003</resetValue>
<fields>
<field>
<name>FRES</name>
<description>Force USB Reset</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PDWN</name>
<description>Power down</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LPMODE</name>
<description>Low-power mode</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FSUSP</name>
<description>Force suspend</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RESUME</name>
<description>Resume request</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ESOFM</name>
<description>Expected start of frame interrupt               mask</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SOFM</name>
<description>Start of frame interrupt               mask</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RESETM</name>
<description>USB reset interrupt mask</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SUSPM</name>
<description>Suspend mode interrupt               mask</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>WKUPM</name>
<description>Wakeup interrupt mask</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ERRM</name>
<description>Error interrupt mask</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PMAOVRM</name>
<description>Packet memory area over / underrun               interrupt mask</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CTRM</name>
<description>Correct transfer interrupt               mask</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>ISTR</name>
<displayName>ISTR</displayName>
<description>interrupt status register</description>
<addressOffset>0x44</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>EP_ID</name>
<description>Endpoint Identifier</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
<access>read-only</access>
</field>
<field>
<name>DIR</name>
<description>Direction of transaction</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>ESOF</name>
<description>Expected start frame</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>SOF</name>
<description>start of frame</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>RESET</name>
<description>reset request</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>SUSP</name>
<description>Suspend mode request</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>WKUP</name>
<description>Wakeup</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>ERR</name>
<description>Error</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>PMAOVR</name>
<description>Packet memory area over /               underrun</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CTR</name>
<description>Correct transfer</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
</fields>
</register>
<register>
<name>FNR</name>
<displayName>FNR</displayName>
<description>frame number register</description>
<addressOffset>0x48</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>FN</name>
<description>Frame number</description>
<bitOffset>0</bitOffset>
<bitWidth>11</bitWidth>
</field>
<field>
<name>LSOF</name>
<description>Lost SOF</description>
<bitOffset>11</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>LCK</name>
<description>Locked</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RXDM</name>
<description>Receive data - line status</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RXDP</name>
<description>Receive data + line status</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>DADDR</name>
<displayName>DADDR</displayName>
<description>device address</description>
<addressOffset>0x4C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>ADD</name>
<description>Device address</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ADD1</name>
<description>Device address</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ADD2</name>
<description>Device address</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ADD3</name>
<description>Device address</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ADD4</name>
<description>Device address</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ADD5</name>
<description>Device address</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ADD6</name>
<description>Device address</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>EF</name>
<description>Enable function</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>BTABLE</name>
<displayName>BTABLE</displayName>
<description>Buffer table address</description>
<addressOffset>0x50</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>BTABLE</name>
<description>Buffer table</description>
<bitOffset>3</bitOffset>
<bitWidth>13</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral>
<name>I2C1</name>
<description>Inter-integrated circuit</description>
<groupName>I2C</groupName>
<baseAddress>0x40005400</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<interrupt>
<name>I2C1_EV_EXTI23</name>
<description>I2C1 event interrupt and EXTI Line23
        interrupt</description>
<value>31</value>
</interrupt>
<interrupt>
<name>I2C1_ER</name>
<description>I2C1 error interrupt</description>
<value>32</value>
</interrupt>
<registers>
<register>
<name>CR1</name>
<displayName>CR1</displayName>
<description>Control register 1</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>PE</name>
<description>Peripheral enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TXIE</name>
<description>TX Interrupt enable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>RXIE</name>
<description>RX Interrupt enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>ADDRIE</name>
<description>Address match interrupt enable (slave               only)</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>NACKIE</name>
<description>Not acknowledge received interrupt               enable</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>STOPIE</name>
<description>STOP detection Interrupt               enable</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TCIE</name>
<description>Transfer Complete interrupt               enable</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>ERRIE</name>
<description>Error interrupts enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>DNF</name>
<description>Digital noise filter</description>
<bitOffset>8</bitOffset>
<bitWidth>4</bitWidth>
<access>read-write</access>
</field>
<field>
<name>ANFOFF</name>
<description>Analog noise filter OFF</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>SWRST</name>
<description>Software reset</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
<access>write-only</access>
</field>
<field>
<name>TXDMAEN</name>
<description>DMA transmission requests               enable</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>RXDMAEN</name>
<description>DMA reception requests               enable</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>SBC</name>
<description>Slave byte control</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>NOSTRETCH</name>
<description>Clock stretching disable</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>WUPEN</name>
<description>Wakeup from STOP enable</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>GCEN</name>
<description>General call enable</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>SMBHEN</name>
<description>SMBus Host address enable</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>SMBDEN</name>
<description>SMBus Device Default address               enable</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>ALERTEN</name>
<description>SMBUS alert enable</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>PECEN</name>
<description>PEC enable</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
<register>
<name>CR2</name>
<displayName>CR2</displayName>
<description>Control register 2</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>PECBYTE</name>
<description>Packet error checking byte</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>AUTOEND</name>
<description>Automatic end mode (master               mode)</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RELOAD</name>
<description>NBYTES reload mode</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>NBYTES</name>
<description>Number of bytes</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>NACK</name>
<description>NACK generation (slave               mode)</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>STOP</name>
<description>Stop generation (master               mode)</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>START</name>
<description>Start generation</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>HEAD10R</name>
<description>10-bit address header only read               direction (master receiver mode)</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ADD10</name>
<description>10-bit addressing mode (master               mode)</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RD_WRN</name>
<description>Transfer direction (master               mode)</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SADD8</name>
<description>Slave address bit 9:8 (master               mode)</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>SADD1</name>
<description>Slave address bit 7:1 (master               mode)</description>
<bitOffset>1</bitOffset>
<bitWidth>7</bitWidth>
</field>
<field>
<name>SADD0</name>
<description>Slave address bit 0 (master               mode)</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>OAR1</name>
<displayName>OAR1</displayName>
<description>Own address register 1</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>OA1_0</name>
<description>Interface address</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OA1_1</name>
<description>Interface address</description>
<bitOffset>1</bitOffset>
<bitWidth>7</bitWidth>
</field>
<field>
<name>OA1_8</name>
<description>Interface address</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OA1MODE</name>
<description>Own Address 1 10-bit mode</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OA1EN</name>
<description>Own Address 1 enable</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>OAR2</name>
<displayName>OAR2</displayName>
<description>Own address register 2</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>OA2</name>
<description>Interface address</description>
<bitOffset>1</bitOffset>
<bitWidth>7</bitWidth>
</field>
<field>
<name>OA2MSK</name>
<description>Own Address 2 masks</description>
<bitOffset>8</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>OA2EN</name>
<description>Own Address 2 enable</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>TIMINGR</name>
<displayName>TIMINGR</displayName>
<description>Timing register</description>
<addressOffset>0x10</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>SCLL</name>
<description>SCL low period (master               mode)</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>SCLH</name>
<description>SCL high period (master               mode)</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>SDADEL</name>
<description>Data hold time</description>
<bitOffset>16</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>SCLDEL</name>
<description>Data setup time</description>
<bitOffset>20</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>PRESC</name>
<description>Timing prescaler</description>
<bitOffset>28</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>TIMEOUTR</name>
<displayName>TIMEOUTR</displayName>
<description>Status register 1</description>
<addressOffset>0x14</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>TIMEOUTA</name>
<description>Bus timeout A</description>
<bitOffset>0</bitOffset>
<bitWidth>12</bitWidth>
</field>
<field>
<name>TIDLE</name>
<description>Idle clock timeout               detection</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIMOUTEN</name>
<description>Clock timeout enable</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIMEOUTB</name>
<description>Bus timeout B</description>
<bitOffset>16</bitOffset>
<bitWidth>12</bitWidth>
</field>
<field>
<name>TEXTEN</name>
<description>Extended clock timeout               enable</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>ISR</name>
<displayName>ISR</displayName>
<description>Interrupt and Status register</description>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<resetValue>0x00000001</resetValue>
<fields>
<field>
<name>ADDCODE</name>
<description>Address match code (Slave               mode)</description>
<bitOffset>17</bitOffset>
<bitWidth>7</bitWidth>
<access>read-only</access>
</field>
<field>
<name>DIR</name>
<description>Transfer direction (Slave               mode)</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>BUSY</name>
<description>Bus busy</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>ALERT</name>
<description>SMBus alert</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>TIMEOUT</name>
<description>Timeout or t_low detection               flag</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>PECERR</name>
<description>PEC Error in reception</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>OVR</name>
<description>Overrun/Underrun (slave               mode)</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>ARLO</name>
<description>Arbitration lost</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>BERR</name>
<description>Bus error</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>TCR</name>
<description>Transfer Complete Reload</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>TC</name>
<description>Transfer Complete (master               mode)</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>STOPF</name>
<description>Stop detection flag</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>NACKF</name>
<description>Not acknowledge received               flag</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>ADDR</name>
<description>Address matched (slave               mode)</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>RXNE</name>
<description>Receive data register not empty               (receivers)</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>TXIS</name>
<description>Transmit interrupt status               (transmitters)</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TXE</name>
<description>Transmit data register empty               (transmitters)</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
<register>
<name>ICR</name>
<displayName>ICR</displayName>
<description>Interrupt clear register</description>
<addressOffset>0x1C</addressOffset>
<size>0x20</size>
<access>write-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>ALERTCF</name>
<description>Alert flag clear</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIMOUTCF</name>
<description>Timeout detection flag               clear</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PECCF</name>
<description>PEC Error flag clear</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OVRCF</name>
<description>Overrun/Underrun flag               clear</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ARLOCF</name>
<description>Arbitration lost flag               clear</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BERRCF</name>
<description>Bus error flag clear</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>STOPCF</name>
<description>Stop detection flag clear</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>NACKCF</name>
<description>Not Acknowledge flag clear</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ADDRCF</name>
<description>Address Matched flag clear</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>PECR</name>
<displayName>PECR</displayName>
<description>PEC register</description>
<addressOffset>0x20</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>PEC</name>
<description>Packet error checking               register</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>RXDR</name>
<displayName>RXDR</displayName>
<description>Receive data register</description>
<addressOffset>0x24</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>RXDATA</name>
<description>8-bit receive data</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>TXDR</name>
<displayName>TXDR</displayName>
<description>Transmit data register</description>
<addressOffset>0x28</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>TXDATA</name>
<description>8-bit transmit data</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral derivedFrom="I2C1">
<name>I2C2</name>
<baseAddress>0x40005800</baseAddress>
<interrupt>
<name>I2C2_EV_EXTI24</name>
<description>I2C2 event interrupt &amp; EXTI Line24
        interrupt</description>
<value>33</value>
</interrupt>
<interrupt>
<name>I2C2_ER</name>
<description>I2C2 error interrupt</description>
<value>34</value>
</interrupt>
</peripheral>
<peripheral derivedFrom="I2C1">
<name>I2C3</name>
<baseAddress>0x40007800</baseAddress>
<interrupt>
<name>I2C2_EV_EXTI24</name>
<description>I2C2 event interrupt &amp; EXTI Line24
        interrupt</description>
<value>33</value>
</interrupt>
<interrupt>
<name>I2C2_ER</name>
<description>I2C2 error interrupt</description>
<value>34</value>
</interrupt>
</peripheral>
<peripheral>
<name>IWDG</name>
<description>Independent watchdog</description>
<groupName>IWDG</groupName>
<baseAddress>0x40003000</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<registers>
<register>
<name>KR</name>
<displayName>KR</displayName>
<description>Key register</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>write-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>KEY</name>
<description>Key value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>PR</name>
<displayName>PR</displayName>
<description>Prescaler register</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>PR</name>
<description>Prescaler divider</description>
<bitOffset>0</bitOffset>
<bitWidth>3</bitWidth>
</field>
</fields>
</register>
<register>
<name>RLR</name>
<displayName>RLR</displayName>
<description>Reload register</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000FFF</resetValue>
<fields>
<field>
<name>RL</name>
<description>Watchdog counter reload               value</description>
<bitOffset>0</bitOffset>
<bitWidth>12</bitWidth>
</field>
</fields>
</register>
<register>
<name>SR</name>
<displayName>SR</displayName>
<description>Status register</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>PVU</name>
<description>Watchdog prescaler value               update</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RVU</name>
<description>Watchdog counter reload value               update</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>WVU</name>
<description>Watchdog counter window value               update</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>WINR</name>
<displayName>WINR</displayName>
<description>Window register</description>
<addressOffset>0x10</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000FFF</resetValue>
<fields>
<field>
<name>WIN</name>
<description>Watchdog counter window               value</description>
<bitOffset>0</bitOffset>
<bitWidth>12</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral>
<name>WWDG</name>
<description>Window watchdog</description>
<groupName>WWDG</groupName>
<baseAddress>0x40002C00</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<interrupt>
<name>WWDG</name>
<description>Window Watchdog interrupt</description>
<value>0</value>
</interrupt>
<registers>
<register>
<name>CR</name>
<displayName>CR</displayName>
<description>Control register</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000007F</resetValue>
<fields>
<field>
<name>T</name>
<description>7-bit counter</description>
<bitOffset>0</bitOffset>
<bitWidth>7</bitWidth>
</field>
<field>
<name>WDGA</name>
<description>Activation bit</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CFR</name>
<displayName>CFR</displayName>
<description>Configuration register</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000007F</resetValue>
<fields>
<field>
<name>EWI</name>
<description>Early wakeup interrupt</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>WDGTB</name>
<description>Timer base</description>
<bitOffset>7</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>W</name>
<description>7-bit window value</description>
<bitOffset>0</bitOffset>
<bitWidth>7</bitWidth>
</field>
</fields>
</register>
<register>
<name>SR</name>
<displayName>SR</displayName>
<description>Status register</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>EWIF</name>
<description>Early wakeup interrupt               flag</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral>
<name>RTC</name>
<description>Real-time clock</description>
<groupName>RTC</groupName>
<baseAddress>0x40002800</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<interrupt>
<name>RTC_WKUP</name>
<description>RTC Wakeup interrupt through the EXTI
        line</description>
<value>3</value>
</interrupt>
<interrupt>
<name>RTCAlarm</name>
<description>RTC alarm interrupt</description>
<value>41</value>
</interrupt>
<registers>
<register>
<name>TR</name>
<displayName>TR</displayName>
<description>time register</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>PM</name>
<description>AM/PM notation</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>HT</name>
<description>Hour tens in BCD format</description>
<bitOffset>20</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>HU</name>
<description>Hour units in BCD format</description>
<bitOffset>16</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>MNT</name>
<description>Minute tens in BCD format</description>
<bitOffset>12</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>MNU</name>
<description>Minute units in BCD format</description>
<bitOffset>8</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>ST</name>
<description>Second tens in BCD format</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>SU</name>
<description>Second units in BCD format</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>DR</name>
<displayName>DR</displayName>
<description>date register</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00002101</resetValue>
<fields>
<field>
<name>YT</name>
<description>Year tens in BCD format</description>
<bitOffset>20</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>YU</name>
<description>Year units in BCD format</description>
<bitOffset>16</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>WDU</name>
<description>Week day units</description>
<bitOffset>13</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>MT</name>
<description>Month tens in BCD format</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MU</name>
<description>Month units in BCD format</description>
<bitOffset>8</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>DT</name>
<description>Date tens in BCD format</description>
<bitOffset>4</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>DU</name>
<description>Date units in BCD format</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>CR</name>
<displayName>CR</displayName>
<description>control register</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>WCKSEL</name>
<description>Wakeup clock selection</description>
<bitOffset>0</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>TSEDGE</name>
<description>Time-stamp event active               edge</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>REFCKON</name>
<description>Reference clock detection enable (50 or               60 Hz)</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BYPSHAD</name>
<description>Bypass the shadow               registers</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>FMT</name>
<description>Hour format</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ALRAE</name>
<description>Alarm A enable</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ALRBE</name>
<description>Alarm B enable</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>WUTE</name>
<description>Wakeup timer enable</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TSE</name>
<description>Time stamp enable</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ALRAIE</name>
<description>Alarm A interrupt enable</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ALRBIE</name>
<description>Alarm B interrupt enable</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>WUTIE</name>
<description>Wakeup timer interrupt               enable</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TSIE</name>
<description>Time-stamp interrupt               enable</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ADD1H</name>
<description>Add 1 hour (summer time               change)</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SUB1H</name>
<description>Subtract 1 hour (winter time               change)</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BKP</name>
<description>Backup</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>COSEL</name>
<description>Calibration output               selection</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>POL</name>
<description>Output polarity</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OSEL</name>
<description>Output selection</description>
<bitOffset>21</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>COE</name>
<description>Calibration output enable</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>ISR</name>
<displayName>ISR</displayName>
<description>initialization and status           register</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<resetValue>0x00000007</resetValue>
<fields>
<field>
<name>ALRAWF</name>
<description>Alarm A write flag</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>ALRBWF</name>
<description>Alarm B write flag</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>WUTWF</name>
<description>Wakeup timer write flag</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>SHPF</name>
<description>Shift operation pending</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>INITS</name>
<description>Initialization status flag</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>RSF</name>
<description>Registers synchronization               flag</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>INITF</name>
<description>Initialization flag</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>INIT</name>
<description>Initialization mode</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>ALRAF</name>
<description>Alarm A flag</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>ALRBF</name>
<description>Alarm B flag</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>WUTF</name>
<description>Wakeup timer flag</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TSF</name>
<description>Time-stamp flag</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TSOVF</name>
<description>Time-stamp overflow flag</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TAMP1F</name>
<description>Tamper detection flag</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TAMP2F</name>
<description>RTC_TAMP2 detection flag</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TAMP3F</name>
<description>RTC_TAMP3 detection flag</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>RECALPF</name>
<description>Recalibration pending Flag</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
</fields>
</register>
<register>
<name>PRER</name>
<displayName>PRER</displayName>
<description>prescaler register</description>
<addressOffset>0x10</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x007F00FF</resetValue>
<fields>
<field>
<name>PREDIV_A</name>
<description>Asynchronous prescaler               factor</description>
<bitOffset>16</bitOffset>
<bitWidth>7</bitWidth>
</field>
<field>
<name>PREDIV_S</name>
<description>Synchronous prescaler               factor</description>
<bitOffset>0</bitOffset>
<bitWidth>15</bitWidth>
</field>
</fields>
</register>
<register>
<name>WUTR</name>
<displayName>WUTR</displayName>
<description>wakeup timer register</description>
<addressOffset>0x14</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000FFFF</resetValue>
<fields>
<field>
<name>WUT</name>
<description>Wakeup auto-reload value               bits</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>ALRMAR</name>
<displayName>ALRMAR</displayName>
<description>alarm A register</description>
<addressOffset>0x1C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>MSK4</name>
<description>Alarm A date mask</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>WDSEL</name>
<description>Week day selection</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DT</name>
<description>Date tens in BCD format</description>
<bitOffset>28</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>DU</name>
<description>Date units or day in BCD               format</description>
<bitOffset>24</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>MSK3</name>
<description>Alarm A hours mask</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PM</name>
<description>AM/PM notation</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>HT</name>
<description>Hour tens in BCD format</description>
<bitOffset>20</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>HU</name>
<description>Hour units in BCD format</description>
<bitOffset>16</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>MSK2</name>
<description>Alarm A minutes mask</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MNT</name>
<description>Minute tens in BCD format</description>
<bitOffset>12</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>MNU</name>
<description>Minute units in BCD format</description>
<bitOffset>8</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>MSK1</name>
<description>Alarm A seconds mask</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ST</name>
<description>Second tens in BCD format</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>SU</name>
<description>Second units in BCD format</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>ALRMBR</name>
<displayName>ALRMBR</displayName>
<description>alarm B register</description>
<addressOffset>0x20</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>MSK4</name>
<description>Alarm B date mask</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>WDSEL</name>
<description>Week day selection</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DT</name>
<description>Date tens in BCD format</description>
<bitOffset>28</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>DU</name>
<description>Date units or day in BCD               format</description>
<bitOffset>24</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>MSK3</name>
<description>Alarm B hours mask</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PM</name>
<description>AM/PM notation</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>HT</name>
<description>Hour tens in BCD format</description>
<bitOffset>20</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>HU</name>
<description>Hour units in BCD format</description>
<bitOffset>16</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>MSK2</name>
<description>Alarm B minutes mask</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MNT</name>
<description>Minute tens in BCD format</description>
<bitOffset>12</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>MNU</name>
<description>Minute units in BCD format</description>
<bitOffset>8</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>MSK1</name>
<description>Alarm B seconds mask</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ST</name>
<description>Second tens in BCD format</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>SU</name>
<description>Second units in BCD format</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>WPR</name>
<displayName>WPR</displayName>
<description>write protection register</description>
<addressOffset>0x24</addressOffset>
<size>0x20</size>
<access>write-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>KEY</name>
<description>Write protection key</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>SSR</name>
<displayName>SSR</displayName>
<description>sub second register</description>
<addressOffset>0x28</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>SS</name>
<description>Sub second value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>SHIFTR</name>
<displayName>SHIFTR</displayName>
<description>shift control register</description>
<addressOffset>0x2C</addressOffset>
<size>0x20</size>
<access>write-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>ADD1S</name>
<description>Add one second</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SUBFS</name>
<description>Subtract a fraction of a               second</description>
<bitOffset>0</bitOffset>
<bitWidth>15</bitWidth>
</field>
</fields>
</register>
<register>
<name>TSTR</name>
<displayName>TSTR</displayName>
<description>time stamp time register</description>
<addressOffset>0x30</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>SU</name>
<description>Second units in BCD format</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>ST</name>
<description>Second tens in BCD format</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>MNU</name>
<description>Minute units in BCD format</description>
<bitOffset>8</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>MNT</name>
<description>Minute tens in BCD format</description>
<bitOffset>12</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>HU</name>
<description>Hour units in BCD format</description>
<bitOffset>16</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>HT</name>
<description>Hour tens in BCD format</description>
<bitOffset>20</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>PM</name>
<description>AM/PM notation</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>TSDR</name>
<displayName>TSDR</displayName>
<description>time stamp date register</description>
<addressOffset>0x34</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>WDU</name>
<description>Week day units</description>
<bitOffset>13</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>MT</name>
<description>Month tens in BCD format</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MU</name>
<description>Month units in BCD format</description>
<bitOffset>8</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>DT</name>
<description>Date tens in BCD format</description>
<bitOffset>4</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>DU</name>
<description>Date units in BCD format</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>TSSSR</name>
<displayName>TSSSR</displayName>
<description>timestamp sub second register</description>
<addressOffset>0x38</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>SS</name>
<description>Sub second value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>CALR</name>
<displayName>CALR</displayName>
<description>calibration register</description>
<addressOffset>0x3C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CALP</name>
<description>Increase frequency of RTC by 488.5               ppm</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CALW8</name>
<description>Use an 8-second calibration cycle               period</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CALW16</name>
<description>Use a 16-second calibration cycle               period</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CALM</name>
<description>Calibration minus</description>
<bitOffset>0</bitOffset>
<bitWidth>9</bitWidth>
</field>
</fields>
</register>
<register>
<name>TAFCR</name>
<displayName>TAFCR</displayName>
<description>tamper and alternate function configuration           register</description>
<addressOffset>0x40</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>TAMP1E</name>
<description>Tamper 1 detection enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TAMP1TRG</name>
<description>Active level for tamper 1</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TAMPIE</name>
<description>Tamper interrupt enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TAMP2E</name>
<description>Tamper 2 detection enable</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TAMP2TRG</name>
<description>Active level for tamper 2</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TAMP3E</name>
<description>Tamper 3 detection enable</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TAMP3TRG</name>
<description>Active level for tamper 3</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TAMPTS</name>
<description>Activate timestamp on tamper detection               event</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TAMPFREQ</name>
<description>Tamper sampling frequency</description>
<bitOffset>8</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>TAMPFLT</name>
<description>Tamper filter count</description>
<bitOffset>11</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>TAMPPRCH</name>
<description>Tamper precharge duration</description>
<bitOffset>13</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>TAMPPUDIS</name>
<description>TAMPER pull-up disable</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PC13VALUE</name>
<description>PC13 value</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PC13MODE</name>
<description>PC13 mode</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PC14VALUE</name>
<description>PC14 value</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PC14MODE</name>
<description>PC 14 mode</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PC15VALUE</name>
<description>PC15 value</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PC15MODE</name>
<description>PC15 mode</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>ALRMASSR</name>
<displayName>ALRMASSR</displayName>
<description>alarm A sub second register</description>
<addressOffset>0x44</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>MASKSS</name>
<description>Mask the most-significant bits starting               at this bit</description>
<bitOffset>24</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>SS</name>
<description>Sub seconds value</description>
<bitOffset>0</bitOffset>
<bitWidth>15</bitWidth>
</field>
</fields>
</register>
<register>
<name>ALRMBSSR</name>
<displayName>ALRMBSSR</displayName>
<description>alarm B sub second register</description>
<addressOffset>0x48</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>MASKSS</name>
<description>Mask the most-significant bits starting               at this bit</description>
<bitOffset>24</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>SS</name>
<description>Sub seconds value</description>
<bitOffset>0</bitOffset>
<bitWidth>15</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP0R</name>
<displayName>BKP0R</displayName>
<description>backup register</description>
<addressOffset>0x50</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP1R</name>
<displayName>BKP1R</displayName>
<description>backup register</description>
<addressOffset>0x54</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP2R</name>
<displayName>BKP2R</displayName>
<description>backup register</description>
<addressOffset>0x58</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP3R</name>
<displayName>BKP3R</displayName>
<description>backup register</description>
<addressOffset>0x5C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP4R</name>
<displayName>BKP4R</displayName>
<description>backup register</description>
<addressOffset>0x60</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP5R</name>
<displayName>BKP5R</displayName>
<description>backup register</description>
<addressOffset>0x64</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP6R</name>
<displayName>BKP6R</displayName>
<description>backup register</description>
<addressOffset>0x68</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP7R</name>
<displayName>BKP7R</displayName>
<description>backup register</description>
<addressOffset>0x6C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP8R</name>
<displayName>BKP8R</displayName>
<description>backup register</description>
<addressOffset>0x70</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP9R</name>
<displayName>BKP9R</displayName>
<description>backup register</description>
<addressOffset>0x74</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP10R</name>
<displayName>BKP10R</displayName>
<description>backup register</description>
<addressOffset>0x78</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP11R</name>
<displayName>BKP11R</displayName>
<description>backup register</description>
<addressOffset>0x7C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP12R</name>
<displayName>BKP12R</displayName>
<description>backup register</description>
<addressOffset>0x80</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP13R</name>
<displayName>BKP13R</displayName>
<description>backup register</description>
<addressOffset>0x84</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP14R</name>
<displayName>BKP14R</displayName>
<description>backup register</description>
<addressOffset>0x88</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP15R</name>
<displayName>BKP15R</displayName>
<description>backup register</description>
<addressOffset>0x8C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP16R</name>
<displayName>BKP16R</displayName>
<description>backup register</description>
<addressOffset>0x90</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP17R</name>
<displayName>BKP17R</displayName>
<description>backup register</description>
<addressOffset>0x94</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP18R</name>
<displayName>BKP18R</displayName>
<description>backup register</description>
<addressOffset>0x98</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP19R</name>
<displayName>BKP19R</displayName>
<description>backup register</description>
<addressOffset>0x9C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP20R</name>
<displayName>BKP20R</displayName>
<description>backup register</description>
<addressOffset>0xA0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP21R</name>
<displayName>BKP21R</displayName>
<description>backup register</description>
<addressOffset>0xA4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP22R</name>
<displayName>BKP22R</displayName>
<description>backup register</description>
<addressOffset>0xA8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP23R</name>
<displayName>BKP23R</displayName>
<description>backup register</description>
<addressOffset>0xAC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP24R</name>
<displayName>BKP24R</displayName>
<description>backup register</description>
<addressOffset>0xB0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP25R</name>
<displayName>BKP25R</displayName>
<description>backup register</description>
<addressOffset>0xB4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP26R</name>
<displayName>BKP26R</displayName>
<description>backup register</description>
<addressOffset>0xB8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP27R</name>
<displayName>BKP27R</displayName>
<description>backup register</description>
<addressOffset>0xBC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP28R</name>
<displayName>BKP28R</displayName>
<description>backup register</description>
<addressOffset>0xC0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP29R</name>
<displayName>BKP29R</displayName>
<description>backup register</description>
<addressOffset>0xC4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP30R</name>
<displayName>BKP30R</displayName>
<description>backup register</description>
<addressOffset>0xC8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>BKP31R</name>
<displayName>BKP31R</displayName>
<description>backup register</description>
<addressOffset>0xCC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>BKP</name>
<description>BKP</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral>
<name>TIM6</name>
<description>Basic timers</description>
<groupName>TIMs</groupName>
<baseAddress>0x40001000</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<interrupt>
<name>TIM6_DACUNDER</name>
<description>TIM6 global and DAC12 underrun
        interrupts</description>
<value>54</value>
</interrupt>
<registers>
<register>
<name>CR1</name>
<displayName>CR1</displayName>
<description>control register 1</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>CEN</name>
<description>Counter enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UDIS</name>
<description>Update disable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>URS</name>
<description>Update request source</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OPM</name>
<description>One-pulse mode</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ARPE</name>
<description>Auto-reload preload enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UIFREMAP</name>
<description>UIF status bit remapping</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CR2</name>
<displayName>CR2</displayName>
<description>control register 2</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>MMS</name>
<description>Master mode selection</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
</field>
</fields>
</register>
<register>
<name>DIER</name>
<displayName>DIER</displayName>
<description>DMA/Interrupt enable register</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>UDE</name>
<description>Update DMA request enable</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UIE</name>
<description>Update interrupt enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>SR</name>
<displayName>SR</displayName>
<description>status register</description>
<addressOffset>0x10</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>UIF</name>
<description>Update interrupt flag</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>EGR</name>
<displayName>EGR</displayName>
<description>event generation register</description>
<addressOffset>0x14</addressOffset>
<size>0x20</size>
<access>write-only</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>UG</name>
<description>Update generation</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CNT</name>
<displayName>CNT</displayName>
<description>counter</description>
<addressOffset>0x24</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CNT</name>
<description>Low counter value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
<access>read-write</access>
</field>
<field>
<name>UIFCPY</name>
<description>UIF Copy</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
</fields>
</register>
<register>
<name>PSC</name>
<displayName>PSC</displayName>
<description>prescaler</description>
<addressOffset>0x28</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>PSC</name>
<description>Prescaler value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>ARR</name>
<displayName>ARR</displayName>
<description>auto-reload register</description>
<addressOffset>0x2C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>ARR</name>
<description>Low Auto-reload value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral derivedFrom="TIM6">
<name>TIM7</name>
<baseAddress>0x40001400</baseAddress>
<interrupt>
<name>TIM7</name>
<description>TIM7 global interrupt</description>
<value>55</value>
</interrupt>
</peripheral>
<peripheral>
<name>DAC</name>
<description>Digital-to-analog converter</description>
<groupName>DAC</groupName>
<baseAddress>0x40007400</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<interrupt>
<name>TIM6_DACUNDER</name>
<description>TIM6 global and DAC12 underrun
        interrupts</description>
<value>54</value>
</interrupt>
<registers>
<register>
<name>CR</name>
<displayName>CR</displayName>
<description>control register</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DMAUDRIE2</name>
<description>DAC channel2 DMA underrun interrupt               enable</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DMAEN2</name>
<description>DAC channel2 DMA enable</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MAMP2</name>
<description>DAC channel2 mask/amplitude               selector</description>
<bitOffset>24</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>WAVE2</name>
<description>DAC channel2 noise/triangle wave               generation enable</description>
<bitOffset>22</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>TSEL2</name>
<description>DAC channel2 trigger               selection</description>
<bitOffset>19</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>TEN2</name>
<description>DAC channel2 trigger               enable</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BOFF2</name>
<description>DAC channel2 output buffer               disable</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>EN2</name>
<description>DAC channel2 enable</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DMAUDRIE1</name>
<description>DAC channel1 DMA Underrun Interrupt               enable</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DMAEN1</name>
<description>DAC channel1 DMA enable</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MAMP1</name>
<description>DAC channel1 mask/amplitude               selector</description>
<bitOffset>8</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>WAVE1</name>
<description>DAC channel1 noise/triangle wave               generation enable</description>
<bitOffset>6</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>TSEL1</name>
<description>DAC channel1 trigger               selection</description>
<bitOffset>3</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>TEN1</name>
<description>DAC channel1 trigger               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BOFF1</name>
<description>DAC channel1 output buffer               disable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>EN1</name>
<description>DAC channel1 enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>SWTRIGR</name>
<displayName>SWTRIGR</displayName>
<description>software trigger register</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>write-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>SWTRIG2</name>
<description>DAC channel2 software               trigger</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SWTRIG1</name>
<description>DAC channel1 software               trigger</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>DHR12R1</name>
<displayName>DHR12R1</displayName>
<description>channel1 12-bit right-aligned data holding           register</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DACC1DHR</name>
<description>DAC channel1 12-bit right-aligned               data</description>
<bitOffset>0</bitOffset>
<bitWidth>12</bitWidth>
</field>
</fields>
</register>
<register>
<name>DHR12L1</name>
<displayName>DHR12L1</displayName>
<description>channel1 12-bit left aligned data holding           register</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DACC1DHR</name>
<description>DAC channel1 12-bit left-aligned               data</description>
<bitOffset>4</bitOffset>
<bitWidth>12</bitWidth>
</field>
</fields>
</register>
<register>
<name>DHR8R1</name>
<displayName>DHR8R1</displayName>
<description>channel1 8-bit right aligned data holding           register</description>
<addressOffset>0x10</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DACC1DHR</name>
<description>DAC channel1 8-bit right-aligned               data</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>DHR12R2</name>
<displayName>DHR12R2</displayName>
<description>channel2 12-bit right aligned data holding           register</description>
<addressOffset>0x14</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DACC2DHR</name>
<description>DAC channel2 12-bit right-aligned               data</description>
<bitOffset>0</bitOffset>
<bitWidth>12</bitWidth>
</field>
</fields>
</register>
<register>
<name>DHR12L2</name>
<displayName>DHR12L2</displayName>
<description>channel2 12-bit left aligned data holding           register</description>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DACC2DHR</name>
<description>DAC channel2 12-bit left-aligned               data</description>
<bitOffset>4</bitOffset>
<bitWidth>12</bitWidth>
</field>
</fields>
</register>
<register>
<name>DHR8R2</name>
<displayName>DHR8R2</displayName>
<description>channel2 8-bit right-aligned data holding           register</description>
<addressOffset>0x1C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DACC2DHR</name>
<description>DAC channel2 8-bit right-aligned               data</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>DHR12RD</name>
<displayName>DHR12RD</displayName>
<description>Dual DAC 12-bit right-aligned data holding           register</description>
<addressOffset>0x20</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DACC2DHR</name>
<description>DAC channel2 12-bit right-aligned               data</description>
<bitOffset>16</bitOffset>
<bitWidth>12</bitWidth>
</field>
<field>
<name>DACC1DHR</name>
<description>DAC channel1 12-bit right-aligned               data</description>
<bitOffset>0</bitOffset>
<bitWidth>12</bitWidth>
</field>
</fields>
</register>
<register>
<name>DHR12LD</name>
<displayName>DHR12LD</displayName>
<description>DUAL DAC 12-bit left aligned data holding           register</description>
<addressOffset>0x24</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DACC2DHR</name>
<description>DAC channel2 12-bit left-aligned               data</description>
<bitOffset>20</bitOffset>
<bitWidth>12</bitWidth>
</field>
<field>
<name>DACC1DHR</name>
<description>DAC channel1 12-bit left-aligned               data</description>
<bitOffset>4</bitOffset>
<bitWidth>12</bitWidth>
</field>
</fields>
</register>
<register>
<name>DHR8RD</name>
<displayName>DHR8RD</displayName>
<description>DUAL DAC 8-bit right aligned data holding           register</description>
<addressOffset>0x28</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DACC2DHR</name>
<description>DAC channel2 8-bit right-aligned               data</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>DACC1DHR</name>
<description>DAC channel1 8-bit right-aligned               data</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>DOR1</name>
<displayName>DOR1</displayName>
<description>channel1 data output register</description>
<addressOffset>0x2C</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DACC1DOR</name>
<description>DAC channel1 data output</description>
<bitOffset>0</bitOffset>
<bitWidth>12</bitWidth>
</field>
</fields>
</register>
<register>
<name>DOR2</name>
<displayName>DOR2</displayName>
<description>channel2 data output register</description>
<addressOffset>0x30</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DACC2DOR</name>
<description>DAC channel2 data output</description>
<bitOffset>0</bitOffset>
<bitWidth>12</bitWidth>
</field>
</fields>
</register>
<register>
<name>SR</name>
<displayName>SR</displayName>
<description>status register</description>
<addressOffset>0x34</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DMAUDR2</name>
<description>DAC channel2 DMA underrun               flag</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DMAUDR1</name>
<description>DAC channel1 DMA underrun               flag</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral>
<name>NVIC</name>
<description>Nested Vectored Interrupt       Controller</description>
<groupName>NVIC</groupName>
<baseAddress>0xE000E000</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x1001</size>
<usage>registers</usage>
</addressBlock>
<registers>
<register>
<name>ICTR</name>
<displayName>ICTR</displayName>
<description>Interrupt Controller Type           Register</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>INTLINESNUM</name>
<description>Total number of interrupt lines in               groups</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>STIR</name>
<displayName>STIR</displayName>
<description>Software Triggered Interrupt           Register</description>
<addressOffset>0xF00</addressOffset>
<size>0x20</size>
<access>write-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>INTID</name>
<description>interrupt to be triggered</description>
<bitOffset>0</bitOffset>
<bitWidth>9</bitWidth>
</field>
</fields>
</register>
<register>
<name>ISER0</name>
<displayName>ISER0</displayName>
<description>Interrupt Set-Enable Register</description>
<addressOffset>0x100</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>SETENA</name>
<description>SETENA</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>ISER1</name>
<displayName>ISER1</displayName>
<description>Interrupt Set-Enable Register</description>
<addressOffset>0x104</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>SETENA</name>
<description>SETENA</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>ISER2</name>
<displayName>ISER2</displayName>
<description>Interrupt Set-Enable Register</description>
<addressOffset>0x108</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>SETENA</name>
<description>SETENA</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>ICER0</name>
<displayName>ICER0</displayName>
<description>Interrupt Clear-Enable           Register</description>
<addressOffset>0x180</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CLRENA</name>
<description>CLRENA</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>ICER1</name>
<displayName>ICER1</displayName>
<description>Interrupt Clear-Enable           Register</description>
<addressOffset>0x184</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CLRENA</name>
<description>CLRENA</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>ICER2</name>
<displayName>ICER2</displayName>
<description>Interrupt Clear-Enable           Register</description>
<addressOffset>0x188</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CLRENA</name>
<description>CLRENA</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>ISPR0</name>
<displayName>ISPR0</displayName>
<description>Interrupt Set-Pending Register</description>
<addressOffset>0x200</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>SETPEND</name>
<description>SETPEND</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>ISPR1</name>
<displayName>ISPR1</displayName>
<description>Interrupt Set-Pending Register</description>
<addressOffset>0x204</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>SETPEND</name>
<description>SETPEND</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>ISPR2</name>
<displayName>ISPR2</displayName>
<description>Interrupt Set-Pending Register</description>
<addressOffset>0x208</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>SETPEND</name>
<description>SETPEND</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>ICPR0</name>
<displayName>ICPR0</displayName>
<description>Interrupt Clear-Pending           Register</description>
<addressOffset>0x280</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CLRPEND</name>
<description>CLRPEND</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>ICPR1</name>
<displayName>ICPR1</displayName>
<description>Interrupt Clear-Pending           Register</description>
<addressOffset>0x284</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CLRPEND</name>
<description>CLRPEND</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>ICPR2</name>
<displayName>ICPR2</displayName>
<description>Interrupt Clear-Pending           Register</description>
<addressOffset>0x288</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CLRPEND</name>
<description>CLRPEND</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>IABR0</name>
<displayName>IABR0</displayName>
<description>Interrupt Active Bit Register</description>
<addressOffset>0x300</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>ACTIVE</name>
<description>ACTIVE</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>IABR1</name>
<displayName>IABR1</displayName>
<description>Interrupt Active Bit Register</description>
<addressOffset>0x304</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>ACTIVE</name>
<description>ACTIVE</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>IABR2</name>
<displayName>IABR2</displayName>
<description>Interrupt Active Bit Register</description>
<addressOffset>0x308</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>ACTIVE</name>
<description>ACTIVE</description>
<bitOffset>0</bitOffset>
<bitWidth>32</bitWidth>
</field>
</fields>
</register>
<register>
<name>IPR0</name>
<displayName>IPR0</displayName>
<description>Interrupt Priority Register</description>
<addressOffset>0x400</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IPR_N0</name>
<description>IPR_N0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N1</name>
<description>IPR_N1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N2</name>
<description>IPR_N2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N3</name>
<description>IPR_N3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>IPR1</name>
<displayName>IPR1</displayName>
<description>Interrupt Priority Register</description>
<addressOffset>0x404</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IPR_N0</name>
<description>IPR_N0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N1</name>
<description>IPR_N1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N2</name>
<description>IPR_N2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N3</name>
<description>IPR_N3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>IPR2</name>
<displayName>IPR2</displayName>
<description>Interrupt Priority Register</description>
<addressOffset>0x408</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IPR_N0</name>
<description>IPR_N0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N1</name>
<description>IPR_N1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N2</name>
<description>IPR_N2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N3</name>
<description>IPR_N3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>IPR3</name>
<displayName>IPR3</displayName>
<description>Interrupt Priority Register</description>
<addressOffset>0x40C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IPR_N0</name>
<description>IPR_N0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N1</name>
<description>IPR_N1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N2</name>
<description>IPR_N2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N3</name>
<description>IPR_N3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>IPR4</name>
<displayName>IPR4</displayName>
<description>Interrupt Priority Register</description>
<addressOffset>0x410</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IPR_N0</name>
<description>IPR_N0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N1</name>
<description>IPR_N1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N2</name>
<description>IPR_N2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N3</name>
<description>IPR_N3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>IPR5</name>
<displayName>IPR5</displayName>
<description>Interrupt Priority Register</description>
<addressOffset>0x414</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IPR_N0</name>
<description>IPR_N0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N1</name>
<description>IPR_N1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N2</name>
<description>IPR_N2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N3</name>
<description>IPR_N3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>IPR6</name>
<displayName>IPR6</displayName>
<description>Interrupt Priority Register</description>
<addressOffset>0x418</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IPR_N0</name>
<description>IPR_N0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N1</name>
<description>IPR_N1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N2</name>
<description>IPR_N2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N3</name>
<description>IPR_N3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>IPR7</name>
<displayName>IPR7</displayName>
<description>Interrupt Priority Register</description>
<addressOffset>0x41C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IPR_N0</name>
<description>IPR_N0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N1</name>
<description>IPR_N1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N2</name>
<description>IPR_N2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N3</name>
<description>IPR_N3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>IPR8</name>
<displayName>IPR8</displayName>
<description>Interrupt Priority Register</description>
<addressOffset>0x420</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IPR_N0</name>
<description>IPR_N0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N1</name>
<description>IPR_N1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N2</name>
<description>IPR_N2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N3</name>
<description>IPR_N3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>IPR9</name>
<displayName>IPR9</displayName>
<description>Interrupt Priority Register</description>
<addressOffset>0x424</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IPR_N0</name>
<description>IPR_N0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N1</name>
<description>IPR_N1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N2</name>
<description>IPR_N2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N3</name>
<description>IPR_N3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>IPR10</name>
<displayName>IPR10</displayName>
<description>Interrupt Priority Register</description>
<addressOffset>0x428</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IPR_N0</name>
<description>IPR_N0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N1</name>
<description>IPR_N1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N2</name>
<description>IPR_N2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N3</name>
<description>IPR_N3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>IPR11</name>
<displayName>IPR11</displayName>
<description>Interrupt Priority Register</description>
<addressOffset>0x42C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IPR_N0</name>
<description>IPR_N0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N1</name>
<description>IPR_N1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N2</name>
<description>IPR_N2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N3</name>
<description>IPR_N3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>IPR12</name>
<displayName>IPR12</displayName>
<description>Interrupt Priority Register</description>
<addressOffset>0x430</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IPR_N0</name>
<description>IPR_N0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N1</name>
<description>IPR_N1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N2</name>
<description>IPR_N2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N3</name>
<description>IPR_N3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>IPR13</name>
<displayName>IPR13</displayName>
<description>Interrupt Priority Register</description>
<addressOffset>0x434</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IPR_N0</name>
<description>IPR_N0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N1</name>
<description>IPR_N1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N2</name>
<description>IPR_N2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N3</name>
<description>IPR_N3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>IPR14</name>
<displayName>IPR14</displayName>
<description>Interrupt Priority Register</description>
<addressOffset>0x438</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IPR_N0</name>
<description>IPR_N0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N1</name>
<description>IPR_N1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N2</name>
<description>IPR_N2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N3</name>
<description>IPR_N3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>IPR15</name>
<displayName>IPR15</displayName>
<description>Interrupt Priority Register</description>
<addressOffset>0x43C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IPR_N0</name>
<description>IPR_N0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N1</name>
<description>IPR_N1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N2</name>
<description>IPR_N2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N3</name>
<description>IPR_N3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>IPR16</name>
<displayName>IPR16</displayName>
<description>Interrupt Priority Register</description>
<addressOffset>0x440</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IPR_N0</name>
<description>IPR_N0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N1</name>
<description>IPR_N1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N2</name>
<description>IPR_N2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N3</name>
<description>IPR_N3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>IPR17</name>
<displayName>IPR17</displayName>
<description>Interrupt Priority Register</description>
<addressOffset>0x444</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IPR_N0</name>
<description>IPR_N0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N1</name>
<description>IPR_N1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N2</name>
<description>IPR_N2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N3</name>
<description>IPR_N3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>IPR18</name>
<displayName>IPR18</displayName>
<description>Interrupt Priority Register</description>
<addressOffset>0x448</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IPR_N0</name>
<description>IPR_N0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N1</name>
<description>IPR_N1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N2</name>
<description>IPR_N2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N3</name>
<description>IPR_N3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>IPR19</name>
<displayName>IPR19</displayName>
<description>Interrupt Priority Register</description>
<addressOffset>0x44C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IPR_N0</name>
<description>IPR_N0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N1</name>
<description>IPR_N1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N2</name>
<description>IPR_N2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N3</name>
<description>IPR_N3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>IPR20</name>
<displayName>IPR20</displayName>
<description>Interrupt Priority Register</description>
<addressOffset>0x450</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IPR_N0</name>
<description>IPR_N0</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N1</name>
<description>IPR_N1</description>
<bitOffset>8</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N2</name>
<description>IPR_N2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>IPR_N3</name>
<description>IPR_N3</description>
<bitOffset>24</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral>
<name>FPU</name>
<description>Floting point unit</description>
<groupName>FPU</groupName>
<baseAddress>0xE000ED88</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x200</size>
<usage>registers</usage>
</addressBlock>
<interrupt>
<name>FPU</name>
<description>Floating point interrupt</description>
<value>81</value>
</interrupt>
<registers>
<register>
<name>CPACR</name>
<displayName>CPACR</displayName>
<description>Coprocessor Access Control           Register</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CP0</name>
<description>Access privileges for coprocessor               0</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CP1</name>
<description>Access privileges for coprocessor               1</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CP2</name>
<description>Access privileges for coprocessor               2</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CP3</name>
<description>Access privileges for coprocessor               3</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CP4</name>
<description>Access privileges for coprocessor               4</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CP5</name>
<description>Access privileges for coprocessor               5</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CP6</name>
<description>Access privileges for coprocessor               6</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>CP7</name>
<description>Access privileges for coprocessor               7</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CP10</name>
<description>Access privileges for coprocessor               10</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CP11</name>
<description>Access privileges for coprocessor               11</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>FPCCR</name>
<displayName>FPCCR</displayName>
<description>FP Context Control Register</description>
<addressOffset>0x1AC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0xC0000000</resetValue>
<fields>
<field>
<name>LSPACT</name>
<description>LSPACT</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>USER</name>
<description>USER</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>THREAD</name>
<description>THREAD</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>HFRDY</name>
<description>HFRDY</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MMRDY</name>
<description>MMRDY</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BFRDY</name>
<description>BFRDY</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MONRDY</name>
<description>MONRDY</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>LSPEN</name>
<description>LSPEN</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ASPEN</name>
<description>ASPEN</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>FPCAR</name>
<displayName>FPCAR</displayName>
<description>FP Context Address Register</description>
<addressOffset>0x1B0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>ADDRESS</name>
<description>ADDRESS</description>
<bitOffset>3</bitOffset>
<bitWidth>29</bitWidth>
</field>
</fields>
</register>
<register>
<name>FPDSCR</name>
<displayName>FPDSCR</displayName>
<description>FP Default Status Control           Register</description>
<addressOffset>0x1B4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>RMode</name>
<description>RMode</description>
<bitOffset>22</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>FZ</name>
<description>FZ</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DN</name>
<description>DN</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>AHP</name>
<description>AHP</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>MVFR0</name>
<displayName>MVFR0</displayName>
<description>Media and VFP Feature Register           0</description>
<addressOffset>0x1B8</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x10110021</resetValue>
<fields>
<field>
<name>A_SIMD</name>
<description>A_SIMD registers</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>Single_precision</name>
<description>Single_precision</description>
<bitOffset>4</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>Double_precision</name>
<description>Double_precision</description>
<bitOffset>8</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>FP_exception_trapping</name>
<description>FP exception trapping</description>
<bitOffset>12</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>Divide</name>
<description>Divide</description>
<bitOffset>16</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>Square_root</name>
<description>Square root</description>
<bitOffset>20</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>Short_vectors</name>
<description>Short vectors</description>
<bitOffset>24</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>FP_rounding_modes</name>
<description>FP rounding modes</description>
<bitOffset>28</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>MVFR1</name>
<displayName>MVFR1</displayName>
<description>Media and VFP Feature Register           1</description>
<addressOffset>0x1BC</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x11000011</resetValue>
<fields>
<field>
<name>FtZ_mode</name>
<description>FtZ mode</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>D_NaN_mode</name>
<description>D_NaN mode</description>
<bitOffset>4</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>FP_HPFP</name>
<description>FP HPFP</description>
<bitOffset>24</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>FP_fused_MAC</name>
<description>FP fused MAC</description>
<bitOffset>28</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral>
<name>DBGMCU</name>
<description>Debug support</description>
<groupName>DBGMCU</groupName>
<baseAddress>0xE0042000</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<registers>
<register>
<name>IDCODE</name>
<displayName>IDCODE</displayName>
<description>MCU Device ID Code Register</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x0</resetValue>
<fields>
<field>
<name>DEV_ID</name>
<description>Device Identifier</description>
<bitOffset>0</bitOffset>
<bitWidth>12</bitWidth>
</field>
<field>
<name>REV_ID</name>
<description>Revision Identifier</description>
<bitOffset>16</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>CR</name>
<displayName>CR</displayName>
<description>Debug MCU Configuration           Register</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0</resetValue>
<fields>
<field>
<name>DBG_SLEEP</name>
<description>Debug Sleep mode</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DBG_STOP</name>
<description>Debug Stop Mode</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DBG_STANDBY</name>
<description>Debug Standby Mode</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TRACE_IOEN</name>
<description>Trace pin assignment               control</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TRACE_MODE</name>
<description>Trace pin assignment               control</description>
<bitOffset>6</bitOffset>
<bitWidth>2</bitWidth>
</field>
</fields>
</register>
<register>
<name>APB1FZ</name>
<displayName>APB1FZ</displayName>
<description>APB Low Freeze Register</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0</resetValue>
<fields>
<field>
<name>DBG_TIM2_STOP</name>
<description>Debug Timer 2 stopped when Core is               halted</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DBG_TIM3_STOP</name>
<description>Debug Timer 3 stopped when Core is               halted</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DBG_TIM4_STOP</name>
<description>Debug Timer 4 stopped when Core is               halted</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DBG_TIM5_STOP</name>
<description>Debug Timer 5 stopped when Core is               halted</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DBG_TIM6_STOP</name>
<description>Debug Timer 6 stopped when Core is               halted</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DBG_TIM7_STOP</name>
<description>Debug Timer 7 stopped when Core is               halted</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DBG_TIM12_STOP</name>
<description>Debug Timer 12 stopped when Core is               halted</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DBG_TIM13_STOP</name>
<description>Debug Timer 13 stopped when Core is               halted</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DBG_TIMER14_STOP</name>
<description>Debug Timer 14 stopped when Core is               halted</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DBG_TIM18_STOP</name>
<description>Debug Timer 18 stopped when Core is               halted</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DBG_RTC_STOP</name>
<description>Debug RTC stopped when Core is               halted</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DBG_WWDG_STOP</name>
<description>Debug Window Wachdog stopped when Core               is halted</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DBG_IWDG_STOP</name>
<description>Debug Independent Wachdog stopped when               Core is halted</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>I2C1_SMBUS_TIMEOUT</name>
<description>SMBUS timeout mode stopped when Core is               halted</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>I2C2_SMBUS_TIMEOUT</name>
<description>SMBUS timeout mode stopped when Core is               halted</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DBG_CAN_STOP</name>
<description>Debug CAN stopped when core is               halted</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>APB2FZ</name>
<displayName>APB2FZ</displayName>
<description>APB High Freeze Register</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0</resetValue>
<fields>
<field>
<name>DBG_TIM15_STOP</name>
<description>Debug Timer 15 stopped when Core is               halted</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DBG_TIM16_STOP</name>
<description>Debug Timer 16 stopped when Core is               halted</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DBG_TIM17_STO</name>
<description>Debug Timer 17 stopped when Core is               halted</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DBG_TIM19_STOP</name>
<description>Debug Timer 19 stopped when Core is               halted</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral>
<name>TIM1</name>
<description>Advanced timer</description>
<groupName>TIMs</groupName>
<baseAddress>0x40012C00</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<interrupt>
<name>TIM1_CC</name>
<description>TIM1 capture compare interrupt</description>
<value>27</value>
</interrupt>
<registers>
<register>
<name>CR1</name>
<displayName>CR1</displayName>
<description>control register 1</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>CEN</name>
<description>Counter enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UDIS</name>
<description>Update disable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>URS</name>
<description>Update request source</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OPM</name>
<description>One-pulse mode</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DIR</name>
<description>Direction</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CMS</name>
<description>Center-aligned mode               selection</description>
<bitOffset>5</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>ARPE</name>
<description>Auto-reload preload enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CKD</name>
<description>Clock division</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>UIFREMAP</name>
<description>UIF status bit remapping</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CR2</name>
<displayName>CR2</displayName>
<description>control register 2</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>CCPC</name>
<description>Capture/compare preloaded               control</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CCUS</name>
<description>Capture/compare control update               selection</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CCDS</name>
<description>Capture/compare DMA               selection</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MMS</name>
<description>Master mode selection</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>TI1S</name>
<description>TI1 selection</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OIS1</name>
<description>Output Idle state 1</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OIS1N</name>
<description>Output Idle state 1</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OIS2</name>
<description>Output Idle state 2</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OIS2N</name>
<description>Output Idle state 2</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OIS3</name>
<description>Output Idle state 3</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OIS3N</name>
<description>Output Idle state 3</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OIS4</name>
<description>Output Idle state 4</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OIS5</name>
<description>Output Idle state 5</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OIS6</name>
<description>Output Idle state 6</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MMS2</name>
<description>Master mode selection 2</description>
<bitOffset>20</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>SMCR</name>
<displayName>SMCR</displayName>
<description>slave mode control register</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>SMS</name>
<description>Slave mode selection</description>
<bitOffset>0</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>OCCS</name>
<description>OCREF clear selection</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TS</name>
<description>Trigger selection</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>MSM</name>
<description>Master/Slave mode</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ETF</name>
<description>External trigger filter</description>
<bitOffset>8</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>ETPS</name>
<description>External trigger prescaler</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>ECE</name>
<description>External clock enable</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ETP</name>
<description>External trigger polarity</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SMS3</name>
<description>Slave mode selection bit 3</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>DIER</name>
<displayName>DIER</displayName>
<description>DMA/Interrupt enable register</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>TDE</name>
<description>Trigger DMA request enable</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>COMDE</name>
<description>Reserved</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4DE</name>
<description>Capture/Compare 4 DMA request               enable</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3DE</name>
<description>Capture/Compare 3 DMA request               enable</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2DE</name>
<description>Capture/Compare 2 DMA request               enable</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1DE</name>
<description>Capture/Compare 1 DMA request               enable</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UDE</name>
<description>Update DMA request enable</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BIE</name>
<description>Break interrupt enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIE</name>
<description>Trigger interrupt enable</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>COMIE</name>
<description>COM interrupt enable</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4IE</name>
<description>Capture/Compare 4 interrupt               enable</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3IE</name>
<description>Capture/Compare 3 interrupt               enable</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2IE</name>
<description>Capture/Compare 2 interrupt               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1IE</name>
<description>Capture/Compare 1 interrupt               enable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UIE</name>
<description>Update interrupt enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>SR</name>
<displayName>SR</displayName>
<description>status register</description>
<addressOffset>0x10</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>UIF</name>
<description>Update interrupt flag</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1IF</name>
<description>Capture/compare 1 interrupt               flag</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2IF</name>
<description>Capture/Compare 2 interrupt               flag</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3IF</name>
<description>Capture/Compare 3 interrupt               flag</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4IF</name>
<description>Capture/Compare 4 interrupt               flag</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>COMIF</name>
<description>COM interrupt flag</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIF</name>
<description>Trigger interrupt flag</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BIF</name>
<description>Break interrupt flag</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>B2IF</name>
<description>Break 2 interrupt flag</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1OF</name>
<description>Capture/Compare 1 overcapture               flag</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2OF</name>
<description>Capture/compare 2 overcapture               flag</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3OF</name>
<description>Capture/Compare 3 overcapture               flag</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4OF</name>
<description>Capture/Compare 4 overcapture               flag</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>C5IF</name>
<description>Capture/Compare 5 interrupt               flag</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>C6IF</name>
<description>Capture/Compare 6 interrupt               flag</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>EGR</name>
<displayName>EGR</displayName>
<description>event generation register</description>
<addressOffset>0x14</addressOffset>
<size>0x20</size>
<access>write-only</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>UG</name>
<description>Update generation</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1G</name>
<description>Capture/compare 1               generation</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2G</name>
<description>Capture/compare 2               generation</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3G</name>
<description>Capture/compare 3               generation</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4G</name>
<description>Capture/compare 4               generation</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>COMG</name>
<description>Capture/Compare control update               generation</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TG</name>
<description>Trigger generation</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BG</name>
<description>Break generation</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>B2G</name>
<description>Break 2 generation</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCMR1_Output</name>
<displayName>CCMR1_Output</displayName>
<description>capture/compare mode register (output           mode)</description>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>OC2CE</name>
<description>Output Compare 2 clear               enable</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC2M</name>
<description>Output Compare 2 mode</description>
<bitOffset>12</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>OC2PE</name>
<description>Output Compare 2 preload               enable</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC2FE</name>
<description>Output Compare 2 fast               enable</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2S</name>
<description>Capture/Compare 2               selection</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OC1CE</name>
<description>Output Compare 1 clear               enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC1M</name>
<description>Output Compare 1 mode</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>OC1PE</name>
<description>Output Compare 1 preload               enable</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC1FE</name>
<description>Output Compare 1 fast               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1S</name>
<description>Capture/Compare 1               selection</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OC1M_3</name>
<description>Output Compare 1 mode bit               3</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC2M_3</name>
<description>Output Compare 2 mode bit               3</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCMR1_Input</name>
<displayName>CCMR1_Input</displayName>
<description>capture/compare mode register 1 (input           mode)</description>
<alternateRegister>CCMR1_Output</alternateRegister>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IC2F</name>
<description>Input capture 2 filter</description>
<bitOffset>12</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>IC2PCS</name>
<description>Input capture 2 prescaler</description>
<bitOffset>10</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>CC2S</name>
<description>Capture/Compare 2               selection</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>IC1F</name>
<description>Input capture 1 filter</description>
<bitOffset>4</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>IC1PCS</name>
<description>Input capture 1 prescaler</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>CC1S</name>
<description>Capture/Compare 1               selection</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCMR2_Output</name>
<displayName>CCMR2_Output</displayName>
<description>capture/compare mode register (output           mode)</description>
<addressOffset>0x1C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>OC4CE</name>
<description>Output compare 4 clear               enable</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC4M</name>
<description>Output compare 4 mode</description>
<bitOffset>12</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>OC4PE</name>
<description>Output compare 4 preload               enable</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC4FE</name>
<description>Output compare 4 fast               enable</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4S</name>
<description>Capture/Compare 4               selection</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OC3CE</name>
<description>Output compare 3 clear               enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC3M</name>
<description>Output compare 3 mode</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>OC3PE</name>
<description>Output compare 3 preload               enable</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC3FE</name>
<description>Output compare 3 fast               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3S</name>
<description>Capture/Compare 3               selection</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OC3M_3</name>
<description>Output Compare 3 mode bit               3</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC4M_3</name>
<description>Output Compare 4 mode bit               3</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCMR2_Input</name>
<displayName>CCMR2_Input</displayName>
<description>capture/compare mode register 2 (input           mode)</description>
<alternateRegister>CCMR2_Output</alternateRegister>
<addressOffset>0x1C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IC4F</name>
<description>Input capture 4 filter</description>
<bitOffset>12</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>IC4PSC</name>
<description>Input capture 4 prescaler</description>
<bitOffset>10</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>CC4S</name>
<description>Capture/Compare 4               selection</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>IC3F</name>
<description>Input capture 3 filter</description>
<bitOffset>4</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>IC3PSC</name>
<description>Input capture 3 prescaler</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>CC3S</name>
<description>Capture/compare 3               selection</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCER</name>
<displayName>CCER</displayName>
<description>capture/compare enable           register</description>
<addressOffset>0x20</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>CC1E</name>
<description>Capture/Compare 1 output               enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1P</name>
<description>Capture/Compare 1 output               Polarity</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1NE</name>
<description>Capture/Compare 1 complementary output               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1NP</name>
<description>Capture/Compare 1 output               Polarity</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2E</name>
<description>Capture/Compare 2 output               enable</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2P</name>
<description>Capture/Compare 2 output               Polarity</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2NE</name>
<description>Capture/Compare 2 complementary output               enable</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2NP</name>
<description>Capture/Compare 2 output               Polarity</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3E</name>
<description>Capture/Compare 3 output               enable</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3P</name>
<description>Capture/Compare 3 output               Polarity</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3NE</name>
<description>Capture/Compare 3 complementary output               enable</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3NP</name>
<description>Capture/Compare 3 output               Polarity</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4E</name>
<description>Capture/Compare 4 output               enable</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4P</name>
<description>Capture/Compare 3 output               Polarity</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4NP</name>
<description>Capture/Compare 4 output               Polarity</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC5E</name>
<description>Capture/Compare 5 output               enable</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC5P</name>
<description>Capture/Compare 5 output               Polarity</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC6E</name>
<description>Capture/Compare 6 output               enable</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC6P</name>
<description>Capture/Compare 6 output               Polarity</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CNT</name>
<displayName>CNT</displayName>
<description>counter</description>
<addressOffset>0x24</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CNT</name>
<description>counter value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
<access>read-write</access>
</field>
<field>
<name>UIFCPY</name>
<description>UIF copy</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
</fields>
</register>
<register>
<name>PSC</name>
<displayName>PSC</displayName>
<description>prescaler</description>
<addressOffset>0x28</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>PSC</name>
<description>Prescaler value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>ARR</name>
<displayName>ARR</displayName>
<description>auto-reload register</description>
<addressOffset>0x2C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>ARR</name>
<description>Auto-reload value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>RCR</name>
<displayName>RCR</displayName>
<description>repetition counter register</description>
<addressOffset>0x30</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>REP</name>
<description>Repetition counter value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR1</name>
<displayName>CCR1</displayName>
<description>capture/compare register 1</description>
<addressOffset>0x34</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CCR1</name>
<description>Capture/Compare 1 value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR2</name>
<displayName>CCR2</displayName>
<description>capture/compare register 2</description>
<addressOffset>0x38</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CCR2</name>
<description>Capture/Compare 2 value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR3</name>
<displayName>CCR3</displayName>
<description>capture/compare register 3</description>
<addressOffset>0x3C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CCR3</name>
<description>Capture/Compare 3 value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR4</name>
<displayName>CCR4</displayName>
<description>capture/compare register 4</description>
<addressOffset>0x40</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CCR4</name>
<description>Capture/Compare 3 value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>BDTR</name>
<displayName>BDTR</displayName>
<description>break and dead-time register</description>
<addressOffset>0x44</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DTG</name>
<description>Dead-time generator setup</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>LOCK</name>
<description>Lock configuration</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSSI</name>
<description>Off-state selection for Idle               mode</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OSSR</name>
<description>Off-state selection for Run               mode</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BKE</name>
<description>Break enable</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BKP</name>
<description>Break polarity</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>AOE</name>
<description>Automatic output enable</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MOE</name>
<description>Main output enable</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BKF</name>
<description>Break filter</description>
<bitOffset>16</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>BK2F</name>
<description>Break 2 filter</description>
<bitOffset>20</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>BK2E</name>
<description>Break 2 enable</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BK2P</name>
<description>Break 2 polarity</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>DCR</name>
<displayName>DCR</displayName>
<description>DMA control register</description>
<addressOffset>0x48</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DBL</name>
<description>DMA burst length</description>
<bitOffset>8</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>DBA</name>
<description>DMA base address</description>
<bitOffset>0</bitOffset>
<bitWidth>5</bitWidth>
</field>
</fields>
</register>
<register>
<name>DMAR</name>
<displayName>DMAR</displayName>
<description>DMA address for full transfer</description>
<addressOffset>0x4C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DMAB</name>
<description>DMA register for burst               accesses</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCMR3_Output</name>
<displayName>CCMR3_Output</displayName>
<description>capture/compare mode register 3 (output           mode)</description>
<addressOffset>0x54</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>OC5FE</name>
<description>Output compare 5 fast               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC5PE</name>
<description>Output compare 5 preload               enable</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC5M</name>
<description>Output compare 5 mode</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>OC5CE</name>
<description>Output compare 5 clear               enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC6FE</name>
<description>Output compare 6 fast               enable</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC6PE</name>
<description>Output compare 6 preload               enable</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC6M</name>
<description>Output compare 6 mode</description>
<bitOffset>12</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>OC6CE</name>
<description>Output compare 6 clear               enable</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC5M_3</name>
<description>Outout Compare 5 mode bit               3</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC6M_3</name>
<description>Outout Compare 6 mode bit               3</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR5</name>
<displayName>CCR5</displayName>
<description>capture/compare register 5</description>
<addressOffset>0x58</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CCR5</name>
<description>Capture/Compare 5 value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
<field>
<name>GC5C1</name>
<description>Group Channel 5 and Channel               1</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>GC5C2</name>
<description>Group Channel 5 and Channel               2</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>GC5C3</name>
<description>Group Channel 5 and Channel               3</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR6</name>
<displayName>CCR6</displayName>
<description>capture/compare register 6</description>
<addressOffset>0x5C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CCR6</name>
<description>Capture/Compare 6 value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>OR</name>
<displayName>OR</displayName>
<description>option registers</description>
<addressOffset>0x60</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>TIM1_ETR_ADC1_RMP</name>
<description>TIM1_ETR_ADC1 remapping               capability</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>TIM1_ETR_ADC4_RMP</name>
<description>TIM1_ETR_ADC4 remapping               capability</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral derivedFrom="TIM1">
<name>TIM20</name>
<baseAddress>0x40015000</baseAddress>
<interrupt>
<name>TIM1_CC</name>
<description>TIM1 capture compare interrupt</description>
<value>27</value>
</interrupt>
</peripheral>
<peripheral>
<name>TIM8</name>
<description>Advanced-timers</description>
<groupName>TIMs</groupName>
<baseAddress>0x40013400</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x400</size>
<usage>registers</usage>
</addressBlock>
<interrupt>
<name>TIM8_BRK</name>
<description>TIM8 break interrupt</description>
<value>43</value>
</interrupt>
<interrupt>
<name>TIM8_UP</name>
<description>TIM8 update interrupt</description>
<value>44</value>
</interrupt>
<interrupt>
<name>TIM8_TRG_COM</name>
<description>TIM8 Trigger and commutation
        interrupts</description>
<value>45</value>
</interrupt>
<interrupt>
<name>TIM8_CC</name>
<description>TIM8 capture compare interrupt</description>
<value>46</value>
</interrupt>
<registers>
<register>
<name>CR1</name>
<displayName>CR1</displayName>
<description>control register 1</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>CEN</name>
<description>Counter enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UDIS</name>
<description>Update disable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>URS</name>
<description>Update request source</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OPM</name>
<description>One-pulse mode</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DIR</name>
<description>Direction</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CMS</name>
<description>Center-aligned mode               selection</description>
<bitOffset>5</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>ARPE</name>
<description>Auto-reload preload enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CKD</name>
<description>Clock division</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>UIFREMAP</name>
<description>UIF status bit remapping</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CR2</name>
<displayName>CR2</displayName>
<description>control register 2</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>CCPC</name>
<description>Capture/compare preloaded               control</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CCUS</name>
<description>Capture/compare control update               selection</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CCDS</name>
<description>Capture/compare DMA               selection</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MMS</name>
<description>Master mode selection</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>TI1S</name>
<description>TI1 selection</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OIS1</name>
<description>Output Idle state 1</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OIS1N</name>
<description>Output Idle state 1</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OIS2</name>
<description>Output Idle state 2</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OIS2N</name>
<description>Output Idle state 2</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OIS3</name>
<description>Output Idle state 3</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OIS3N</name>
<description>Output Idle state 3</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OIS4</name>
<description>Output Idle state 4</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OIS5</name>
<description>Output Idle state 5</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OIS6</name>
<description>Output Idle state 6</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MMS2</name>
<description>Master mode selection 2</description>
<bitOffset>20</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>SMCR</name>
<displayName>SMCR</displayName>
<description>slave mode control register</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>SMS</name>
<description>Slave mode selection</description>
<bitOffset>0</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>OCCS</name>
<description>OCREF clear selection</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TS</name>
<description>Trigger selection</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>MSM</name>
<description>Master/Slave mode</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ETF</name>
<description>External trigger filter</description>
<bitOffset>8</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>ETPS</name>
<description>External trigger prescaler</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>ECE</name>
<description>External clock enable</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ETP</name>
<description>External trigger polarity</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SMS3</name>
<description>Slave mode selection bit 3</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>DIER</name>
<displayName>DIER</displayName>
<description>DMA/Interrupt enable register</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>TDE</name>
<description>Trigger DMA request enable</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>COMDE</name>
<description>Reserved</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4DE</name>
<description>Capture/Compare 4 DMA request               enable</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3DE</name>
<description>Capture/Compare 3 DMA request               enable</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2DE</name>
<description>Capture/Compare 2 DMA request               enable</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1DE</name>
<description>Capture/Compare 1 DMA request               enable</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UDE</name>
<description>Update DMA request enable</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BIE</name>
<description>Break interrupt enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIE</name>
<description>Trigger interrupt enable</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>COMIE</name>
<description>COM interrupt enable</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4IE</name>
<description>Capture/Compare 4 interrupt               enable</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3IE</name>
<description>Capture/Compare 3 interrupt               enable</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2IE</name>
<description>Capture/Compare 2 interrupt               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1IE</name>
<description>Capture/Compare 1 interrupt               enable</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>UIE</name>
<description>Update interrupt enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>SR</name>
<displayName>SR</displayName>
<description>status register</description>
<addressOffset>0x10</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>UIF</name>
<description>Update interrupt flag</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1IF</name>
<description>Capture/compare 1 interrupt               flag</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2IF</name>
<description>Capture/Compare 2 interrupt               flag</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3IF</name>
<description>Capture/Compare 3 interrupt               flag</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4IF</name>
<description>Capture/Compare 4 interrupt               flag</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>COMIF</name>
<description>COM interrupt flag</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIF</name>
<description>Trigger interrupt flag</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BIF</name>
<description>Break interrupt flag</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>B2IF</name>
<description>Break 2 interrupt flag</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1OF</name>
<description>Capture/Compare 1 overcapture               flag</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2OF</name>
<description>Capture/compare 2 overcapture               flag</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3OF</name>
<description>Capture/Compare 3 overcapture               flag</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4OF</name>
<description>Capture/Compare 4 overcapture               flag</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>C5IF</name>
<description>Capture/Compare 5 interrupt               flag</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>C6IF</name>
<description>Capture/Compare 6 interrupt               flag</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>EGR</name>
<displayName>EGR</displayName>
<description>event generation register</description>
<addressOffset>0x14</addressOffset>
<size>0x20</size>
<access>write-only</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>UG</name>
<description>Update generation</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1G</name>
<description>Capture/compare 1               generation</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2G</name>
<description>Capture/compare 2               generation</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3G</name>
<description>Capture/compare 3               generation</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4G</name>
<description>Capture/compare 4               generation</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>COMG</name>
<description>Capture/Compare control update               generation</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TG</name>
<description>Trigger generation</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BG</name>
<description>Break generation</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>B2G</name>
<description>Break 2 generation</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCMR1_Output</name>
<displayName>CCMR1_Output</displayName>
<description>capture/compare mode register (output           mode)</description>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>OC2CE</name>
<description>Output Compare 2 clear               enable</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC2M</name>
<description>Output Compare 2 mode</description>
<bitOffset>12</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>OC2PE</name>
<description>Output Compare 2 preload               enable</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC2FE</name>
<description>Output Compare 2 fast               enable</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2S</name>
<description>Capture/Compare 2               selection</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OC1CE</name>
<description>Output Compare 1 clear               enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC1M</name>
<description>Output Compare 1 mode</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>OC1PE</name>
<description>Output Compare 1 preload               enable</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC1FE</name>
<description>Output Compare 1 fast               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1S</name>
<description>Capture/Compare 1               selection</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OC1M_3</name>
<description>Output Compare 1 mode bit               3</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC2M_3</name>
<description>Output Compare 2 mode bit               3</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCMR1_Input</name>
<displayName>CCMR1_Input</displayName>
<description>capture/compare mode register 1 (input           mode)</description>
<alternateRegister>CCMR1_Output</alternateRegister>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IC2F</name>
<description>Input capture 2 filter</description>
<bitOffset>12</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>IC2PCS</name>
<description>Input capture 2 prescaler</description>
<bitOffset>10</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>CC2S</name>
<description>Capture/Compare 2               selection</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>IC1F</name>
<description>Input capture 1 filter</description>
<bitOffset>4</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>IC1PCS</name>
<description>Input capture 1 prescaler</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>CC1S</name>
<description>Capture/Compare 1               selection</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCMR2_Output</name>
<displayName>CCMR2_Output</displayName>
<description>capture/compare mode register (output           mode)</description>
<addressOffset>0x1C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>OC4CE</name>
<description>Output compare 4 clear               enable</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC4M</name>
<description>Output compare 4 mode</description>
<bitOffset>12</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>OC4PE</name>
<description>Output compare 4 preload               enable</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC4FE</name>
<description>Output compare 4 fast               enable</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4S</name>
<description>Capture/Compare 4               selection</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OC3CE</name>
<description>Output compare 3 clear               enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC3M</name>
<description>Output compare 3 mode</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>OC3PE</name>
<description>Output compare 3 preload               enable</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC3FE</name>
<description>Output compare 3 fast               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3S</name>
<description>Capture/Compare 3               selection</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OC3M_3</name>
<description>Output Compare 3 mode bit               3</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC4M_3</name>
<description>Output Compare 4 mode bit               3</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCMR2_Input</name>
<displayName>CCMR2_Input</displayName>
<description>capture/compare mode register 2 (input           mode)</description>
<alternateRegister>CCMR2_Output</alternateRegister>
<addressOffset>0x1C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>IC4F</name>
<description>Input capture 4 filter</description>
<bitOffset>12</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>IC4PSC</name>
<description>Input capture 4 prescaler</description>
<bitOffset>10</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>CC4S</name>
<description>Capture/Compare 4               selection</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>IC3F</name>
<description>Input capture 3 filter</description>
<bitOffset>4</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>IC3PSC</name>
<description>Input capture 3 prescaler</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>CC3S</name>
<description>Capture/compare 3               selection</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCER</name>
<displayName>CCER</displayName>
<description>capture/compare enable           register</description>
<addressOffset>0x20</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>CC1E</name>
<description>Capture/Compare 1 output               enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1P</name>
<description>Capture/Compare 1 output               Polarity</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1NE</name>
<description>Capture/Compare 1 complementary output               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC1NP</name>
<description>Capture/Compare 1 output               Polarity</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2E</name>
<description>Capture/Compare 2 output               enable</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2P</name>
<description>Capture/Compare 2 output               Polarity</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2NE</name>
<description>Capture/Compare 2 complementary output               enable</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC2NP</name>
<description>Capture/Compare 2 output               Polarity</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3E</name>
<description>Capture/Compare 3 output               enable</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3P</name>
<description>Capture/Compare 3 output               Polarity</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3NE</name>
<description>Capture/Compare 3 complementary output               enable</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC3NP</name>
<description>Capture/Compare 3 output               Polarity</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4E</name>
<description>Capture/Compare 4 output               enable</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4P</name>
<description>Capture/Compare 3 output               Polarity</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC4NP</name>
<description>Capture/Compare 4 output               Polarity</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC5E</name>
<description>Capture/Compare 5 output               enable</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC5P</name>
<description>Capture/Compare 5 output               Polarity</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC6E</name>
<description>Capture/Compare 6 output               enable</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CC6P</name>
<description>Capture/Compare 6 output               Polarity</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CNT</name>
<displayName>CNT</displayName>
<description>counter</description>
<addressOffset>0x24</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CNT</name>
<description>counter value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
<access>read-write</access>
</field>
<field>
<name>UIFCPY</name>
<description>UIF copy</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
</fields>
</register>
<register>
<name>PSC</name>
<displayName>PSC</displayName>
<description>prescaler</description>
<addressOffset>0x28</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>PSC</name>
<description>Prescaler value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>ARR</name>
<displayName>ARR</displayName>
<description>auto-reload register</description>
<addressOffset>0x2C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>ARR</name>
<description>Auto-reload value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>RCR</name>
<displayName>RCR</displayName>
<description>repetition counter register</description>
<addressOffset>0x30</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>REP</name>
<description>Repetition counter value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR1</name>
<displayName>CCR1</displayName>
<description>capture/compare register 1</description>
<addressOffset>0x34</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CCR1</name>
<description>Capture/Compare 1 value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR2</name>
<displayName>CCR2</displayName>
<description>capture/compare register 2</description>
<addressOffset>0x38</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CCR2</name>
<description>Capture/Compare 2 value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR3</name>
<displayName>CCR3</displayName>
<description>capture/compare register 3</description>
<addressOffset>0x3C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CCR3</name>
<description>Capture/Compare 3 value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR4</name>
<displayName>CCR4</displayName>
<description>capture/compare register 4</description>
<addressOffset>0x40</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CCR4</name>
<description>Capture/Compare 3 value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>BDTR</name>
<displayName>BDTR</displayName>
<description>break and dead-time register</description>
<addressOffset>0x44</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DTG</name>
<description>Dead-time generator setup</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>LOCK</name>
<description>Lock configuration</description>
<bitOffset>8</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>OSSI</name>
<description>Off-state selection for Idle               mode</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OSSR</name>
<description>Off-state selection for Run               mode</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BKE</name>
<description>Break enable</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BKP</name>
<description>Break polarity</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>AOE</name>
<description>Automatic output enable</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MOE</name>
<description>Main output enable</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BKF</name>
<description>Break filter</description>
<bitOffset>16</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>BK2F</name>
<description>Break 2 filter</description>
<bitOffset>20</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>BK2E</name>
<description>Break 2 enable</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BK2P</name>
<description>Break 2 polarity</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>DCR</name>
<displayName>DCR</displayName>
<description>DMA control register</description>
<addressOffset>0x48</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DBL</name>
<description>DMA burst length</description>
<bitOffset>8</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>DBA</name>
<description>DMA base address</description>
<bitOffset>0</bitOffset>
<bitWidth>5</bitWidth>
</field>
</fields>
</register>
<register>
<name>DMAR</name>
<displayName>DMAR</displayName>
<description>DMA address for full transfer</description>
<addressOffset>0x4C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DMAB</name>
<description>DMA register for burst               accesses</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCMR3_Output</name>
<displayName>CCMR3_Output</displayName>
<description>capture/compare mode register 3 (output           mode)</description>
<addressOffset>0x54</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>OC5FE</name>
<description>Output compare 5 fast               enable</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC5PE</name>
<description>Output compare 5 preload               enable</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC5M</name>
<description>Output compare 5 mode</description>
<bitOffset>4</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>OC5CE</name>
<description>Output compare 5 clear               enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC6FE</name>
<description>Output compare 6 fast               enable</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC6PE</name>
<description>Output compare 6 preload               enable</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC6M</name>
<description>Output compare 6 mode</description>
<bitOffset>12</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>OC6CE</name>
<description>Output compare 6 clear               enable</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC5M_3</name>
<description>Outout Compare 5 mode bit               3</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OC6M_3</name>
<description>Outout Compare 6 mode bit               3</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR5</name>
<displayName>CCR5</displayName>
<description>capture/compare register 5</description>
<addressOffset>0x58</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CCR5</name>
<description>Capture/Compare 5 value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
<field>
<name>GC5C1</name>
<description>Group Channel 5 and Channel               1</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>GC5C2</name>
<description>Group Channel 5 and Channel               2</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>GC5C3</name>
<description>Group Channel 5 and Channel               3</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR6</name>
<displayName>CCR6</displayName>
<description>capture/compare register 6</description>
<addressOffset>0x5C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CCR6</name>
<description>Capture/Compare 6 value</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>OR</name>
<displayName>OR</displayName>
<description>option registers</description>
<addressOffset>0x60</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>TIM8_ETR_ADC2_RMP</name>
<description>TIM8_ETR_ADC2 remapping               capability</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>TIM8_ETR_ADC3_RMP</name>
<description>TIM8_ETR_ADC3 remapping               capability</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral>
<name>ADC1</name>
<description>Analog-to-Digital Converter</description>
<groupName>ADC</groupName>
<baseAddress>0x50000000</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x100</size>
<usage>registers</usage>
</addressBlock>
<interrupt>
<name>ADC1_2</name>
<description>ADC1 and ADC2 global interrupt</description>
<value>18</value>
</interrupt>
<registers>
<register>
<name>ISR</name>
<displayName>ISR</displayName>
<description>interrupt and status register</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>JQOVF</name>
<description>JQOVF</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>AWD3</name>
<description>AWD3</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>AWD2</name>
<description>AWD2</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>AWD1</name>
<description>AWD1</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>JEOS</name>
<description>JEOS</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>JEOC</name>
<description>JEOC</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OVR</name>
<description>OVR</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>EOS</name>
<description>EOS</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>EOC</name>
<description>EOC</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>EOSMP</name>
<description>EOSMP</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ADRDY</name>
<description>ADRDY</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>IER</name>
<displayName>IER</displayName>
<description>interrupt enable register</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>JQOVFIE</name>
<description>JQOVFIE</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>AWD3IE</name>
<description>AWD3IE</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>AWD2IE</name>
<description>AWD2IE</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>AWD1IE</name>
<description>AWD1IE</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>JEOSIE</name>
<description>JEOSIE</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>JEOCIE</name>
<description>JEOCIE</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OVRIE</name>
<description>OVRIE</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>EOSIE</name>
<description>EOSIE</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>EOCIE</name>
<description>EOCIE</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>EOSMPIE</name>
<description>EOSMPIE</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ADRDYIE</name>
<description>ADRDYIE</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CR</name>
<displayName>CR</displayName>
<description>control register</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>ADCAL</name>
<description>ADCAL</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ADCALDIF</name>
<description>ADCALDIF</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DEEPPWD</name>
<description>DEEPPWD</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ADVREGEN</name>
<description>ADVREGEN</description>
<bitOffset>28</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>JADSTP</name>
<description>JADSTP</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ADSTP</name>
<description>ADSTP</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>JADSTART</name>
<description>JADSTART</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ADSTART</name>
<description>ADSTART</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ADDIS</name>
<description>ADDIS</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ADEN</name>
<description>ADEN</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CFGR</name>
<displayName>CFGR</displayName>
<description>configuration register</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>AWDCH1CH</name>
<description>AWDCH1CH</description>
<bitOffset>26</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>JAUTO</name>
<description>JAUTO</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>JAWD1EN</name>
<description>JAWD1EN</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>AWD1EN</name>
<description>AWD1EN</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>AWD1SGL</name>
<description>AWD1SGL</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>JQM</name>
<description>JQM</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>JDISCEN</name>
<description>JDISCEN</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DISCNUM</name>
<description>DISCNUM</description>
<bitOffset>17</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>DISCEN</name>
<description>DISCEN</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>AUTOFF</name>
<description>AUTOFF</description>
<bitOffset>15</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>AUTDLY</name>
<description>AUTDLY</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>CONT</name>
<description>CONT</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OVRMOD</name>
<description>OVRMOD</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>EXTEN</name>
<description>EXTEN</description>
<bitOffset>10</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>EXTSEL</name>
<description>EXTSEL</description>
<bitOffset>6</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>ALIGN</name>
<description>ALIGN</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>RES</name>
<description>RES</description>
<bitOffset>3</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>DMACFG</name>
<description>DMACFG</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DMAEN</name>
<description>DMAEN</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>SMPR1</name>
<displayName>SMPR1</displayName>
<description>sample time register 1</description>
<addressOffset>0x14</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>SMP9</name>
<description>SMP9</description>
<bitOffset>27</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>SMP8</name>
<description>SMP8</description>
<bitOffset>24</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>SMP7</name>
<description>SMP7</description>
<bitOffset>21</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>SMP6</name>
<description>SMP6</description>
<bitOffset>18</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>SMP5</name>
<description>SMP5</description>
<bitOffset>15</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>SMP4</name>
<description>SMP4</description>
<bitOffset>12</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>SMP3</name>
<description>SMP3</description>
<bitOffset>9</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>SMP2</name>
<description>SMP2</description>
<bitOffset>6</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>SMP1</name>
<description>SMP1</description>
<bitOffset>3</bitOffset>
<bitWidth>3</bitWidth>
</field>
</fields>
</register>
<register>
<name>SMPR2</name>
<displayName>SMPR2</displayName>
<description>sample time register 2</description>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>SMP18</name>
<description>SMP18</description>
<bitOffset>24</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>SMP17</name>
<description>SMP17</description>
<bitOffset>21</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>SMP16</name>
<description>SMP16</description>
<bitOffset>18</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>SMP15</name>
<description>SMP15</description>
<bitOffset>15</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>SMP14</name>
<description>SMP14</description>
<bitOffset>12</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>SMP13</name>
<description>SMP13</description>
<bitOffset>9</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>SMP12</name>
<description>SMP12</description>
<bitOffset>6</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>SMP11</name>
<description>SMP11</description>
<bitOffset>3</bitOffset>
<bitWidth>3</bitWidth>
</field>
<field>
<name>SMP10</name>
<description>SMP10</description>
<bitOffset>0</bitOffset>
<bitWidth>3</bitWidth>
</field>
</fields>
</register>
<register>
<name>TR1</name>
<displayName>TR1</displayName>
<description>watchdog threshold register 1</description>
<addressOffset>0x20</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0FFF0000</resetValue>
<fields>
<field>
<name>HT1</name>
<description>HT1</description>
<bitOffset>16</bitOffset>
<bitWidth>12</bitWidth>
</field>
<field>
<name>LT1</name>
<description>LT1</description>
<bitOffset>0</bitOffset>
<bitWidth>12</bitWidth>
</field>
</fields>
</register>
<register>
<name>TR2</name>
<displayName>TR2</displayName>
<description>watchdog threshold register</description>
<addressOffset>0x24</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0FFF0000</resetValue>
<fields>
<field>
<name>HT2</name>
<description>HT2</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>LT2</name>
<description>LT2</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>TR3</name>
<displayName>TR3</displayName>
<description>watchdog threshold register 3</description>
<addressOffset>0x28</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0FFF0000</resetValue>
<fields>
<field>
<name>HT3</name>
<description>HT3</description>
<bitOffset>16</bitOffset>
<bitWidth>8</bitWidth>
</field>
<field>
<name>LT3</name>
<description>LT3</description>
<bitOffset>0</bitOffset>
<bitWidth>8</bitWidth>
</field>
</fields>
</register>
<register>
<name>SQR1</name>
<displayName>SQR1</displayName>
<description>regular sequence register 1</description>
<addressOffset>0x30</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>SQ4</name>
<description>SQ4</description>
<bitOffset>24</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>SQ3</name>
<description>SQ3</description>
<bitOffset>18</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>SQ2</name>
<description>SQ2</description>
<bitOffset>12</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>SQ1</name>
<description>SQ1</description>
<bitOffset>6</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>L3</name>
<description>L3</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>SQR2</name>
<displayName>SQR2</displayName>
<description>regular sequence register 2</description>
<addressOffset>0x34</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>SQ9</name>
<description>SQ9</description>
<bitOffset>24</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>SQ8</name>
<description>SQ8</description>
<bitOffset>18</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>SQ7</name>
<description>SQ7</description>
<bitOffset>12</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>SQ6</name>
<description>SQ6</description>
<bitOffset>6</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>SQ5</name>
<description>SQ5</description>
<bitOffset>0</bitOffset>
<bitWidth>5</bitWidth>
</field>
</fields>
</register>
<register>
<name>SQR3</name>
<displayName>SQR3</displayName>
<description>regular sequence register 3</description>
<addressOffset>0x38</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>SQ14</name>
<description>SQ14</description>
<bitOffset>24</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>SQ13</name>
<description>SQ13</description>
<bitOffset>18</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>SQ12</name>
<description>SQ12</description>
<bitOffset>12</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>SQ11</name>
<description>SQ11</description>
<bitOffset>6</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>SQ10</name>
<description>SQ10</description>
<bitOffset>0</bitOffset>
<bitWidth>5</bitWidth>
</field>
</fields>
</register>
<register>
<name>SQR4</name>
<displayName>SQR4</displayName>
<description>regular sequence register 4</description>
<addressOffset>0x3C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>SQ16</name>
<description>SQ16</description>
<bitOffset>6</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>SQ15</name>
<description>SQ15</description>
<bitOffset>0</bitOffset>
<bitWidth>5</bitWidth>
</field>
</fields>
</register>
<register>
<name>DR</name>
<displayName>DR</displayName>
<description>regular Data Register</description>
<addressOffset>0x40</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>regularDATA</name>
<description>regularDATA</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>JSQR</name>
<displayName>JSQR</displayName>
<description>injected sequence register</description>
<addressOffset>0x4C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>JSQ4</name>
<description>JSQ4</description>
<bitOffset>26</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>JSQ3</name>
<description>JSQ3</description>
<bitOffset>20</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>JSQ2</name>
<description>JSQ2</description>
<bitOffset>14</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>JSQ1</name>
<description>JSQ1</description>
<bitOffset>8</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>JEXTEN</name>
<description>JEXTEN</description>
<bitOffset>6</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>JEXTSEL</name>
<description>JEXTSEL</description>
<bitOffset>2</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>JL</name>
<description>JL</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
</fields>
</register>
<register>
<name>OFR1</name>
<displayName>OFR1</displayName>
<description>offset register 1</description>
<addressOffset>0x60</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>OFFSET1_EN</name>
<description>OFFSET1_EN</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OFFSET1_CH</name>
<description>OFFSET1_CH</description>
<bitOffset>26</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>OFFSET1</name>
<description>OFFSET1</description>
<bitOffset>0</bitOffset>
<bitWidth>12</bitWidth>
</field>
</fields>
</register>
<register>
<name>OFR2</name>
<displayName>OFR2</displayName>
<description>offset register 2</description>
<addressOffset>0x64</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>OFFSET2_EN</name>
<description>OFFSET2_EN</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OFFSET2_CH</name>
<description>OFFSET2_CH</description>
<bitOffset>26</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>OFFSET2</name>
<description>OFFSET2</description>
<bitOffset>0</bitOffset>
<bitWidth>12</bitWidth>
</field>
</fields>
</register>
<register>
<name>OFR3</name>
<displayName>OFR3</displayName>
<description>offset register 3</description>
<addressOffset>0x68</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>OFFSET3_EN</name>
<description>OFFSET3_EN</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OFFSET3_CH</name>
<description>OFFSET3_CH</description>
<bitOffset>26</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>OFFSET3</name>
<description>OFFSET3</description>
<bitOffset>0</bitOffset>
<bitWidth>12</bitWidth>
</field>
</fields>
</register>
<register>
<name>OFR4</name>
<displayName>OFR4</displayName>
<description>offset register 4</description>
<addressOffset>0x6C</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>OFFSET4_EN</name>
<description>OFFSET4_EN</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OFFSET4_CH</name>
<description>OFFSET4_CH</description>
<bitOffset>26</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>OFFSET4</name>
<description>OFFSET4</description>
<bitOffset>0</bitOffset>
<bitWidth>12</bitWidth>
</field>
</fields>
</register>
<register>
<name>JDR1</name>
<displayName>JDR1</displayName>
<description>injected data register 1</description>
<addressOffset>0x80</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>JDATA1</name>
<description>JDATA1</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>JDR2</name>
<displayName>JDR2</displayName>
<description>injected data register 2</description>
<addressOffset>0x84</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>JDATA2</name>
<description>JDATA2</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>JDR3</name>
<displayName>JDR3</displayName>
<description>injected data register 3</description>
<addressOffset>0x88</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>JDATA3</name>
<description>JDATA3</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>JDR4</name>
<displayName>JDR4</displayName>
<description>injected data register 4</description>
<addressOffset>0x8C</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>JDATA4</name>
<description>JDATA4</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
<register>
<name>AWD2CR</name>
<displayName>AWD2CR</displayName>
<description>Analog Watchdog 2 Configuration           Register</description>
<addressOffset>0xA0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>AWD2CH</name>
<description>AWD2CH</description>
<bitOffset>1</bitOffset>
<bitWidth>18</bitWidth>
</field>
</fields>
</register>
<register>
<name>AWD3CR</name>
<displayName>AWD3CR</displayName>
<description>Analog Watchdog 3 Configuration           Register</description>
<addressOffset>0xA4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>AWD3CH</name>
<description>AWD3CH</description>
<bitOffset>1</bitOffset>
<bitWidth>18</bitWidth>
</field>
</fields>
</register>
<register>
<name>DIFSEL</name>
<displayName>DIFSEL</displayName>
<description>Differential Mode Selection Register           2</description>
<addressOffset>0xB0</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>DIFSEL_1_15</name>
<description>Differential mode for channels 15 to               1</description>
<bitOffset>1</bitOffset>
<bitWidth>15</bitWidth>
<access>read-write</access>
</field>
<field>
<name>DIFSEL_16_18</name>
<description>Differential mode for channels 18 to               16</description>
<bitOffset>16</bitOffset>
<bitWidth>3</bitWidth>
<access>read-only</access>
</field>
</fields>
</register>
<register>
<name>CALFACT</name>
<displayName>CALFACT</displayName>
<description>Calibration Factors</description>
<addressOffset>0xB4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>CALFACT_D</name>
<description>CALFACT_D</description>
<bitOffset>16</bitOffset>
<bitWidth>7</bitWidth>
</field>
<field>
<name>CALFACT_S</name>
<description>CALFACT_S</description>
<bitOffset>0</bitOffset>
<bitWidth>7</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral derivedFrom="ADC1">
<name>ADC2</name>
<baseAddress>0x50000100</baseAddress>
<interrupt>
<name>ADC1_2</name>
<description>ADC1 and ADC2 global interrupt</description>
<value>18</value>
</interrupt>
</peripheral>
<peripheral derivedFrom="ADC1">
<name>ADC3</name>
<baseAddress>0x50000400</baseAddress>
<interrupt>
<name>ADC3</name>
<description>ADC3 global interrupt</description>
<value>47</value>
</interrupt>
</peripheral>
<peripheral derivedFrom="ADC1">
<name>ADC4</name>
<baseAddress>0x50000500</baseAddress>
<interrupt>
<name>ADC4</name>
<description>ADC4 global interrupt</description>
<value>61</value>
</interrupt>
</peripheral>
<peripheral>
<name>ADC1_2</name>
<description>Analog-to-Digital Converter</description>
<groupName>ADC</groupName>
<baseAddress>0x50000300</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0xD</size>
<usage>registers</usage>
</addressBlock>
<registers>
<register>
<name>CSR</name>
<displayName>CSR</displayName>
<description>ADC Common status register</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>ADDRDY_MST</name>
<description>ADDRDY_MST</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>EOSMP_MST</name>
<description>EOSMP_MST</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>EOC_MST</name>
<description>EOC_MST</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>EOS_MST</name>
<description>EOS_MST</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OVR_MST</name>
<description>OVR_MST</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>JEOC_MST</name>
<description>JEOC_MST</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>JEOS_MST</name>
<description>JEOS_MST</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>AWD1_MST</name>
<description>AWD1_MST</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>AWD2_MST</name>
<description>AWD2_MST</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>AWD3_MST</name>
<description>AWD3_MST</description>
<bitOffset>9</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>JQOVF_MST</name>
<description>JQOVF_MST</description>
<bitOffset>10</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ADRDY_SLV</name>
<description>ADRDY_SLV</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>EOSMP_SLV</name>
<description>EOSMP_SLV</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>EOC_SLV</name>
<description>End of regular conversion of the slave               ADC</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>EOS_SLV</name>
<description>End of regular sequence flag of the               slave ADC</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>OVR_SLV</name>
<description>Overrun flag of the slave               ADC</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>JEOC_SLV</name>
<description>End of injected conversion flag of the               slave ADC</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>JEOS_SLV</name>
<description>End of injected sequence flag of the               slave ADC</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>AWD1_SLV</name>
<description>Analog watchdog 1 flag of the slave               ADC</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>AWD2_SLV</name>
<description>Analog watchdog 2 flag of the slave               ADC</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>AWD3_SLV</name>
<description>Analog watchdog 3 flag of the slave               ADC</description>
<bitOffset>25</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>JQOVF_SLV</name>
<description>Injected Context Queue Overflow flag of               the slave ADC</description>
<bitOffset>26</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CCR</name>
<displayName>CCR</displayName>
<description>ADC common control register</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>MULT</name>
<description>Multi ADC mode selection</description>
<bitOffset>0</bitOffset>
<bitWidth>5</bitWidth>
</field>
<field>
<name>DELAY</name>
<description>Delay between 2 sampling               phases</description>
<bitOffset>8</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>DMACFG</name>
<description>DMA configuration (for multi-ADC               mode)</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>MDMA</name>
<description>Direct memory access mode for multi ADC               mode</description>
<bitOffset>14</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>CKMODE</name>
<description>ADC clock mode</description>
<bitOffset>16</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>VREFEN</name>
<description>VREFINT enable</description>
<bitOffset>22</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TSEN</name>
<description>Temperature sensor enable</description>
<bitOffset>23</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>VBATEN</name>
<description>VBAT enable</description>
<bitOffset>24</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>CDR</name>
<displayName>CDR</displayName>
<description>ADC common regular data register for dual           and triple modes</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<access>read-only</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>RDATA_SLV</name>
<description>Regular data of the slave               ADC</description>
<bitOffset>16</bitOffset>
<bitWidth>16</bitWidth>
</field>
<field>
<name>RDATA_MST</name>
<description>Regular data of the master               ADC</description>
<bitOffset>0</bitOffset>
<bitWidth>16</bitWidth>
</field>
</fields>
</register>
</registers>
</peripheral>
<peripheral derivedFrom="ADC1_2">
<name>ADC3_4</name>
<baseAddress>0x50000700</baseAddress>
</peripheral>
<peripheral>
<name>SYSCFG</name>
<description>System configuration controller</description>
<groupName>SYSCFG</groupName>
<baseAddress>0x40010000</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x19</size>
<usage>registers</usage>
</addressBlock>
<registers>
<register>
<name>CFGR1</name>
<displayName>CFGR1</displayName>
<description>configuration register 1</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>MEM_MODE</name>
<description>Memory mapping selection               bits</description>
<bitOffset>0</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>USB_IT_RMP</name>
<description>USB interrupt remap</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIM1_ITR_RMP</name>
<description>Timer 1 ITR3 selection</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>DAC_TRIG_RMP</name>
<description>DAC trigger remap (when TSEL =               001)</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ADC24_DMA_RMP</name>
<description>ADC24 DMA remapping bit</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIM16_DMA_RMP</name>
<description>TIM16 DMA request remapping               bit</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIM17_DMA_RMP</name>
<description>TIM17 DMA request remapping               bit</description>
<bitOffset>12</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIM6_DAC1_DMA_RMP</name>
<description>TIM6 and DAC1 DMA request remapping               bit</description>
<bitOffset>13</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>TIM7_DAC2_DMA_RMP</name>
<description>TIM7 and DAC2 DMA request remapping               bit</description>
<bitOffset>14</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>I2C_PB6_FM</name>
<description>Fast Mode Plus (FM+) driving capability               activation bits.</description>
<bitOffset>16</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>I2C_PB7_FM</name>
<description>Fast Mode Plus (FM+) driving capability               activation bits.</description>
<bitOffset>17</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>I2C_PB8_FM</name>
<description>Fast Mode Plus (FM+) driving capability               activation bits.</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>I2C_PB9_FM</name>
<description>Fast Mode Plus (FM+) driving capability               activation bits.</description>
<bitOffset>19</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>I2C1_FM</name>
<description>I2C1 Fast Mode Plus</description>
<bitOffset>20</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>I2C2_FM</name>
<description>I2C2 Fast Mode Plus</description>
<bitOffset>21</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>ENCODER_MODE</name>
<description>Encoder mode</description>
<bitOffset>22</bitOffset>
<bitWidth>2</bitWidth>
</field>
<field>
<name>FPU_IT</name>
<description>Interrupt enable bits from               FPU</description>
<bitOffset>26</bitOffset>
<bitWidth>6</bitWidth>
</field>
</fields>
</register>
<register>
<name>EXTICR1</name>
<displayName>EXTICR1</displayName>
<description>external interrupt configuration register           1</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>EXTI3</name>
<description>EXTI 3 configuration bits</description>
<bitOffset>12</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>EXTI2</name>
<description>EXTI 2 configuration bits</description>
<bitOffset>8</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>EXTI1</name>
<description>EXTI 1 configuration bits</description>
<bitOffset>4</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>EXTI0</name>
<description>EXTI 0 configuration bits</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>EXTICR2</name>
<displayName>EXTICR2</displayName>
<description>external interrupt configuration register           2</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>EXTI7</name>
<description>EXTI 7 configuration bits</description>
<bitOffset>12</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>EXTI6</name>
<description>EXTI 6 configuration bits</description>
<bitOffset>8</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>EXTI5</name>
<description>EXTI 5 configuration bits</description>
<bitOffset>4</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>EXTI4</name>
<description>EXTI 4 configuration bits</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>EXTICR3</name>
<displayName>EXTICR3</displayName>
<description>external interrupt configuration register           3</description>
<addressOffset>0x10</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>EXTI11</name>
<description>EXTI 11 configuration bits</description>
<bitOffset>12</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>EXTI10</name>
<description>EXTI 10 configuration bits</description>
<bitOffset>8</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>EXTI9</name>
<description>EXTI 9 configuration bits</description>
<bitOffset>4</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>EXTI8</name>
<description>EXTI 8 configuration bits</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>EXTICR4</name>
<displayName>EXTICR4</displayName>
<description>external interrupt configuration register           4</description>
<addressOffset>0x14</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>EXTI15</name>
<description>EXTI 15 configuration bits</description>
<bitOffset>12</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>EXTI14</name>
<description>EXTI 14 configuration bits</description>
<bitOffset>8</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>EXTI13</name>
<description>EXTI 13 configuration bits</description>
<bitOffset>4</bitOffset>
<bitWidth>4</bitWidth>
</field>
<field>
<name>EXTI12</name>
<description>EXTI 12 configuration bits</description>
<bitOffset>0</bitOffset>
<bitWidth>4</bitWidth>
</field>
</fields>
</register>
<register>
<name>CFGR2</name>
<displayName>CFGR2</displayName>
<description>configuration register 2</description>
<addressOffset>0x18</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>LOCUP_LOCK</name>
<description>Cortex-M0 LOCKUP bit enable               bit</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SRAM_PARITY_LOCK</name>
<description>SRAM parity lock bit</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PVD_LOCK</name>
<description>PVD lock enable bit</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>BYP_ADD_PAR</name>
<description>Bypass address bit 29 in parity               calculation</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>SRAM_PEF</name>
<description>SRAM parity flag</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
</field>
</fields>
</register>
<register>
<name>RCR</name>
<displayName>RCR</displayName>
<description>CCM SRAM protection register</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<access>read-write</access>
<resetValue>0x0000</resetValue>
<fields>
<field>
<name>PAGE0_WP</name>
<description>CCM SRAM page write protection               bit</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PAGE1_WP</name>
<description>CCM SRAM page write protection               bit</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PAGE2_WP</name>
<description>CCM SRAM page write protection               bit</description>
<bitOffset>2</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PAGE3_WP</name>
<description>CCM SRAM page write protection               bit</description>
<bitOffset>3</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PAGE4_WP</name>
<description>CCM SRAM page write protection               bit</description>
<bitOffset>4</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PAGE5_WP</name>
<description>CCM SRAM page write protection               bit</description>
<bitOffset>5</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PAGE6_WP</name>
<description>CCM SRAM page write protection               bit</description>
<bitOffset>6</bitOffset>
<bitWidth>1</bitWidth>
</field>
<field>
<name>PAGE7_WP</name>
<description>CCM SRAM page write protection               bit</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
</field>
            <field>
              <name>PAGE8_WP</name>
              <description>CCM SRAM page write protection
              bit</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PAGE9_WP</name>
              <description>CCM SRAM page write protection
              bit</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PAGE10_WP</name>
              <description>CCM SRAM page write protection
              bit</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PAGE11_WP</name>
              <description>CCM SRAM page write protection
              bit</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PAGE12_WP</name>
              <description>CCM SRAM page write protection
              bit</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PAGE13_WP</name>
              <description>CCM SRAM page write protection
              bit</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PAGE14_WP</name>
              <description>CCM SRAM page write protection
              bit</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PAGE15_WP</name>
              <description>CCM SRAM page write protection
              bit</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
</fields>
</register>
</registers>
</peripheral>
<peripheral>
<name>OPAMP</name>
<description>Operational amplifier</description>
<groupName>OPAMP</groupName>
<baseAddress>0x40010038</baseAddress>
<addressBlock>
<offset>0x0</offset>
<size>0x3C8</size>
<usage>registers</usage>
</addressBlock>
<registers>
<register>
<name>OPAMP1_CR</name>
<displayName>OPAMP1_CR</displayName>
<description>OPAMP1 control register</description>
<addressOffset>0x0</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>OPAMP1_EN</name>
<description>OPAMP1 enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>FORCE_VP</name>
<description>FORCE_VP</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>VP_SEL</name>
<description>OPAMP1 Non inverting input               selection</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>VM_SEL</name>
<description>OPAMP1 inverting input               selection</description>
<bitOffset>5</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TCM_EN</name>
<description>Timer controlled Mux mode               enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>VMS_SEL</name>
<description>OPAMP1 inverting input secondary               selection</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>VPS_SEL</name>
<description>OPAMP1 Non inverting input secondary               selection</description>
<bitOffset>9</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CALON</name>
<description>Calibration mode enable</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CALSEL</name>
<description>Calibration selection</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>PGA_GAIN</name>
<description>Gain in PGA mode</description>
<bitOffset>14</bitOffset>
<bitWidth>4</bitWidth>
<access>read-write</access>
</field>
<field>
<name>USER_TRIM</name>
<description>User trimming enable</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TRIMOFFSETP</name>
<description>Offset trimming value               (PMOS)</description>
<bitOffset>19</bitOffset>
<bitWidth>5</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TRIMOFFSETN</name>
<description>Offset trimming value               (NMOS)</description>
<bitOffset>24</bitOffset>
<bitWidth>5</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TSTREF</name>
<description>TSTREF</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>OUTCAL</name>
<description>OPAMP 1 ouput status flag</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>LOCK</name>
<description>OPAMP 1 lock</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
<register>
<name>OPAMP2_CR</name>
<displayName>OPAMP2_CR</displayName>
<description>OPAMP2 control register</description>
<addressOffset>0x4</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>OPAMP2EN</name>
<description>OPAMP2 enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>FORCE_VP</name>
<description>FORCE_VP</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>VP_SEL</name>
<description>OPAMP2 Non inverting input               selection</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>VM_SEL</name>
<description>OPAMP2 inverting input               selection</description>
<bitOffset>5</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TCM_EN</name>
<description>Timer controlled Mux mode               enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>VMS_SEL</name>
<description>OPAMP2 inverting input secondary               selection</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>VPS_SEL</name>
<description>OPAMP2 Non inverting input secondary               selection</description>
<bitOffset>9</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CALON</name>
<description>Calibration mode enable</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CAL_SEL</name>
<description>Calibration selection</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>PGA_GAIN</name>
<description>Gain in PGA mode</description>
<bitOffset>14</bitOffset>
<bitWidth>4</bitWidth>
<access>read-write</access>
</field>
<field>
<name>USER_TRIM</name>
<description>User trimming enable</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TRIMOFFSETP</name>
<description>Offset trimming value               (PMOS)</description>
<bitOffset>19</bitOffset>
<bitWidth>5</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TRIMOFFSETN</name>
<description>Offset trimming value               (NMOS)</description>
<bitOffset>24</bitOffset>
<bitWidth>5</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TSTREF</name>
<description>TSTREF</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>OUTCAL</name>
<description>OPAMP 2 ouput status flag</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>LOCK</name>
<description>OPAMP 2 lock</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
<register>
<name>OPAMP3_CR</name>
<displayName>OPAMP3_CR</displayName>
<description>OPAMP3 control register</description>
<addressOffset>0x8</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>OPAMP3EN</name>
<description>OPAMP3 enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>FORCE_VP</name>
<description>FORCE_VP</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>VP_SEL</name>
<description>OPAMP3 Non inverting input               selection</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>VM_SEL</name>
<description>OPAMP3 inverting input               selection</description>
<bitOffset>5</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TCM_EN</name>
<description>Timer controlled Mux mode               enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>VMS_SEL</name>
<description>OPAMP3 inverting input secondary               selection</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>VPS_SEL</name>
<description>OPAMP3 Non inverting input secondary               selection</description>
<bitOffset>9</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CALON</name>
<description>Calibration mode enable</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CALSEL</name>
<description>Calibration selection</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>PGA_GAIN</name>
<description>Gain in PGA mode</description>
<bitOffset>14</bitOffset>
<bitWidth>4</bitWidth>
<access>read-write</access>
</field>
<field>
<name>USER_TRIM</name>
<description>User trimming enable</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TRIMOFFSETP</name>
<description>Offset trimming value               (PMOS)</description>
<bitOffset>19</bitOffset>
<bitWidth>5</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TRIMOFFSETN</name>
<description>Offset trimming value               (NMOS)</description>
<bitOffset>24</bitOffset>
<bitWidth>5</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TSTREF</name>
<description>TSTREF</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>OUTCAL</name>
<description>OPAMP 3 ouput status flag</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>LOCK</name>
<description>OPAMP 3 lock</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
<register>
<name>OPAMP4_CR</name>
<displayName>OPAMP4_CR</displayName>
<description>OPAMP4 control register</description>
<addressOffset>0xC</addressOffset>
<size>0x20</size>
<resetValue>0x00000000</resetValue>
<fields>
<field>
<name>OPAMP4EN</name>
<description>OPAMP4 enable</description>
<bitOffset>0</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>FORCE_VP</name>
<description>FORCE_VP</description>
<bitOffset>1</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>VP_SEL</name>
<description>OPAMP4 Non inverting input               selection</description>
<bitOffset>2</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>VM_SEL</name>
<description>OPAMP4 inverting input               selection</description>
<bitOffset>5</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TCM_EN</name>
<description>Timer controlled Mux mode               enable</description>
<bitOffset>7</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>VMS_SEL</name>
<description>OPAMP4 inverting input secondary               selection</description>
<bitOffset>8</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>VPS_SEL</name>
<description>OPAMP4 Non inverting input secondary               selection</description>
<bitOffset>9</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CALON</name>
<description>Calibration mode enable</description>
<bitOffset>11</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>CALSEL</name>
<description>Calibration selection</description>
<bitOffset>12</bitOffset>
<bitWidth>2</bitWidth>
<access>read-write</access>
</field>
<field>
<name>PGA_GAIN</name>
<description>Gain in PGA mode</description>
<bitOffset>14</bitOffset>
<bitWidth>4</bitWidth>
<access>read-write</access>
</field>
<field>
<name>USER_TRIM</name>
<description>User trimming enable</description>
<bitOffset>18</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TRIMOFFSETP</name>
<description>Offset trimming value               (PMOS)</description>
<bitOffset>19</bitOffset>
<bitWidth>5</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TRIMOFFSETN</name>
<description>Offset trimming value               (NMOS)</description>
<bitOffset>24</bitOffset>
<bitWidth>5</bitWidth>
<access>read-write</access>
</field>
<field>
<name>TSTREF</name>
<description>TSTREF</description>
<bitOffset>29</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
<field>
<name>OUTCAL</name>
<description>OPAMP 4 ouput status flag</description>
<bitOffset>30</bitOffset>
<bitWidth>1</bitWidth>
<access>read-only</access>
</field>
<field>
<name>LOCK</name>
<description>OPAMP 4 lock</description>
<bitOffset>31</bitOffset>
<bitWidth>1</bitWidth>
<access>read-write</access>
</field>
</fields>
</register>
</registers>
</peripheral>
</peripherals>
</device>