<?xml version="1.0" encoding="utf-8" standalone="no"?>
<device schemaVersion="1.1"
xmlns:xs="http://www.w3.org/2001/XMLSchema-instance"
xs:noNamespaceSchemaLocation="CMSIS-SVD_Schema_1_1.xsd">
  <name>STM32F410xx</name>
  <version>1.0</version>
  <description>STM32F410xx</description>
  <!--Bus Interface Properties-->
  <!--Cortex-M4 is byte addressable-->
  <addressUnitBits>8</addressUnitBits>
  <!--the maximum data bit width accessible within a single transfer-->
  <width>32</width>
  <!--Register Default Properties-->
  <size>0x20</size>
  <resetValue>0x0</resetValue>
  <resetMask>0xFFFFFFFF</resetMask>
  <peripherals>
    <peripheral>
      <name>ADC_Common</name>
      <description>ADC common registers</description>
      <groupName>ADC</groupName>
      <baseAddress>0x40012300</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x5</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>CSR</name>
          <displayName>CSR</displayName>
          <description>ADC Common status register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OVR3</name>
              <description>Overrun flag of ADC3</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STRT3</name>
              <description>Regular channel Start flag of ADC
              3</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>JSTRT3</name>
              <description>Injected channel Start flag of ADC
              3</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>JEOC3</name>
              <description>Injected channel end of conversion of
              ADC 3</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EOC3</name>
              <description>End of conversion of ADC 3</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>AWD3</name>
              <description>Analog watchdog flag of ADC
              3</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OVR2</name>
              <description>Overrun flag of ADC 2</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STRT2</name>
              <description>Regular channel Start flag of ADC
              2</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>JSTRT2</name>
              <description>Injected channel Start flag of ADC
              2</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>JEOC2</name>
              <description>Injected channel end of conversion of
              ADC 2</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EOC2</name>
              <description>End of conversion of ADC 2</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>AWD2</name>
              <description>Analog watchdog flag of ADC
              2</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OVR1</name>
              <description>Overrun flag of ADC 1</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STRT1</name>
              <description>Regular channel Start flag of ADC
              1</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>JSTRT1</name>
              <description>Injected channel Start flag of ADC
              1</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>JEOC1</name>
              <description>Injected channel end of conversion of
              ADC 1</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EOC1</name>
              <description>End of conversion of ADC 1</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>AWD1</name>
              <description>Analog watchdog flag of ADC
              1</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR</name>
          <displayName>CCR</displayName>
          <description>ADC common control register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>TSVREFE</name>
              <description>Temperature sensor and VREFINT
              enable</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>VBATE</name>
              <description>VBAT enable</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ADCPRE</name>
              <description>ADC prescaler</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>DMA</name>
              <description>Direct memory access mode for multi ADC
              mode</description>
              <bitOffset>14</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>DDS</name>
              <description>DMA disable selection for multi-ADC
              mode</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DELAY</name>
              <description>Delay between 2 sampling
              phases</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>ADC1</name>
      <description>Analog-to-digital converter</description>
      <groupName>ADC</groupName>
      <baseAddress>0x40012000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>ADC</name>
        <description>ADC1 global interrupt</description>
        <value>18</value>
      </interrupt>
      <registers>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>status register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OVR</name>
              <description>Overrun</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STRT</name>
              <description>Regular channel start flag</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>JSTRT</name>
              <description>Injected channel start
              flag</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>JEOC</name>
              <description>Injected channel end of
              conversion</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EOC</name>
              <description>Regular channel end of
              conversion</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>AWD</name>
              <description>Analog watchdog flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>control register 1</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OVRIE</name>
              <description>Overrun interrupt enable</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RES</name>
              <description>Resolution</description>
              <bitOffset>24</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>AWDEN</name>
              <description>Analog watchdog enable on regular
              channels</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>JAWDEN</name>
              <description>Analog watchdog enable on injected
              channels</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DISCNUM</name>
              <description>Discontinuous mode channel
              count</description>
              <bitOffset>13</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>JDISCEN</name>
              <description>Discontinuous mode on injected
              channels</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DISCEN</name>
              <description>Discontinuous mode on regular
              channels</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>JAUTO</name>
              <description>Automatic injected group
              conversion</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>AWDSGL</name>
              <description>Enable the watchdog on a single channel
              in scan mode</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SCAN</name>
              <description>Scan mode</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>JEOCIE</name>
              <description>Interrupt enable for injected
              channels</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>AWDIE</name>
              <description>Analog watchdog interrupt
              enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EOCIE</name>
              <description>Interrupt enable for EOC</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>AWDCH</name>
              <description>Analog watchdog channel select
              bits</description>
              <bitOffset>0</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR2</name>
          <displayName>CR2</displayName>
          <description>control register 2</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SWSTART</name>
              <description>Start conversion of regular
              channels</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EXTEN</name>
              <description>External trigger enable for regular
              channels</description>
              <bitOffset>28</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>EXTSEL</name>
              <description>External event select for regular
              group</description>
              <bitOffset>24</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>JSWSTART</name>
              <description>Start conversion of injected
              channels</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>JEXTEN</name>
              <description>External trigger enable for injected
              channels</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>JEXTSEL</name>
              <description>External event select for injected
              group</description>
              <bitOffset>16</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>ALIGN</name>
              <description>Data alignment</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EOCS</name>
              <description>End of conversion
              selection</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DDS</name>
              <description>DMA disable selection (for single ADC
              mode)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMA</name>
              <description>Direct memory access mode (for single
              ADC mode)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CONT</name>
              <description>Continuous conversion</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ADON</name>
              <description>A/D Converter ON / OFF</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SMPR1</name>
          <displayName>SMPR1</displayName>
          <description>sample time register 1</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SMPx_x</name>
              <description>Sample time bits</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SMPR2</name>
          <displayName>SMPR2</displayName>
          <description>sample time register 2</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SMPx_x</name>
              <description>Sample time bits</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>JOFR1</name>
          <displayName>JOFR1</displayName>
          <description>injected channel data offset register
          x</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>JOFFSET1</name>
              <description>Data offset for injected channel
              x</description>
              <bitOffset>0</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>JOFR2</name>
          <displayName>JOFR2</displayName>
          <description>injected channel data offset register
          x</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>JOFFSET2</name>
              <description>Data offset for injected channel
              x</description>
              <bitOffset>0</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>JOFR3</name>
          <displayName>JOFR3</displayName>
          <description>injected channel data offset register
          x</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>JOFFSET3</name>
              <description>Data offset for injected channel
              x</description>
              <bitOffset>0</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>JOFR4</name>
          <displayName>JOFR4</displayName>
          <description>injected channel data offset register
          x</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>JOFFSET4</name>
              <description>Data offset for injected channel
              x</description>
              <bitOffset>0</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>HTR</name>
          <displayName>HTR</displayName>
          <description>watchdog higher threshold
          register</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000FFF</resetValue>
          <fields>
            <field>
              <name>HT</name>
              <description>Analog watchdog higher
              threshold</description>
              <bitOffset>0</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>LTR</name>
          <displayName>LTR</displayName>
          <description>watchdog lower threshold
          register</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>LT</name>
              <description>Analog watchdog lower
              threshold</description>
              <bitOffset>0</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SQR1</name>
          <displayName>SQR1</displayName>
          <description>regular sequence register 1</description>
          <addressOffset>0x2C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>L</name>
              <description>Regular channel sequence
              length</description>
              <bitOffset>20</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>SQ16</name>
              <description>16th conversion in regular
              sequence</description>
              <bitOffset>15</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
            <field>
              <name>SQ15</name>
              <description>15th conversion in regular
              sequence</description>
              <bitOffset>10</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
            <field>
              <name>SQ14</name>
              <description>14th conversion in regular
              sequence</description>
              <bitOffset>5</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
            <field>
              <name>SQ13</name>
              <description>13th conversion in regular
              sequence</description>
              <bitOffset>0</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SQR2</name>
          <displayName>SQR2</displayName>
          <description>regular sequence register 2</description>
          <addressOffset>0x30</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SQ12</name>
              <description>12th conversion in regular
              sequence</description>
              <bitOffset>25</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
            <field>
              <name>SQ11</name>
              <description>11th conversion in regular
              sequence</description>
              <bitOffset>20</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
            <field>
              <name>SQ10</name>
              <description>10th conversion in regular
              sequence</description>
              <bitOffset>15</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
            <field>
              <name>SQ9</name>
              <description>9th conversion in regular
              sequence</description>
              <bitOffset>10</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
            <field>
              <name>SQ8</name>
              <description>8th conversion in regular
              sequence</description>
              <bitOffset>5</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
            <field>
              <name>SQ7</name>
              <description>7th conversion in regular
              sequence</description>
              <bitOffset>0</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SQR3</name>
          <displayName>SQR3</displayName>
          <description>regular sequence register 3</description>
          <addressOffset>0x34</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SQ6</name>
              <description>6th conversion in regular
              sequence</description>
              <bitOffset>25</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
            <field>
              <name>SQ5</name>
              <description>5th conversion in regular
              sequence</description>
              <bitOffset>20</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
            <field>
              <name>SQ4</name>
              <description>4th conversion in regular
              sequence</description>
              <bitOffset>15</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
            <field>
              <name>SQ3</name>
              <description>3rd conversion in regular
              sequence</description>
              <bitOffset>10</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
            <field>
              <name>SQ2</name>
              <description>2nd conversion in regular
              sequence</description>
              <bitOffset>5</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
            <field>
              <name>SQ1</name>
              <description>1st conversion in regular
              sequence</description>
              <bitOffset>0</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>JSQR</name>
          <displayName>JSQR</displayName>
          <description>injected sequence register</description>
          <addressOffset>0x38</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>JL</name>
              <description>Injected sequence length</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>JSQ4</name>
              <description>4th conversion in injected
              sequence</description>
              <bitOffset>15</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
            <field>
              <name>JSQ3</name>
              <description>3rd conversion in injected
              sequence</description>
              <bitOffset>10</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
            <field>
              <name>JSQ2</name>
              <description>2nd conversion in injected
              sequence</description>
              <bitOffset>5</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
            <field>
              <name>JSQ1</name>
              <description>1st conversion in injected
              sequence</description>
              <bitOffset>0</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>JDR1</name>
          <displayName>JDR1</displayName>
          <description>injected data register x</description>
          <addressOffset>0x3C</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>JDATA</name>
              <description>Injected data</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>JDR2</name>
          <displayName>JDR2</displayName>
          <description>injected data register x</description>
          <addressOffset>0x40</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>JDATA</name>
              <description>Injected data</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>JDR3</name>
          <displayName>JDR3</displayName>
          <description>injected data register x</description>
          <addressOffset>0x44</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>JDATA</name>
              <description>Injected data</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>JDR4</name>
          <displayName>JDR4</displayName>
          <description>injected data register x</description>
          <addressOffset>0x48</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>JDATA</name>
              <description>Injected data</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DR</name>
          <displayName>DR</displayName>
          <description>regular data register</description>
          <addressOffset>0x4C</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DATA</name>
              <description>Regular data</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>CRC</name>
      <description>Cryptographic processor</description>
      <groupName>CRC</groupName>
      <baseAddress>0x40023000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>DR</name>
          <displayName>DR</displayName>
          <description>Data register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0xFFFFFFFF</resetValue>
          <fields>
            <field>
              <name>DR</name>
              <description>Data Register</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IDR</name>
          <displayName>IDR</displayName>
          <description>Independent Data register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IDR</name>
              <description>Independent Data register</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>Control register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CR</name>
              <description>Control regidter</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>DBG</name>
      <description>Debug support</description>
      <groupName>DBG</groupName>
      <baseAddress>0xE0042000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>DBGMCU_IDCODE</name>
          <displayName>DBGMCU_IDCODE</displayName>
          <description>IDCODE</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x10006411</resetValue>
          <fields>
            <field>
              <name>DEV_ID</name>
              <description>DEV_ID</description>
              <bitOffset>0</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
            <field>
              <name>REV_ID</name>
              <description>REV_ID</description>
              <bitOffset>16</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DBGMCU_CR</name>
          <displayName>DBGMCU_CR</displayName>
          <description>Control Register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DBG_SLEEP</name>
              <description>DBG_SLEEP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBG_STOP</name>
              <description>DBG_STOP</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBG_STANDBY</name>
              <description>DBG_STANDBY</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TRACE_IOEN</name>
              <description>TRACE_IOEN</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TRACE_MODE</name>
              <description>TRACE_MODE</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DBGMCU_APB1_FZ</name>
          <displayName>DBGMCU_APB1_FZ</displayName>
          <description>Debug MCU APB1 Freeze registe</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DBG_TIM2_STOP</name>
              <description>DBG_TIM2_STOP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBG_TIM3_STOP</name>
              <description>DBG_TIM3 _STOP</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBG_TIM4_STOP</name>
              <description>DBG_TIM4_STOP</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBG_TIM5_STOP</name>
              <description>DBG_TIM5_STOP</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBG_RTC_Stop</name>
              <description>RTC stopped when Core is
              halted</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBG_WWDG_STOP</name>
              <description>DBG_WWDG_STOP</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBG_IWDEG_STOP</name>
              <description>DBG_IWDEG_STOP</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBG_I2C1_SMBUS_TIMEOUT</name>
              <description>DBG_J2C1_SMBUS_TIMEOUT</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBG_I2C2_SMBUS_TIMEOUT</name>
              <description>DBG_J2C2_SMBUS_TIMEOUT</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBG_I2C3SMBUS_TIMEOUT</name>
              <description>DBG_J2C3SMBUS_TIMEOUT</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DBGMCU_APB2_FZ</name>
          <displayName>DBGMCU_APB2_FZ</displayName>
          <description>Debug MCU APB2 Freeze registe</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DBG_TIM1_STOP</name>
              <description>TIM1 counter stopped when core is
              halted</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBG_TIM9_STOP</name>
              <description>TIM9 counter stopped when core is
              halted</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBG_TIM10_STOP</name>
              <description>TIM10 counter stopped when core is
              halted</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBG_TIM11_STOP</name>
              <description>TIM11 counter stopped when core is
              halted</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>EXTI</name>
      <description>External interrupt/event
      controller</description>
      <groupName>EXTI</groupName>
      <baseAddress>0x40013C00</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>TAMP_STAMP</name>
        <description>Tamper and TimeStamp interrupts through the
        EXTI line</description>
        <value>2</value>
      </interrupt>
      <interrupt>
        <name>EXTI0</name>
        <description>EXTI Line0 interrupt</description>
        <value>6</value>
      </interrupt>
      <interrupt>
        <name>EXTI1</name>
        <description>EXTI Line1 interrupt</description>
        <value>7</value>
      </interrupt>
      <interrupt>
        <name>EXTI2</name>
        <description>EXTI Line2 interrupt</description>
        <value>8</value>
      </interrupt>
      <interrupt>
        <name>EXTI3</name>
        <description>EXTI Line3 interrupt</description>
        <value>9</value>
      </interrupt>
      <interrupt>
        <name>EXTI4</name>
        <description>EXTI Line4 interrupt</description>
        <value>10</value>
      </interrupt>
      <interrupt>
        <name>EXTI9_5</name>
        <description>EXTI Line[9:5] interrupts</description>
        <value>23</value>
      </interrupt>
      <interrupt>
        <name>EXTI15_10</name>
        <description>EXTI Line[15:10] interrupts</description>
        <value>40</value>
      </interrupt>
      <registers>
        <register>
          <name>IMR</name>
          <displayName>IMR</displayName>
          <description>Interrupt mask register
          (EXTI_IMR)</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MR0</name>
              <description>Interrupt Mask on line 0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR1</name>
              <description>Interrupt Mask on line 1</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR2</name>
              <description>Interrupt Mask on line 2</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR3</name>
              <description>Interrupt Mask on line 3</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR4</name>
              <description>Interrupt Mask on line 4</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR5</name>
              <description>Interrupt Mask on line 5</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR6</name>
              <description>Interrupt Mask on line 6</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR7</name>
              <description>Interrupt Mask on line 7</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR8</name>
              <description>Interrupt Mask on line 8</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR9</name>
              <description>Interrupt Mask on line 9</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR10</name>
              <description>Interrupt Mask on line 10</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR11</name>
              <description>Interrupt Mask on line 11</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR12</name>
              <description>Interrupt Mask on line 12</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR13</name>
              <description>Interrupt Mask on line 13</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR14</name>
              <description>Interrupt Mask on line 14</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR15</name>
              <description>Interrupt Mask on line 15</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR16</name>
              <description>Interrupt Mask on line 16</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR17</name>
              <description>Interrupt Mask on line 17</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR18</name>
              <description>Interrupt Mask on line 18</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR19</name>
              <description>Interrupt Mask on line 19</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR20</name>
              <description>Interrupt Mask on line 20</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR21</name>
              <description>Interrupt Mask on line 21</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR22</name>
              <description>Interrupt Mask on line 22</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EMR</name>
          <displayName>EMR</displayName>
          <description>Event mask register (EXTI_EMR)</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MR0</name>
              <description>Event Mask on line 0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR1</name>
              <description>Event Mask on line 1</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR2</name>
              <description>Event Mask on line 2</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR3</name>
              <description>Event Mask on line 3</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR4</name>
              <description>Event Mask on line 4</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR5</name>
              <description>Event Mask on line 5</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR6</name>
              <description>Event Mask on line 6</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR7</name>
              <description>Event Mask on line 7</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR8</name>
              <description>Event Mask on line 8</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR9</name>
              <description>Event Mask on line 9</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR10</name>
              <description>Event Mask on line 10</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR11</name>
              <description>Event Mask on line 11</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR12</name>
              <description>Event Mask on line 12</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR13</name>
              <description>Event Mask on line 13</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR14</name>
              <description>Event Mask on line 14</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR15</name>
              <description>Event Mask on line 15</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR16</name>
              <description>Event Mask on line 16</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR17</name>
              <description>Event Mask on line 17</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR18</name>
              <description>Event Mask on line 18</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR19</name>
              <description>Event Mask on line 19</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR20</name>
              <description>Event Mask on line 20</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR21</name>
              <description>Event Mask on line 21</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MR22</name>
              <description>Event Mask on line 22</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>RTSR</name>
          <displayName>RTSR</displayName>
          <description>Rising Trigger selection register
          (EXTI_RTSR)</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>TR0</name>
              <description>Rising trigger event configuration of
              line 0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR1</name>
              <description>Rising trigger event configuration of
              line 1</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR2</name>
              <description>Rising trigger event configuration of
              line 2</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR3</name>
              <description>Rising trigger event configuration of
              line 3</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR4</name>
              <description>Rising trigger event configuration of
              line 4</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR5</name>
              <description>Rising trigger event configuration of
              line 5</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR6</name>
              <description>Rising trigger event configuration of
              line 6</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR7</name>
              <description>Rising trigger event configuration of
              line 7</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR8</name>
              <description>Rising trigger event configuration of
              line 8</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR9</name>
              <description>Rising trigger event configuration of
              line 9</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR10</name>
              <description>Rising trigger event configuration of
              line 10</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR11</name>
              <description>Rising trigger event configuration of
              line 11</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR12</name>
              <description>Rising trigger event configuration of
              line 12</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR13</name>
              <description>Rising trigger event configuration of
              line 13</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR14</name>
              <description>Rising trigger event configuration of
              line 14</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR15</name>
              <description>Rising trigger event configuration of
              line 15</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR16</name>
              <description>Rising trigger event configuration of
              line 16</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR17</name>
              <description>Rising trigger event configuration of
              line 17</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR18</name>
              <description>Rising trigger event configuration of
              line 18</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR19</name>
              <description>Rising trigger event configuration of
              line 19</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR20</name>
              <description>Rising trigger event configuration of
              line 20</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR21</name>
              <description>Rising trigger event configuration of
              line 21</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR22</name>
              <description>Rising trigger event configuration of
              line 22</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>FTSR</name>
          <displayName>FTSR</displayName>
          <description>Falling Trigger selection register
          (EXTI_FTSR)</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>TR0</name>
              <description>Falling trigger event configuration of
              line 0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR1</name>
              <description>Falling trigger event configuration of
              line 1</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR2</name>
              <description>Falling trigger event configuration of
              line 2</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR3</name>
              <description>Falling trigger event configuration of
              line 3</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR4</name>
              <description>Falling trigger event configuration of
              line 4</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR5</name>
              <description>Falling trigger event configuration of
              line 5</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR6</name>
              <description>Falling trigger event configuration of
              line 6</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR7</name>
              <description>Falling trigger event configuration of
              line 7</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR8</name>
              <description>Falling trigger event configuration of
              line 8</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR9</name>
              <description>Falling trigger event configuration of
              line 9</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR10</name>
              <description>Falling trigger event configuration of
              line 10</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR11</name>
              <description>Falling trigger event configuration of
              line 11</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR12</name>
              <description>Falling trigger event configuration of
              line 12</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR13</name>
              <description>Falling trigger event configuration of
              line 13</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR14</name>
              <description>Falling trigger event configuration of
              line 14</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR15</name>
              <description>Falling trigger event configuration of
              line 15</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR16</name>
              <description>Falling trigger event configuration of
              line 16</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR17</name>
              <description>Falling trigger event configuration of
              line 17</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR18</name>
              <description>Falling trigger event configuration of
              line 18</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR19</name>
              <description>Falling trigger event configuration of
              line 19</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR20</name>
              <description>Falling trigger event configuration of
              line 20</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR21</name>
              <description>Falling trigger event configuration of
              line 21</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TR22</name>
              <description>Falling trigger event configuration of
              line 22</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SWIER</name>
          <displayName>SWIER</displayName>
          <description>Software interrupt event register
          (EXTI_SWIER)</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SWIER0</name>
              <description>Software Interrupt on line
              0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER1</name>
              <description>Software Interrupt on line
              1</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER2</name>
              <description>Software Interrupt on line
              2</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER3</name>
              <description>Software Interrupt on line
              3</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER4</name>
              <description>Software Interrupt on line
              4</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER5</name>
              <description>Software Interrupt on line
              5</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER6</name>
              <description>Software Interrupt on line
              6</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER7</name>
              <description>Software Interrupt on line
              7</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER8</name>
              <description>Software Interrupt on line
              8</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER9</name>
              <description>Software Interrupt on line
              9</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER10</name>
              <description>Software Interrupt on line
              10</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER11</name>
              <description>Software Interrupt on line
              11</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER12</name>
              <description>Software Interrupt on line
              12</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER13</name>
              <description>Software Interrupt on line
              13</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER14</name>
              <description>Software Interrupt on line
              14</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER15</name>
              <description>Software Interrupt on line
              15</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER16</name>
              <description>Software Interrupt on line
              16</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER17</name>
              <description>Software Interrupt on line
              17</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER18</name>
              <description>Software Interrupt on line
              18</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER19</name>
              <description>Software Interrupt on line
              19</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER20</name>
              <description>Software Interrupt on line
              20</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER21</name>
              <description>Software Interrupt on line
              21</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWIER22</name>
              <description>Software Interrupt on line
              22</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>PR</name>
          <displayName>PR</displayName>
          <description>Pending register (EXTI_PR)</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PR0</name>
              <description>Pending bit 0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR1</name>
              <description>Pending bit 1</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR2</name>
              <description>Pending bit 2</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR3</name>
              <description>Pending bit 3</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR4</name>
              <description>Pending bit 4</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR5</name>
              <description>Pending bit 5</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR6</name>
              <description>Pending bit 6</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR7</name>
              <description>Pending bit 7</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR8</name>
              <description>Pending bit 8</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR9</name>
              <description>Pending bit 9</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR10</name>
              <description>Pending bit 10</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR11</name>
              <description>Pending bit 11</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR12</name>
              <description>Pending bit 12</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR13</name>
              <description>Pending bit 13</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR14</name>
              <description>Pending bit 14</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR15</name>
              <description>Pending bit 15</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR16</name>
              <description>Pending bit 16</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR17</name>
              <description>Pending bit 17</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR18</name>
              <description>Pending bit 18</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR19</name>
              <description>Pending bit 19</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR20</name>
              <description>Pending bit 20</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR21</name>
              <description>Pending bit 21</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PR22</name>
              <description>Pending bit 22</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>FLASH</name>
      <description>FLASH</description>
      <groupName>FLASH</groupName>
      <baseAddress>0x40023C00</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>FLASH</name>
        <description>FLASH global interrupt</description>
        <value>4</value>
      </interrupt>
      <registers>
        <register>
          <name>ACR</name>
          <displayName>ACR</displayName>
          <description>Flash access control register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>LATENCY</name>
              <description>Latency</description>
              <bitOffset>0</bitOffset>
              <bitWidth>3</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>PRFTEN</name>
              <description>Prefetch enable</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>ICEN</name>
              <description>Instruction cache enable</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>DCEN</name>
              <description>Data cache enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>ICRST</name>
              <description>Instruction cache reset</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
              <access>write-only</access>
            </field>
            <field>
              <name>DCRST</name>
              <description>Data cache reset</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
        <register>
          <name>KEYR</name>
          <displayName>KEYR</displayName>
          <description>Flash key register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>KEY</name>
              <description>FPEC key</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OPTKEYR</name>
          <displayName>OPTKEYR</displayName>
          <description>Flash option key register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OPTKEY</name>
              <description>Option byte key</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>Status register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>EOP</name>
              <description>End of operation</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>OPERR</name>
              <description>Operation error</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>WRPERR</name>
              <description>Write protection error</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>PGAERR</name>
              <description>Programming alignment
              error</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>PGPERR</name>
              <description>Programming parallelism
              error</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>PGSERR</name>
              <description>Programming sequence error</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>BSY</name>
              <description>Busy</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
          </fields>
        </register>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>Control register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x80000000</resetValue>
          <fields>
            <field>
              <name>PG</name>
              <description>Programming</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SER</name>
              <description>Sector Erase</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MER</name>
              <description>Mass Erase</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SNB</name>
              <description>Sector number</description>
              <bitOffset>3</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>PSIZE</name>
              <description>Program size</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>STRT</name>
              <description>Start</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EOPIE</name>
              <description>End of operation interrupt
              enable</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ERRIE</name>
              <description>Error interrupt enable</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LOCK</name>
              <description>Lock</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OPTCR</name>
          <displayName>OPTCR</displayName>
          <description>Flash option control register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x7FFFAAED</resetValue>
          <fields>
            <field>
              <name>OPTLOCK</name>
              <description>Option lock</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OPTSTRT</name>
              <description>Option start</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BOR_LEV</name>
              <description>BOR reset Level</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>WDG_SW</name>
              <description>WDG_SW User option bytes</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>nRST_STOP</name>
              <description>nRST_STOP User option
              bytes</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>nRST_STDBY</name>
              <description>nRST_STDBY User option
              bytes</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RDP</name>
              <description>Read protect</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>nWRP</name>
              <description>Not write protect</description>
              <bitOffset>16</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
            <field>
              <name>SPRMOD</name>
              <description>SPRMOD</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>IWDG</name>
      <description>Independent watchdog</description>
      <groupName>IWDG</groupName>
      <baseAddress>0x40003000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>KR</name>
          <displayName>KR</displayName>
          <description>Key register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>KEY</name>
              <description>Key value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>PR</name>
          <displayName>PR</displayName>
          <description>Prescaler register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PR</name>
              <description>Prescaler divider</description>
              <bitOffset>0</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>RLR</name>
          <displayName>RLR</displayName>
          <description>Reload register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000FFF</resetValue>
          <fields>
            <field>
              <name>RL</name>
              <description>Watchdog counter reload
              value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>Status register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>RVU</name>
              <description>Watchdog counter reload value
              update</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PVU</name>
              <description>Watchdog prescaler value
              update</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>PWR</name>
      <description>Power control</description>
      <groupName>PWR</groupName>
      <baseAddress>0x40007000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>PVD</name>
        <description>PVD through EXTI line detection
        interrupt</description>
        <value>1</value>
      </interrupt>
      <registers>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>power control register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>VOS</name>
              <description>Regulator voltage scaling output
              selection</description>
              <bitOffset>14</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>ADCDC1</name>
              <description>ADCDC1</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>FPDS</name>
              <description>Flash power down in Stop
              mode</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBP</name>
              <description>Disable backup domain write
              protection</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLS</name>
              <description>PVD level selection</description>
              <bitOffset>5</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>PVDE</name>
              <description>Power voltage detector
              enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CSBF</name>
              <description>Clear standby flag</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CWUF</name>
              <description>Clear wakeup flag</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PDDS</name>
              <description>Power down deepsleep</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LPDS</name>
              <description>Low-power deep sleep</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CSR</name>
          <displayName>CSR</displayName>
          <description>power control/status register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>WUF</name>
              <description>Wakeup flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>SBF</name>
              <description>Standby flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>PVDO</name>
              <description>PVD output</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>BRR</name>
              <description>Backup regulator ready</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>EWUP3</name>
              <description>Enable WKUP3 pin</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>EWUP2</name>
              <description>Enable WKUP2 pin</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>EWUP1</name>
              <description>Enable WKUP1 pin</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>BRE</name>
              <description>Backup regulator enable</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>VOSRDY</name>
              <description>Regulator voltage scaling output
              selection ready bit</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>RCC</name>
      <description>Reset and clock control</description>
      <groupName>RCC</groupName>
      <baseAddress>0x40023800</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>RCC</name>
        <description>RCC global interrupt</description>
        <value>5</value>
      </interrupt>
      <registers>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>clock control register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000083</resetValue>
          <fields>
            <field>
              <name>PLLRDY</name>
              <description>Main PLL (PLL) clock ready
              flag</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>PLLON</name>
              <description>Main PLL (PLL) enable</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>CSSON</name>
              <description>Clock security system
              enable</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>HSEBYP</name>
              <description>HSE clock bypass</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>HSERDY</name>
              <description>HSE clock ready flag</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>HSEON</name>
              <description>HSE clock enable</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>HSICAL</name>
              <description>Internal high-speed clock
              calibration</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>HSITRIM</name>
              <description>Internal high-speed clock
              trimming</description>
              <bitOffset>3</bitOffset>
              <bitWidth>5</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>HSIRDY</name>
              <description>Internal high-speed clock ready
              flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>HSION</name>
              <description>Internal high-speed clock
              enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
        <register>
          <name>PLLCFGR</name>
          <displayName>PLLCFGR</displayName>
          <description>PLL configuration register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x7F003010</resetValue>
          <fields>
            <field>
              <name>PLLM0</name>
              <description>Division factor for the main PLL (PLL)
              and audio PLL (PLLI2S) input clock</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLM1</name>
              <description>Division factor for the main PLL (PLL)
              and audio PLL (PLLI2S) input clock</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLM2</name>
              <description>Division factor for the main PLL (PLL)
              and audio PLL (PLLI2S) input clock</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLM3</name>
              <description>Division factor for the main PLL (PLL)
              and audio PLL (PLLI2S) input clock</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLM4</name>
              <description>Division factor for the main PLL (PLL)
              and audio PLL (PLLI2S) input clock</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLM5</name>
              <description>Division factor for the main PLL (PLL)
              and audio PLL (PLLI2S) input clock</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLN0</name>
              <description>Main PLL (PLL) multiplication factor for
              VCO</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLN1</name>
              <description>Main PLL (PLL) multiplication factor for
              VCO</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLN2</name>
              <description>Main PLL (PLL) multiplication factor for
              VCO</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLN3</name>
              <description>Main PLL (PLL) multiplication factor for
              VCO</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLN4</name>
              <description>Main PLL (PLL) multiplication factor for
              VCO</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLN5</name>
              <description>Main PLL (PLL) multiplication factor for
              VCO</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLN6</name>
              <description>Main PLL (PLL) multiplication factor for
              VCO</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLN7</name>
              <description>Main PLL (PLL) multiplication factor for
              VCO</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLN8</name>
              <description>Main PLL (PLL) multiplication factor for
              VCO</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLP0</name>
              <description>Main PLL (PLL) division factor for main
              system clock</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLP1</name>
              <description>Main PLL (PLL) division factor for main
              system clock</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLSRC</name>
              <description>Main PLL(PLL) and audio PLL (PLLI2S)
              entry clock source</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLQ0</name>
              <description>Main PLL (PLL) division factor for USB
              OTG FS, SDIO and random number generator
              clocks</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLQ1</name>
              <description>Main PLL (PLL) division factor for USB
              OTG FS, SDIO and random number generator
              clocks</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLQ2</name>
              <description>Main PLL (PLL) division factor for USB
              OTG FS, SDIO and random number generator
              clocks</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLQ3</name>
              <description>Main PLL (PLL) division factor for USB
              OTG FS, SDIO and random number generator
              clocks</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLR1</name>
              <description>PLLR1</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLR2</name>
              <description>PLLR2</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PLLR3</name>
              <description>PLLR3</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CFGR</name>
          <displayName>CFGR</displayName>
          <description>clock configuration register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SW0</name>
              <description>System clock switch</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>SW1</name>
              <description>System clock switch</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>SWS0</name>
              <description>System clock switch status</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>SWS1</name>
              <description>System clock switch status</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>HPRE</name>
              <description>AHB prescaler</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>MCO1EN</name>
              <description>MCO output enable</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>MCO2EN</name>
              <description>MCO output enable</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>PPRE1</name>
              <description>APB Low speed prescaler
              (APB1)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>3</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>PPRE2</name>
              <description>APB high-speed prescaler
              (APB2)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>3</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>RTCPRE</name>
              <description>HSE division factor for RTC
              clock</description>
              <bitOffset>16</bitOffset>
              <bitWidth>5</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>MCO1</name>
              <description>Microcontroller clock output
              1</description>
              <bitOffset>21</bitOffset>
              <bitWidth>2</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>MCO1PRE</name>
              <description>MCO1 prescaler</description>
              <bitOffset>24</bitOffset>
              <bitWidth>3</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>MCO2PRE</name>
              <description>MCO2 prescaler</description>
              <bitOffset>27</bitOffset>
              <bitWidth>3</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>MCO2</name>
              <description>Microcontroller clock output
              2</description>
              <bitOffset>30</bitOffset>
              <bitWidth>2</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
        <register>
          <name>CIR</name>
          <displayName>CIR</displayName>
          <description>clock interrupt register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CSSC</name>
              <description>Clock security system interrupt
              clear</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
              <access>write-only</access>
            </field>
            <field>
              <name>PLLI2SRDYC</name>
              <description>PLLI2S ready interrupt
              clear</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
              <access>write-only</access>
            </field>
            <field>
              <name>PLLRDYC</name>
              <description>Main PLL(PLL) ready interrupt
              clear</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
              <access>write-only</access>
            </field>
            <field>
              <name>HSERDYC</name>
              <description>HSE ready interrupt clear</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
              <access>write-only</access>
            </field>
            <field>
              <name>HSIRDYC</name>
              <description>HSI ready interrupt clear</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
              <access>write-only</access>
            </field>
            <field>
              <name>LSERDYC</name>
              <description>LSE ready interrupt clear</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
              <access>write-only</access>
            </field>
            <field>
              <name>LSIRDYC</name>
              <description>LSI ready interrupt clear</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
              <access>write-only</access>
            </field>
            <field>
              <name>PLLRDYIE</name>
              <description>Main PLL (PLL) ready interrupt
              enable</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>HSERDYIE</name>
              <description>HSE ready interrupt enable</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>HSIRDYIE</name>
              <description>HSI ready interrupt enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>LSERDYIE</name>
              <description>LSE ready interrupt enable</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>LSIRDYIE</name>
              <description>LSI ready interrupt enable</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>CSSF</name>
              <description>Clock security system interrupt
              flag</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>PLLRDYF</name>
              <description>Main PLL (PLL) ready interrupt
              flag</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>HSERDYF</name>
              <description>HSE ready interrupt flag</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>HSIRDYF</name>
              <description>HSI ready interrupt flag</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>LSERDYF</name>
              <description>LSE ready interrupt flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>LSIRDYF</name>
              <description>LSI ready interrupt flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
          </fields>
        </register>
        <register>
          <name>AHB1RSTR</name>
          <displayName>AHB1RSTR</displayName>
          <description>AHB1 peripheral reset register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>GPIOARST</name>
              <description>IO port A reset</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>GPIOBRST</name>
              <description>IO port B reset</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>GPIOCRST</name>
              <description>IO port C reset</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>GPIOHRST</name>
              <description>IO port H reset</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CRCRST</name>
              <description>CRC reset</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMA1RST</name>
              <description>DMA2 reset</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMA2RST</name>
              <description>DMA2 reset</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RNGRST</name>
              <description>RNGRST</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>APB1RSTR</name>
          <displayName>APB1RSTR</displayName>
          <description>APB1 peripheral reset register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>TIM5RST</name>
              <description>TIM5 reset</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIM6RST</name>
              <description>TIM6 reset</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LPTIM1RST</name>
              <description>LPTIM1 reset</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WWDGRST</name>
              <description>Window watchdog reset</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SPI2RST</name>
              <description>SPI 2 reset</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UART2RST</name>
              <description>USART 2 reset</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2C1RST</name>
              <description>I2C 1 reset</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2C2RST</name>
              <description>I2C 2 reset</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2C4RST</name>
              <description>I2C4 reset</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PWRRST</name>
              <description>Power interface reset</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DACRST</name>
              <description>DAC reset</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>APB2RSTR</name>
          <displayName>APB2RSTR</displayName>
          <description>APB2 peripheral reset register</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>TIM11RST</name>
              <description>TIM11 reset</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIM9RST</name>
              <description>TIM9 reset</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SYSCFGRST</name>
              <description>System configuration controller
              reset</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SPI1RST</name>
              <description>SPI 1 reset</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ADCRST</name>
              <description>ADC interface reset (common to all
              ADCs)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>USART6RST</name>
              <description>USART6 reset</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>USART1RST</name>
              <description>USART1 reset</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIM1RST</name>
              <description>TIM1 reset</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>AHB1ENR</name>
          <displayName>AHB1ENR</displayName>
          <description>AHB1 peripheral clock register</description>
          <addressOffset>0x30</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00100000</resetValue>
          <fields>
            <field>
              <name>GPIOAEN</name>
              <description>IO port A clock enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>GPIOBEN</name>
              <description>IO port B clock enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>GPIOCEN</name>
              <description>IO port C clock enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>GPIOHEN</name>
              <description>IO port H clock enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CRCEN</name>
              <description>CRC clock enable</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMA1EN</name>
              <description>DMA1 clock enable</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMA2EN</name>
              <description>DMA2 clock enable</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RNGEN</name>
              <description>RNG clock enable</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>APB1ENR</name>
          <displayName>APB1ENR</displayName>
          <description>APB1 peripheral clock enable
          register</description>
          <addressOffset>0x40</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>TIM5EN</name>
              <description>TIM5 clock enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIM6EN</name>
              <description>TIM6 clock enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LPTIM1EN</name>
              <description>LPTIM1 clock enable</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RTCAPBEN</name>
              <description>RTC APB clock enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WWDGEN</name>
              <description>Window watchdog clock
              enable</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SPI2EN</name>
              <description>SPI2 clock enable</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>USART2EN</name>
              <description>USART 2 clock enable</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2C1EN</name>
              <description>I2C1 clock enable</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2C2EN</name>
              <description>I2C2 clock enable</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2C4EN</name>
              <description>I2C4 clock enable</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PWREN</name>
              <description>Power interface clock
              enable</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DACEN</name>
              <description>DAC interface clock enable</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>APB2ENR</name>
          <displayName>APB2ENR</displayName>
          <description>APB2 peripheral clock enable
          register</description>
          <addressOffset>0x44</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>TIM1EN</name>
              <description>TIM1 clock enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>USART1EN</name>
              <description>USART1 clock enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>USART6EN</name>
              <description>USART6 clock enable</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ADC1EN</name>
              <description>ADC1 clock enable</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SPI1EN</name>
              <description>SPI1 clock enable</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SYSCFGEN</name>
              <description>System configuration controller clock
              enable</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EXTITEN</name>
              <description>EXTI ans external IT clock
              enable</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIM9EN</name>
              <description>TIM9 clock enable</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIM11EN</name>
              <description>TIM11 clock enable</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SPI5EN</name>
              <description>SPI5 clock enable</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>AHB1LPENR</name>
          <displayName>AHB1LPENR</displayName>
          <description>AHB1 peripheral clock enable in low power
          mode register</description>
          <addressOffset>0x50</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x7E6791FF</resetValue>
          <fields>
            <field>
              <name>GPIOALPEN</name>
              <description>IO port A clock enable during sleep
              mode</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>GPIOBLPEN</name>
              <description>IO port B clock enable during Sleep
              mode</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>GPIOCLPEN</name>
              <description>IO port C clock enable during Sleep
              mode</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>GPIOHLPEN</name>
              <description>IO port H clock enable during Sleep
              mode</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CRCLPEN</name>
              <description>CRC clock enable during Sleep
              mode</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>FLITFLPEN</name>
              <description>Flash interface clock enable during
              Sleep mode</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SRAM1LPEN</name>
              <description>SRAM 1interface clock enable during
              Sleep mode</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMA1LPEN</name>
              <description>DMA1 clock enable during Sleep
              mode</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMA2LPEN</name>
              <description>DMA2 clock enable during Sleep
              mode</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RNGLPEN</name>
              <description>RNG clock enable during sleep
              mode</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>APB1LPENR</name>
          <displayName>APB1LPENR</displayName>
          <description>APB1 peripheral clock enable in low power
          mode register</description>
          <addressOffset>0x60</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x36FEC9FF</resetValue>
          <fields>
            <field>
              <name>TIM5LPEN</name>
              <description>TIM5 clock enable during Sleep
              mode</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIM6LPEN</name>
              <description>TIM6 clock enable during Sleep
              mode</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LPTIM1LPEN</name>
              <description>LPTIM1 clock enable during sleep
              mode</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RTCAPBLPEN</name>
              <description>RTC APB clock enable during sleep
              mode</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WWDGLPEN</name>
              <description>Window watchdog clock enable during
              Sleep mode</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SPI2LPEN</name>
              <description>SPI2 clock enable during Sleep
              mode</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>USART2LPEN</name>
              <description>USART2 clock enable during Sleep
              mode</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2C1LPEN</name>
              <description>I2C1 clock enable during Sleep
              mode</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2C2LPEN</name>
              <description>I2C2 clock enable during Sleep
              mode</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2C4LPEN</name>
              <description>I2C4 clock enable during Sleep
              mode</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PWRLPEN</name>
              <description>Power interface clock enable during
              Sleep mode</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DACLPEN</name>
              <description>DAC interface clock enable during sleep
              mode</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>APB2LPENR</name>
          <displayName>APB2LPENR</displayName>
          <description>APB2 peripheral clock enabled in low power
          mode register</description>
          <addressOffset>0x64</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00075F33</resetValue>
          <fields>
            <field>
              <name>TIM1LPEN</name>
              <description>TIM1 clock enable during Sleep
              mode</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>USART1LPEN</name>
              <description>USART1 clock enable during Sleep
              mode</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>USART6LPEN</name>
              <description>USART6 clock enable during Sleep
              mode</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ADC1LPEN</name>
              <description>ADC1 clock enable during Sleep
              mode</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SDIOLPEN</name>
              <description>SDIO clock enable during Sleep
              mode</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SPI1LPEN</name>
              <description>SPI 1 clock enable during Sleep
              mode</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SYSCFGLPEN</name>
              <description>System configuration controller clock
              enable during Sleep mode</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EXTITLPEN</name>
              <description>EXTI and External IT clock enable during
              sleep mode</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIM9LPEN</name>
              <description>TIM9 clock enable during sleep
              mode</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIM11LPEN</name>
              <description>TIM11 clock enable during Sleep
              mode</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BDCR</name>
          <displayName>BDCR</displayName>
          <description>Backup domain control register</description>
          <addressOffset>0x70</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BDRST</name>
              <description>Backup domain software
              reset</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>RTCEN</name>
              <description>RTC clock enable</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>RTCSEL1</name>
              <description>RTC clock source selection</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>RTCSEL0</name>
              <description>RTC clock source selection</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>LSEBYP</name>
              <description>External low-speed oscillator
              bypass</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>LSERDY</name>
              <description>External low-speed oscillator
              ready</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>LSEON</name>
              <description>External low-speed oscillator
              enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
        <register>
          <name>CSR</name>
          <displayName>CSR</displayName>
          <description>clock control &amp; status
          register</description>
          <addressOffset>0x74</addressOffset>
          <size>0x20</size>
          <resetValue>0x0E000000</resetValue>
          <fields>
            <field>
              <name>LPWRRSTF</name>
              <description>Low-power reset flag</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>WWDGRSTF</name>
              <description>Window watchdog reset flag</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>WDGRSTF</name>
              <description>Independent watchdog reset
              flag</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>SFTRSTF</name>
              <description>Software reset flag</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>PORRSTF</name>
              <description>POR/PDR reset flag</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>PADRSTF</name>
              <description>PIN reset flag</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>BORRSTF</name>
              <description>BOR reset flag</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>RMVF</name>
              <description>Remove reset flag</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>LSIRDY</name>
              <description>Internal low-speed oscillator
              ready</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>LSION</name>
              <description>Internal low-speed oscillator
              enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
        <register>
          <name>SSCGR</name>
          <displayName>SSCGR</displayName>
          <description>spread spectrum clock generation
          register</description>
          <addressOffset>0x80</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SSCGEN</name>
              <description>Spread spectrum modulation
              enable</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SPREADSEL</name>
              <description>Spread Select</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>INCSTEP</name>
              <description>Incrementation step</description>
              <bitOffset>13</bitOffset>
              <bitWidth>15</bitWidth>
            </field>
            <field>
              <name>MODPER</name>
              <description>Modulation period</description>
              <bitOffset>0</bitOffset>
              <bitWidth>13</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DCKCFGR</name>
          <displayName>DCKCFGR</displayName>
          <description>DCKCFGR register</description>
          <addressOffset>0x8C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>TIMPRE</name>
              <description>TIMPRE</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2SSRC</name>
              <description>I2SSRC</description>
              <bitOffset>25</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DCKCFGR2</name>
          <displayName>DCKCFGR2</displayName>
          <description>DCKCFGR2 register</description>
          <addressOffset>0x94</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>I2C4SEL</name>
              <description>I2C4SEL</description>
              <bitOffset>22</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>LPTIM1SEL</name>
              <description>LPTIM1SEL</description>
              <bitOffset>30</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>RTC</name>
      <description>Real-time clock</description>
      <groupName>RTC</groupName>
      <baseAddress>0x40002800</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>RTC_WKUP</name>
        <description>RTC Wakeup interrupt through the EXTI
        line</description>
        <value>3</value>
      </interrupt>
      <registers>
        <register>
          <name>TR</name>
          <displayName>TR</displayName>
          <description>time register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PM</name>
              <description>AM/PM notation</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HT</name>
              <description>Hour tens in BCD format</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>HU</name>
              <description>Hour units in BCD format</description>
              <bitOffset>16</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>MNT</name>
              <description>Minute tens in BCD format</description>
              <bitOffset>12</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>MNU</name>
              <description>Minute units in BCD format</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>ST</name>
              <description>Second tens in BCD format</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>SU</name>
              <description>Second units in BCD format</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DR</name>
          <displayName>DR</displayName>
          <description>date register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00002101</resetValue>
          <fields>
            <field>
              <name>YT</name>
              <description>Year tens in BCD format</description>
              <bitOffset>20</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>YU</name>
              <description>Year units in BCD format</description>
              <bitOffset>16</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>WDU</name>
              <description>Week day units</description>
              <bitOffset>13</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>MT</name>
              <description>Month tens in BCD format</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MU</name>
              <description>Month units in BCD format</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>DT</name>
              <description>Date tens in BCD format</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>DU</name>
              <description>Date units in BCD format</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>control register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>COE</name>
              <description>Calibration output enable</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OSEL</name>
              <description>Output selection</description>
              <bitOffset>21</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>POL</name>
              <description>Output polarity</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>COSEL</name>
              <description>Calibration Output
              selection</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BKP</name>
              <description>Backup</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SUB1H</name>
              <description>Subtract 1 hour (winter time
              change)</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ADD1H</name>
              <description>Add 1 hour (summer time
              change)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TSIE</name>
              <description>Time-stamp interrupt
              enable</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WUTIE</name>
              <description>Wakeup timer interrupt
              enable</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ALRBIE</name>
              <description>Alarm B interrupt enable</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ALRAIE</name>
              <description>Alarm A interrupt enable</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TSE</name>
              <description>Time stamp enable</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WUTE</name>
              <description>Wakeup timer enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ALRBE</name>
              <description>Alarm B enable</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ALRAE</name>
              <description>Alarm A enable</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DCE</name>
              <description>Coarse digital calibration
              enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>FMT</name>
              <description>Hour format</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BYPSHAD</name>
              <description>Bypass the shadow
              registers</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>REFCKON</name>
              <description>Reference clock detection enable (50 or
              60 Hz)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TSEDGE</name>
              <description>Time-stamp event active
              edge</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WCKSEL</name>
              <description>Wakeup clock selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ISR</name>
          <displayName>ISR</displayName>
          <description>initialization and status
          register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000007</resetValue>
          <fields>
            <field>
              <name>ALRAWF</name>
              <description>Alarm A write flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>ALRBWF</name>
              <description>Alarm B write flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>WUTWF</name>
              <description>Wakeup timer write flag</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>SHPF</name>
              <description>Shift operation pending</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>INITS</name>
              <description>Initialization status flag</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>RSF</name>
              <description>Registers synchronization
              flag</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>INITF</name>
              <description>Initialization flag</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>INIT</name>
              <description>Initialization mode</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>ALRAF</name>
              <description>Alarm A flag</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>ALRBF</name>
              <description>Alarm B flag</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>WUTF</name>
              <description>Wakeup timer flag</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>TSF</name>
              <description>Time-stamp flag</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>TSOVF</name>
              <description>Time-stamp overflow flag</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>TAMP1F</name>
              <description>Tamper detection flag</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>TAMP2F</name>
              <description>TAMPER2 detection flag</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>RECALPF</name>
              <description>Recalibration pending Flag</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
          </fields>
        </register>
        <register>
          <name>PRER</name>
          <displayName>PRER</displayName>
          <description>prescaler register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x007F00FF</resetValue>
          <fields>
            <field>
              <name>PREDIV_A</name>
              <description>Asynchronous prescaler
              factor</description>
              <bitOffset>16</bitOffset>
              <bitWidth>7</bitWidth>
            </field>
            <field>
              <name>PREDIV_S</name>
              <description>Synchronous prescaler
              factor</description>
              <bitOffset>0</bitOffset>
              <bitWidth>15</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>WUTR</name>
          <displayName>WUTR</displayName>
          <description>wakeup timer register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000FFFF</resetValue>
          <fields>
            <field>
              <name>WUT</name>
              <description>Wakeup auto-reload value
              bits</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CALIBR</name>
          <displayName>CALIBR</displayName>
          <description>calibration register</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DCS</name>
              <description>Digital calibration sign</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DC</name>
              <description>Digital calibration</description>
              <bitOffset>0</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ALRMAR</name>
          <displayName>ALRMAR</displayName>
          <description>alarm A register</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MSK4</name>
              <description>Alarm A date mask</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WDSEL</name>
              <description>Week day selection</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DT</name>
              <description>Date tens in BCD format</description>
              <bitOffset>28</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>DU</name>
              <description>Date units or day in BCD
              format</description>
              <bitOffset>24</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>MSK3</name>
              <description>Alarm A hours mask</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PM</name>
              <description>AM/PM notation</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HT</name>
              <description>Hour tens in BCD format</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>HU</name>
              <description>Hour units in BCD format</description>
              <bitOffset>16</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>MSK2</name>
              <description>Alarm A minutes mask</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MNT</name>
              <description>Minute tens in BCD format</description>
              <bitOffset>12</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>MNU</name>
              <description>Minute units in BCD format</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>MSK1</name>
              <description>Alarm A seconds mask</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ST</name>
              <description>Second tens in BCD format</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>SU</name>
              <description>Second units in BCD format</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ALRMBR</name>
          <displayName>ALRMBR</displayName>
          <description>alarm B register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MSK4</name>
              <description>Alarm B date mask</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WDSEL</name>
              <description>Week day selection</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DT</name>
              <description>Date tens in BCD format</description>
              <bitOffset>28</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>DU</name>
              <description>Date units or day in BCD
              format</description>
              <bitOffset>24</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>MSK3</name>
              <description>Alarm B hours mask</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PM</name>
              <description>AM/PM notation</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HT</name>
              <description>Hour tens in BCD format</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>HU</name>
              <description>Hour units in BCD format</description>
              <bitOffset>16</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>MSK2</name>
              <description>Alarm B minutes mask</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MNT</name>
              <description>Minute tens in BCD format</description>
              <bitOffset>12</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>MNU</name>
              <description>Minute units in BCD format</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>MSK1</name>
              <description>Alarm B seconds mask</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ST</name>
              <description>Second tens in BCD format</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>SU</name>
              <description>Second units in BCD format</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>WPR</name>
          <displayName>WPR</displayName>
          <description>write protection register</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>KEY</name>
              <description>Write protection key</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SSR</name>
          <displayName>SSR</displayName>
          <description>sub second register</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SS</name>
              <description>Sub second value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SHIFTR</name>
          <displayName>SHIFTR</displayName>
          <description>shift control register</description>
          <addressOffset>0x2C</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ADD1S</name>
              <description>Add one second</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SUBFS</name>
              <description>Subtract a fraction of a
              second</description>
              <bitOffset>0</bitOffset>
              <bitWidth>15</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>TSTR</name>
          <displayName>TSTR</displayName>
          <description>time stamp time register</description>
          <addressOffset>0x30</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PM</name>
              <description>AM/PM notation</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HT</name>
              <description>Hour tens in BCD format</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>HU</name>
              <description>Hour units in BCD format</description>
              <bitOffset>16</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>MNT</name>
              <description>Minute tens in BCD format</description>
              <bitOffset>12</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>MNU</name>
              <description>Minute units in BCD format</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>ST</name>
              <description>Second tens in BCD format</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>SU</name>
              <description>Second units in BCD format</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>TSDR</name>
          <displayName>TSDR</displayName>
          <description>time stamp date register</description>
          <addressOffset>0x34</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>WDU</name>
              <description>Week day units</description>
              <bitOffset>13</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>MT</name>
              <description>Month tens in BCD format</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MU</name>
              <description>Month units in BCD format</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>DT</name>
              <description>Date tens in BCD format</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>DU</name>
              <description>Date units in BCD format</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>TSSSR</name>
          <displayName>TSSSR</displayName>
          <description>timestamp sub second register</description>
          <addressOffset>0x38</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SS</name>
              <description>Sub second value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CALR</name>
          <displayName>CALR</displayName>
          <description>calibration register</description>
          <addressOffset>0x3C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CALP</name>
              <description>Increase frequency of RTC by 488.5
              ppm</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CALW8</name>
              <description>Use an 8-second calibration cycle
              period</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CALW16</name>
              <description>Use a 16-second calibration cycle
              period</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CALM</name>
              <description>Calibration minus</description>
              <bitOffset>0</bitOffset>
              <bitWidth>9</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>TAFCR</name>
          <displayName>TAFCR</displayName>
          <description>tamper and alternate function configuration
          register</description>
          <addressOffset>0x40</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ALARMOUTTYPE</name>
              <description>AFO_ALARM output type</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TSINSEL</name>
              <description>TIMESTAMP mapping</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TAMP1INSEL</name>
              <description>TAMPER1 mapping</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TAMPPUDIS</name>
              <description>TAMPER pull-up disable</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TAMPPRCH</name>
              <description>Tamper precharge duration</description>
              <bitOffset>13</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>TAMPFLT</name>
              <description>Tamper filter count</description>
              <bitOffset>11</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>TAMPFREQ</name>
              <description>Tamper sampling frequency</description>
              <bitOffset>8</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>TAMPTS</name>
              <description>Activate timestamp on tamper detection
              event</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TAMP2TRG</name>
              <description>Active level for tamper 2</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TAMP2E</name>
              <description>Tamper 2 detection enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TAMPIE</name>
              <description>Tamper interrupt enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TAMP1TRG</name>
              <description>Active level for tamper 1</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TAMP1E</name>
              <description>Tamper 1 detection enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ALRMASSR</name>
          <displayName>ALRMASSR</displayName>
          <description>alarm A sub second register</description>
          <addressOffset>0x44</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MASKSS</name>
              <description>Mask the most-significant bits starting
              at this bit</description>
              <bitOffset>24</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>SS</name>
              <description>Sub seconds value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>15</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ALRMBSSR</name>
          <displayName>ALRMBSSR</displayName>
          <description>alarm B sub second register</description>
          <addressOffset>0x48</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MASKSS</name>
              <description>Mask the most-significant bits starting
              at this bit</description>
              <bitOffset>24</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>SS</name>
              <description>Sub seconds value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>15</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BKP0R</name>
          <displayName>BKP0R</displayName>
          <description>backup register</description>
          <addressOffset>0x50</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BKP</name>
              <description>BKP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BKP1R</name>
          <displayName>BKP1R</displayName>
          <description>backup register</description>
          <addressOffset>0x54</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BKP</name>
              <description>BKP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BKP2R</name>
          <displayName>BKP2R</displayName>
          <description>backup register</description>
          <addressOffset>0x58</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BKP</name>
              <description>BKP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BKP3R</name>
          <displayName>BKP3R</displayName>
          <description>backup register</description>
          <addressOffset>0x5C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BKP</name>
              <description>BKP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BKP4R</name>
          <displayName>BKP4R</displayName>
          <description>backup register</description>
          <addressOffset>0x60</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BKP</name>
              <description>BKP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BKP5R</name>
          <displayName>BKP5R</displayName>
          <description>backup register</description>
          <addressOffset>0x64</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BKP</name>
              <description>BKP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BKP6R</name>
          <displayName>BKP6R</displayName>
          <description>backup register</description>
          <addressOffset>0x68</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BKP</name>
              <description>BKP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BKP7R</name>
          <displayName>BKP7R</displayName>
          <description>backup register</description>
          <addressOffset>0x6C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BKP</name>
              <description>BKP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BKP8R</name>
          <displayName>BKP8R</displayName>
          <description>backup register</description>
          <addressOffset>0x70</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BKP</name>
              <description>BKP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BKP9R</name>
          <displayName>BKP9R</displayName>
          <description>backup register</description>
          <addressOffset>0x74</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BKP</name>
              <description>BKP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BKP10R</name>
          <displayName>BKP10R</displayName>
          <description>backup register</description>
          <addressOffset>0x78</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BKP</name>
              <description>BKP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BKP11R</name>
          <displayName>BKP11R</displayName>
          <description>backup register</description>
          <addressOffset>0x7C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BKP</name>
              <description>BKP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BKP12R</name>
          <displayName>BKP12R</displayName>
          <description>backup register</description>
          <addressOffset>0x80</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BKP</name>
              <description>BKP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BKP13R</name>
          <displayName>BKP13R</displayName>
          <description>backup register</description>
          <addressOffset>0x84</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BKP</name>
              <description>BKP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BKP14R</name>
          <displayName>BKP14R</displayName>
          <description>backup register</description>
          <addressOffset>0x88</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BKP</name>
              <description>BKP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BKP15R</name>
          <displayName>BKP15R</displayName>
          <description>backup register</description>
          <addressOffset>0x8C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BKP</name>
              <description>BKP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BKP16R</name>
          <displayName>BKP16R</displayName>
          <description>backup register</description>
          <addressOffset>0x90</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BKP</name>
              <description>BKP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BKP17R</name>
          <displayName>BKP17R</displayName>
          <description>backup register</description>
          <addressOffset>0x94</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BKP</name>
              <description>BKP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BKP18R</name>
          <displayName>BKP18R</displayName>
          <description>backup register</description>
          <addressOffset>0x98</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BKP</name>
              <description>BKP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BKP19R</name>
          <displayName>BKP19R</displayName>
          <description>backup register</description>
          <addressOffset>0x9C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BKP</name>
              <description>BKP</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>SYSCFG</name>
      <description>System configuration controller</description>
      <groupName>SYSCFG</groupName>
      <baseAddress>0x40013800</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>MEMRM</name>
          <displayName>MEMRM</displayName>
          <description>memory remap register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MEM_MODE</name>
              <description>MEM_MODE</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>PMC</name>
          <displayName>PMC</displayName>
          <description>peripheral mode configuration
          register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ADC1DC2</name>
              <description>ADC1DC2</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EXTICR1</name>
          <displayName>EXTICR1</displayName>
          <description>external interrupt configuration register
          1</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>EXTI3</name>
              <description>EXTI x configuration (x = 0 to
              3)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>EXTI2</name>
              <description>EXTI x configuration (x = 0 to
              3)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>EXTI1</name>
              <description>EXTI x configuration (x = 0 to
              3)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>EXTI0</name>
              <description>EXTI x configuration (x = 0 to
              3)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EXTICR2</name>
          <displayName>EXTICR2</displayName>
          <description>external interrupt configuration register
          2</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>EXTI7</name>
              <description>EXTI x configuration (x = 4 to
              7)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>EXTI6</name>
              <description>EXTI x configuration (x = 4 to
              7)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>EXTI5</name>
              <description>EXTI x configuration (x = 4 to
              7)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>EXTI4</name>
              <description>EXTI x configuration (x = 4 to
              7)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EXTICR3</name>
          <displayName>EXTICR3</displayName>
          <description>external interrupt configuration register
          3</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>EXTI11</name>
              <description>EXTI x configuration (x = 8 to
              11)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>EXTI10</name>
              <description>EXTI10</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>EXTI9</name>
              <description>EXTI x configuration (x = 8 to
              11)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>EXTI8</name>
              <description>EXTI x configuration (x = 8 to
              11)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EXTICR4</name>
          <displayName>EXTICR4</displayName>
          <description>external interrupt configuration register
          4</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>EXTI15</name>
              <description>EXTI x configuration (x = 12 to
              15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>EXTI14</name>
              <description>EXTI x configuration (x = 12 to
              15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>EXTI13</name>
              <description>EXTI x configuration (x = 12 to
              15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>EXTI12</name>
              <description>EXTI x configuration (x = 12 to
              15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CMPCR</name>
          <displayName>CMPCR</displayName>
          <description>Compensation cell control
          register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>READY</name>
              <description>READY</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CMP_PD</name>
              <description>Compensation cell
              power-down</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CFGR</name>
          <displayName>CFGR</displayName>
          <description>Configuration register</description>
          <addressOffset>0x2C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>FMPI2C1_SCL</name>
              <description>FMPI2C1_SCL</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>FMPI2C1_SDA</name>
              <description>FMPI2C1_SDA</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>TIM1</name>
      <description>Advanced-timers</description>
      <groupName>TIM</groupName>
      <baseAddress>0x40010000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>TIM1_BRK_TIM9</name>
        <description>TIM1 Break interrupt and TIM9 global
        interrupt</description>
        <value>24</value>
      </interrupt>
      <interrupt>
        <name>PWM1_UP</name>
        <description>Timer1 Update interrupt</description>
        <value>25</value>
      </interrupt>
      <interrupt>
        <name>TIM1_TRG_COM_TIM11</name>
        <description>TIM1 Trigger and Commutation interrupts and
        TIM11 global interrupt</description>
        <value>26</value>
      </interrupt>
      <interrupt>
        <name>TIM1_CC</name>
        <description>TIM1 Capture Compare interrupt</description>
        <value>27</value>
      </interrupt>
      <registers>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>control register 1</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>CKD</name>
              <description>Clock division</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>ARPE</name>
              <description>Auto-reload preload enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CMS</name>
              <description>Center-aligned mode
              selection</description>
              <bitOffset>5</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>DIR</name>
              <description>Direction</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OPM</name>
              <description>One-pulse mode</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>URS</name>
              <description>Update request source</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UDIS</name>
              <description>Update disable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CEN</name>
              <description>Counter enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR2</name>
          <displayName>CR2</displayName>
          <description>control register 2</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>OIS4</name>
              <description>Output Idle state 4</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OIS3N</name>
              <description>Output Idle state 3</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OIS3</name>
              <description>Output Idle state 3</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OIS2N</name>
              <description>Output Idle state 2</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OIS2</name>
              <description>Output Idle state 2</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OIS1N</name>
              <description>Output Idle state 1</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OIS1</name>
              <description>Output Idle state 1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TI1S</name>
              <description>TI1 selection</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MMS</name>
              <description>Master mode selection</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>CCDS</name>
              <description>Capture/compare DMA
              selection</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CCUS</name>
              <description>Capture/compare control update
              selection</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CCPC</name>
              <description>Capture/compare preloaded
              control</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SMCR</name>
          <displayName>SMCR</displayName>
          <description>slave mode control register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>ETP</name>
              <description>External trigger polarity</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ECE</name>
              <description>External clock enable</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ETPS</name>
              <description>External trigger prescaler</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>ETF</name>
              <description>External trigger filter</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>MSM</name>
              <description>Master/Slave mode</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TS</name>
              <description>Trigger selection</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>SMS</name>
              <description>Slave mode selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DIER</name>
          <displayName>DIER</displayName>
          <description>DMA/Interrupt enable register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>TDE</name>
              <description>Trigger DMA request enable</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>COMDE</name>
              <description>COM DMA request enable</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC4DE</name>
              <description>Capture/Compare 4 DMA request
              enable</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3DE</name>
              <description>Capture/Compare 3 DMA request
              enable</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2DE</name>
              <description>Capture/Compare 2 DMA request
              enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1DE</name>
              <description>Capture/Compare 1 DMA request
              enable</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UDE</name>
              <description>Update DMA request enable</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BIE</name>
              <description>Break interrupt enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIE</name>
              <description>Trigger interrupt enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>COMIE</name>
              <description>COM interrupt enable</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC4IE</name>
              <description>Capture/Compare 4 interrupt
              enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3IE</name>
              <description>Capture/Compare 3 interrupt
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2IE</name>
              <description>Capture/Compare 2 interrupt
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1IE</name>
              <description>Capture/Compare 1 interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UIE</name>
              <description>Update interrupt enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>status register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>CC4OF</name>
              <description>Capture/Compare 4 overcapture
              flag</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3OF</name>
              <description>Capture/Compare 3 overcapture
              flag</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2OF</name>
              <description>Capture/compare 2 overcapture
              flag</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1OF</name>
              <description>Capture/Compare 1 overcapture
              flag</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BIF</name>
              <description>Break interrupt flag</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIF</name>
              <description>Trigger interrupt flag</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>COMIF</name>
              <description>COM interrupt flag</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC4IF</name>
              <description>Capture/Compare 4 interrupt
              flag</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3IF</name>
              <description>Capture/Compare 3 interrupt
              flag</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2IF</name>
              <description>Capture/Compare 2 interrupt
              flag</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1IF</name>
              <description>Capture/compare 1 interrupt
              flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UIF</name>
              <description>Update interrupt flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EGR</name>
          <displayName>EGR</displayName>
          <description>event generation register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>BG</name>
              <description>Break generation</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TG</name>
              <description>Trigger generation</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>COMG</name>
              <description>Capture/Compare control update
              generation</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC4G</name>
              <description>Capture/compare 4
              generation</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3G</name>
              <description>Capture/compare 3
              generation</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2G</name>
              <description>Capture/compare 2
              generation</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1G</name>
              <description>Capture/compare 1
              generation</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UG</name>
              <description>Update generation</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR1_Output</name>
          <displayName>CCMR1_Output</displayName>
          <description>capture/compare mode register 1 (output
          mode)</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OC2CE</name>
              <description>Output Compare 2 clear
              enable</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC2M</name>
              <description>Output Compare 2 mode</description>
              <bitOffset>12</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>OC2PE</name>
              <description>Output Compare 2 preload
              enable</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC2FE</name>
              <description>Output Compare 2 fast
              enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2S</name>
              <description>Capture/Compare 2
              selection</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OC1CE</name>
              <description>Output Compare 1 clear
              enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC1M</name>
              <description>Output Compare 1 mode</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>OC1PE</name>
              <description>Output Compare 1 preload
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC1FE</name>
              <description>Output Compare 1 fast
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1S</name>
              <description>Capture/Compare 1
              selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR1_Input</name>
          <displayName>CCMR1_Input</displayName>
          <description>capture/compare mode register 1 (input
          mode)</description>
          <alternateRegister>CCMR1_Output</alternateRegister>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IC2F</name>
              <description>Input capture 2 filter</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>IC2PCS</name>
              <description>Input capture 2 prescaler</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CC2S</name>
              <description>Capture/Compare 2
              selection</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>IC1F</name>
              <description>Input capture 1 filter</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>ICPCS</name>
              <description>Input capture 1 prescaler</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CC1S</name>
              <description>Capture/Compare 1
              selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR2_Output</name>
          <displayName>CCMR2_Output</displayName>
          <description>capture/compare mode register 2 (output
          mode)</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OC4CE</name>
              <description>Output compare 4 clear
              enable</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC4M</name>
              <description>Output compare 4 mode</description>
              <bitOffset>12</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>OC4PE</name>
              <description>Output compare 4 preload
              enable</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC4FE</name>
              <description>Output compare 4 fast
              enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC4S</name>
              <description>Capture/Compare 4
              selection</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OC3CE</name>
              <description>Output compare 3 clear
              enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC3M</name>
              <description>Output compare 3 mode</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>OC3PE</name>
              <description>Output compare 3 preload
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC3FE</name>
              <description>Output compare 3 fast
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3S</name>
              <description>Capture/Compare 3
              selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR2_Input</name>
          <displayName>CCMR2_Input</displayName>
          <description>capture/compare mode register 2 (input
          mode)</description>
          <alternateRegister>CCMR2_Output</alternateRegister>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IC4F</name>
              <description>Input capture 4 filter</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>IC4PSC</name>
              <description>Input capture 4 prescaler</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CC4S</name>
              <description>Capture/Compare 4
              selection</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>IC3F</name>
              <description>Input capture 3 filter</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>IC3PSC</name>
              <description>Input capture 3 prescaler</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CC3S</name>
              <description>Capture/compare 3
              selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCER</name>
          <displayName>CCER</displayName>
          <description>capture/compare enable
          register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>CC4P</name>
              <description>Capture/Compare 3 output
              Polarity</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC4E</name>
              <description>Capture/Compare 4 output
              enable</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3NP</name>
              <description>Capture/Compare 3 output
              Polarity</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3NE</name>
              <description>Capture/Compare 3 complementary output
              enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3P</name>
              <description>Capture/Compare 3 output
              Polarity</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3E</name>
              <description>Capture/Compare 3 output
              enable</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2NP</name>
              <description>Capture/Compare 2 output
              Polarity</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2NE</name>
              <description>Capture/Compare 2 complementary output
              enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2P</name>
              <description>Capture/Compare 2 output
              Polarity</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2E</name>
              <description>Capture/Compare 2 output
              enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1NP</name>
              <description>Capture/Compare 1 output
              Polarity</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1NE</name>
              <description>Capture/Compare 1 complementary output
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1P</name>
              <description>Capture/Compare 1 output
              Polarity</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1E</name>
              <description>Capture/Compare 1 output
              enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CNT</name>
          <displayName>CNT</displayName>
          <description>counter</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CNT</name>
              <description>counter value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>PSC</name>
          <displayName>PSC</displayName>
          <description>prescaler</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>PSC</name>
              <description>Prescaler value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ARR</name>
          <displayName>ARR</displayName>
          <description>auto-reload register</description>
          <addressOffset>0x2C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ARR</name>
              <description>Auto-reload value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR1</name>
          <displayName>CCR1</displayName>
          <description>capture/compare register 1</description>
          <addressOffset>0x34</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CCR1</name>
              <description>Capture/Compare 1 value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR2</name>
          <displayName>CCR2</displayName>
          <description>capture/compare register 2</description>
          <addressOffset>0x38</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CCR2</name>
              <description>Capture/Compare 2 value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR3</name>
          <displayName>CCR3</displayName>
          <description>capture/compare register 3</description>
          <addressOffset>0x3C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CCR3</name>
              <description>Capture/Compare value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR4</name>
          <displayName>CCR4</displayName>
          <description>capture/compare register 4</description>
          <addressOffset>0x40</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CCR4</name>
              <description>Capture/Compare value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DCR</name>
          <displayName>DCR</displayName>
          <description>DMA control register</description>
          <addressOffset>0x48</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>DBL</name>
              <description>DMA burst length</description>
              <bitOffset>8</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
            <field>
              <name>DBA</name>
              <description>DMA base address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DMAR</name>
          <displayName>DMAR</displayName>
          <description>DMA address for full transfer</description>
          <addressOffset>0x4C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>DMAB</name>
              <description>DMA register for burst
              accesses</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>RCR</name>
          <displayName>RCR</displayName>
          <description>repetition counter register</description>
          <addressOffset>0x30</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>REP</name>
              <description>Repetition counter value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BDTR</name>
          <displayName>BDTR</displayName>
          <description>break and dead-time register</description>
          <addressOffset>0x44</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>MOE</name>
              <description>Main output enable</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>AOE</name>
              <description>Automatic output enable</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BKP</name>
              <description>Break polarity</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BKE</name>
              <description>Break enable</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OSSR</name>
              <description>Off-state selection for Run
              mode</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OSSI</name>
              <description>Off-state selection for Idle
              mode</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LOCK</name>
              <description>Lock configuration</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>DTG</name>
              <description>Dead-time generator setup</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral derivedFrom="TIM1">
      <name>TIM8</name>
      <baseAddress>0x40010400</baseAddress>
    </peripheral>
    <peripheral>
      <name>TIM11</name>
      <description>General-purpose-timers</description>
      <groupName>TIM</groupName>
      <baseAddress>0x40014800</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>control register 1</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>CKD</name>
              <description>Clock division</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>ARPE</name>
              <description>Auto-reload preload enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>URS</name>
              <description>Update request source</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UDIS</name>
              <description>Update disable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CEN</name>
              <description>Counter enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DIER</name>
          <displayName>DIER</displayName>
          <description>DMA/Interrupt enable register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>CC1IE</name>
              <description>Capture/Compare 1 interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UIE</name>
              <description>Update interrupt enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>status register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>CC1OF</name>
              <description>Capture/Compare 1 overcapture
              flag</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1IF</name>
              <description>Capture/compare 1 interrupt
              flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UIF</name>
              <description>Update interrupt flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EGR</name>
          <displayName>EGR</displayName>
          <description>event generation register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>CC1G</name>
              <description>Capture/compare 1
              generation</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UG</name>
              <description>Update generation</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR1_Output</name>
          <displayName>CCMR1_Output</displayName>
          <description>capture/compare mode register 1 (output
          mode)</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OC1M</name>
              <description>Output Compare 1 mode</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>OC1PE</name>
              <description>Output Compare 1 preload
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC1FE</name>
              <description>Output Compare 1 fast
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1S</name>
              <description>Capture/Compare 1
              selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR1_Input</name>
          <displayName>CCMR1_Input</displayName>
          <description>capture/compare mode register 1 (input
          mode)</description>
          <alternateRegister>CCMR1_Output</alternateRegister>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IC1F</name>
              <description>Input capture 1 filter</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>ICPCS</name>
              <description>Input capture 1 prescaler</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CC1S</name>
              <description>Capture/Compare 1
              selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCER</name>
          <displayName>CCER</displayName>
          <description>capture/compare enable
          register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>CC1NP</name>
              <description>Capture/Compare 1 output
              Polarity</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1P</name>
              <description>Capture/Compare 1 output
              Polarity</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1E</name>
              <description>Capture/Compare 1 output
              enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CNT</name>
          <displayName>CNT</displayName>
          <description>counter</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CNT</name>
              <description>counter value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>PSC</name>
          <displayName>PSC</displayName>
          <description>prescaler</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>PSC</name>
              <description>Prescaler value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ARR</name>
          <displayName>ARR</displayName>
          <description>auto-reload register</description>
          <addressOffset>0x2C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ARR</name>
              <description>Auto-reload value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR1</name>
          <displayName>CCR1</displayName>
          <description>capture/compare register 1</description>
          <addressOffset>0x34</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CCR1</name>
              <description>Capture/Compare 1 value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OR</name>
          <displayName>OR</displayName>
          <description>option register</description>
          <addressOffset>0x50</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>RMP</name>
              <description>Input 1 remapping
              capability</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>TIM5</name>
      <description>General-purpose-timers</description>
      <groupName>TIM</groupName>
      <baseAddress>0x40000C00</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>control register 1</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>CKD</name>
              <description>Clock division</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>ARPE</name>
              <description>Auto-reload preload enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CMS</name>
              <description>Center-aligned mode
              selection</description>
              <bitOffset>5</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>DIR</name>
              <description>Direction</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OPM</name>
              <description>One-pulse mode</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>URS</name>
              <description>Update request source</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UDIS</name>
              <description>Update disable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CEN</name>
              <description>Counter enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR2</name>
          <displayName>CR2</displayName>
          <description>control register 2</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>TI1S</name>
              <description>TI1 selection</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MMS</name>
              <description>Master mode selection</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>CCDS</name>
              <description>Capture/compare DMA
              selection</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SMCR</name>
          <displayName>SMCR</displayName>
          <description>slave mode control register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>ETP</name>
              <description>External trigger polarity</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ECE</name>
              <description>External clock enable</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ETPS</name>
              <description>External trigger prescaler</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>ETF</name>
              <description>External trigger filter</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>MSM</name>
              <description>Master/Slave mode</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TS</name>
              <description>Trigger selection</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>SMS</name>
              <description>Slave mode selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DIER</name>
          <displayName>DIER</displayName>
          <description>DMA/Interrupt enable register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>TDE</name>
              <description>Trigger DMA request enable</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC4DE</name>
              <description>Capture/Compare 4 DMA request
              enable</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3DE</name>
              <description>Capture/Compare 3 DMA request
              enable</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2DE</name>
              <description>Capture/Compare 2 DMA request
              enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1DE</name>
              <description>Capture/Compare 1 DMA request
              enable</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UDE</name>
              <description>Update DMA request enable</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIE</name>
              <description>Trigger interrupt enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC4IE</name>
              <description>Capture/Compare 4 interrupt
              enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3IE</name>
              <description>Capture/Compare 3 interrupt
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2IE</name>
              <description>Capture/Compare 2 interrupt
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1IE</name>
              <description>Capture/Compare 1 interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UIE</name>
              <description>Update interrupt enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>status register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>CC4OF</name>
              <description>Capture/Compare 4 overcapture
              flag</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3OF</name>
              <description>Capture/Compare 3 overcapture
              flag</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2OF</name>
              <description>Capture/compare 2 overcapture
              flag</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1OF</name>
              <description>Capture/Compare 1 overcapture
              flag</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIF</name>
              <description>Trigger interrupt flag</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC4IF</name>
              <description>Capture/Compare 4 interrupt
              flag</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3IF</name>
              <description>Capture/Compare 3 interrupt
              flag</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2IF</name>
              <description>Capture/Compare 2 interrupt
              flag</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1IF</name>
              <description>Capture/compare 1 interrupt
              flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UIF</name>
              <description>Update interrupt flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EGR</name>
          <displayName>EGR</displayName>
          <description>event generation register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>TG</name>
              <description>Trigger generation</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC4G</name>
              <description>Capture/compare 4
              generation</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3G</name>
              <description>Capture/compare 3
              generation</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2G</name>
              <description>Capture/compare 2
              generation</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1G</name>
              <description>Capture/compare 1
              generation</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UG</name>
              <description>Update generation</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR1_Output</name>
          <displayName>CCMR1_Output</displayName>
          <description>capture/compare mode register 1 (output
          mode)</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OC2CE</name>
              <description>OC2CE</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC2M</name>
              <description>OC2M</description>
              <bitOffset>12</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>OC2PE</name>
              <description>OC2PE</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC2FE</name>
              <description>OC2FE</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2S</name>
              <description>CC2S</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OC1CE</name>
              <description>OC1CE</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC1M</name>
              <description>OC1M</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>OC1PE</name>
              <description>OC1PE</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC1FE</name>
              <description>OC1FE</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1S</name>
              <description>CC1S</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR1_Input</name>
          <displayName>CCMR1_Input</displayName>
          <description>capture/compare mode register 1 (input
          mode)</description>
          <alternateRegister>CCMR1_Output</alternateRegister>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IC2F</name>
              <description>Input capture 2 filter</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>IC2PCS</name>
              <description>Input capture 2 prescaler</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CC2S</name>
              <description>Capture/Compare 2
              selection</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>IC1F</name>
              <description>Input capture 1 filter</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>ICPCS</name>
              <description>Input capture 1 prescaler</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CC1S</name>
              <description>Capture/Compare 1
              selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR2_Output</name>
          <displayName>CCMR2_Output</displayName>
          <description>capture/compare mode register 2 (output
          mode)</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>O24CE</name>
              <description>O24CE</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC4M</name>
              <description>OC4M</description>
              <bitOffset>12</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>OC4PE</name>
              <description>OC4PE</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC4FE</name>
              <description>OC4FE</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC4S</name>
              <description>CC4S</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OC3CE</name>
              <description>OC3CE</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC3M</name>
              <description>OC3M</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>OC3PE</name>
              <description>OC3PE</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC3FE</name>
              <description>OC3FE</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3S</name>
              <description>CC3S</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR2_Input</name>
          <displayName>CCMR2_Input</displayName>
          <description>capture/compare mode register 2 (input
          mode)</description>
          <alternateRegister>CCMR2_Output</alternateRegister>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IC4F</name>
              <description>Input capture 4 filter</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>IC4PSC</name>
              <description>Input capture 4 prescaler</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CC4S</name>
              <description>Capture/Compare 4
              selection</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>IC3F</name>
              <description>Input capture 3 filter</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>IC3PSC</name>
              <description>Input capture 3 prescaler</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CC3S</name>
              <description>Capture/compare 3
              selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCER</name>
          <displayName>CCER</displayName>
          <description>capture/compare enable
          register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>CC4NP</name>
              <description>Capture/Compare 4 output
              Polarity</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC4P</name>
              <description>Capture/Compare 3 output
              Polarity</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC4E</name>
              <description>Capture/Compare 4 output
              enable</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3NP</name>
              <description>Capture/Compare 3 output
              Polarity</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3P</name>
              <description>Capture/Compare 3 output
              Polarity</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC3E</name>
              <description>Capture/Compare 3 output
              enable</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2NP</name>
              <description>Capture/Compare 2 output
              Polarity</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2P</name>
              <description>Capture/Compare 2 output
              Polarity</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2E</name>
              <description>Capture/Compare 2 output
              enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1NP</name>
              <description>Capture/Compare 1 output
              Polarity</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1P</name>
              <description>Capture/Compare 1 output
              Polarity</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1E</name>
              <description>Capture/Compare 1 output
              enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CNT</name>
          <displayName>CNT</displayName>
          <description>counter</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CNT_H</name>
              <description>High counter value</description>
              <bitOffset>16</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
            <field>
              <name>CNT_L</name>
              <description>Low counter value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>PSC</name>
          <displayName>PSC</displayName>
          <description>prescaler</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>PSC</name>
              <description>Prescaler value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ARR</name>
          <displayName>ARR</displayName>
          <description>auto-reload register</description>
          <addressOffset>0x2C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ARR_H</name>
              <description>High Auto-reload value</description>
              <bitOffset>16</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
            <field>
              <name>ARR_L</name>
              <description>Low Auto-reload value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR1</name>
          <displayName>CCR1</displayName>
          <description>capture/compare register 1</description>
          <addressOffset>0x34</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CCR1_H</name>
              <description>High Capture/Compare 1
              value</description>
              <bitOffset>16</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
            <field>
              <name>CCR1_L</name>
              <description>Low Capture/Compare 1
              value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR2</name>
          <displayName>CCR2</displayName>
          <description>capture/compare register 2</description>
          <addressOffset>0x38</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CCR2_H</name>
              <description>High Capture/Compare 2
              value</description>
              <bitOffset>16</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
            <field>
              <name>CCR2_L</name>
              <description>Low Capture/Compare 2
              value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR3</name>
          <displayName>CCR3</displayName>
          <description>capture/compare register 3</description>
          <addressOffset>0x3C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CCR3_H</name>
              <description>High Capture/Compare value</description>
              <bitOffset>16</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
            <field>
              <name>CCR3_L</name>
              <description>Low Capture/Compare value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR4</name>
          <displayName>CCR4</displayName>
          <description>capture/compare register 4</description>
          <addressOffset>0x40</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CCR4_H</name>
              <description>High Capture/Compare value</description>
              <bitOffset>16</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
            <field>
              <name>CCR4_L</name>
              <description>Low Capture/Compare value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DCR</name>
          <displayName>DCR</displayName>
          <description>DMA control register</description>
          <addressOffset>0x48</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>DBL</name>
              <description>DMA burst length</description>
              <bitOffset>8</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
            <field>
              <name>DBA</name>
              <description>DMA base address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>5</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DMAR</name>
          <displayName>DMAR</displayName>
          <description>DMA address for full transfer</description>
          <addressOffset>0x4C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>DMAB</name>
              <description>DMA register for burst
              accesses</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OR</name>
          <displayName>OR</displayName>
          <description>TIM5 option register</description>
          <addressOffset>0x50</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>IT4_RMP</name>
              <description>Timer Input 4 remap</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>TIM9</name>
      <description>General purpose timers</description>
      <groupName>TIM</groupName>
      <baseAddress>0x40014000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>control register 1</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>CKD</name>
              <description>Clock division</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>ARPE</name>
              <description>Auto-reload preload enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OPM</name>
              <description>One-pulse mode</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>URS</name>
              <description>Update request source</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UDIS</name>
              <description>Update disable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CEN</name>
              <description>Counter enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR2</name>
          <displayName>CR2</displayName>
          <description>control register 2</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>MMS</name>
              <description>Master mode selection</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SMCR</name>
          <displayName>SMCR</displayName>
          <description>slave mode control register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>MSM</name>
              <description>Master/Slave mode</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TS</name>
              <description>Trigger selection</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>SMS</name>
              <description>Slave mode selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DIER</name>
          <displayName>DIER</displayName>
          <description>DMA/Interrupt enable register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>TIE</name>
              <description>Trigger interrupt enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2IE</name>
              <description>Capture/Compare 2 interrupt
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1IE</name>
              <description>Capture/Compare 1 interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UIE</name>
              <description>Update interrupt enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>status register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>CC2OF</name>
              <description>Capture/compare 2 overcapture
              flag</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1OF</name>
              <description>Capture/Compare 1 overcapture
              flag</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIF</name>
              <description>Trigger interrupt flag</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2IF</name>
              <description>Capture/Compare 2 interrupt
              flag</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1IF</name>
              <description>Capture/compare 1 interrupt
              flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UIF</name>
              <description>Update interrupt flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EGR</name>
          <displayName>EGR</displayName>
          <description>event generation register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>TG</name>
              <description>Trigger generation</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2G</name>
              <description>Capture/compare 2
              generation</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1G</name>
              <description>Capture/compare 1
              generation</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UG</name>
              <description>Update generation</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR1_Output</name>
          <displayName>CCMR1_Output</displayName>
          <description>capture/compare mode register 1 (output
          mode)</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OC2M</name>
              <description>Output Compare 2 mode</description>
              <bitOffset>12</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>OC2PE</name>
              <description>Output Compare 2 preload
              enable</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC2FE</name>
              <description>Output Compare 2 fast
              enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2S</name>
              <description>Capture/Compare 2
              selection</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OC1M</name>
              <description>Output Compare 1 mode</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>OC1PE</name>
              <description>Output Compare 1 preload
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OC1FE</name>
              <description>Output Compare 1 fast
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1S</name>
              <description>Capture/Compare 1
              selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCMR1_Input</name>
          <displayName>CCMR1_Input</displayName>
          <description>capture/compare mode register 1 (input
          mode)</description>
          <alternateRegister>CCMR1_Output</alternateRegister>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IC2F</name>
              <description>Input capture 2 filter</description>
              <bitOffset>12</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>IC2PCS</name>
              <description>Input capture 2 prescaler</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CC2S</name>
              <description>Capture/Compare 2
              selection</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>IC1F</name>
              <description>Input capture 1 filter</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>ICPCS</name>
              <description>Input capture 1 prescaler</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CC1S</name>
              <description>Capture/Compare 1
              selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCER</name>
          <displayName>CCER</displayName>
          <description>capture/compare enable
          register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>CC2NP</name>
              <description>Capture/Compare 2 output
              Polarity</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2P</name>
              <description>Capture/Compare 2 output
              Polarity</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC2E</name>
              <description>Capture/Compare 2 output
              enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1NP</name>
              <description>Capture/Compare 1 output
              Polarity</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1P</name>
              <description>Capture/Compare 1 output
              Polarity</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CC1E</name>
              <description>Capture/Compare 1 output
              enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CNT</name>
          <displayName>CNT</displayName>
          <description>counter</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CNT</name>
              <description>counter value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>PSC</name>
          <displayName>PSC</displayName>
          <description>prescaler</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>PSC</name>
              <description>Prescaler value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ARR</name>
          <displayName>ARR</displayName>
          <description>auto-reload register</description>
          <addressOffset>0x2C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ARR</name>
              <description>Auto-reload value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR1</name>
          <displayName>CCR1</displayName>
          <description>capture/compare register 1</description>
          <addressOffset>0x34</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CCR1</name>
              <description>Capture/Compare 1 value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR2</name>
          <displayName>CCR2</displayName>
          <description>capture/compare register 2</description>
          <addressOffset>0x38</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CCR2</name>
              <description>Capture/Compare 2 value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>USART1</name>
      <description>Universal synchronous asynchronous receiver
      transmitter</description>
      <groupName>USART</groupName>
      <baseAddress>0x40011000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>Status register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <resetValue>0x00C00000</resetValue>
          <fields>
            <field>
              <name>CTS</name>
              <description>CTS flag</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>LBD</name>
              <description>LIN break detection flag</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>TXE</name>
              <description>Transmit data register
              empty</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>TC</name>
              <description>Transmission complete</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>RXNE</name>
              <description>Read data register not
              empty</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>IDLE</name>
              <description>IDLE line detected</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>ORE</name>
              <description>Overrun error</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>NF</name>
              <description>Noise detected flag</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>FE</name>
              <description>Framing error</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>PE</name>
              <description>Parity error</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
          </fields>
        </register>
        <register>
          <name>DR</name>
          <displayName>DR</displayName>
          <description>Data register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DR</name>
              <description>Data value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>9</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BRR</name>
          <displayName>BRR</displayName>
          <description>Baud rate register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>DIV_Mantissa</name>
              <description>mantissa of USARTDIV</description>
              <bitOffset>4</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
            <field>
              <name>DIV_Fraction</name>
              <description>fraction of USARTDIV</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>Control register 1</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>OVER8</name>
              <description>Oversampling mode</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UE</name>
              <description>USART enable</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>M</name>
              <description>Word length</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WAKE</name>
              <description>Wakeup method</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PCE</name>
              <description>Parity control enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PS</name>
              <description>Parity selection</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PEIE</name>
              <description>PE interrupt enable</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TXEIE</name>
              <description>TXE interrupt enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIE</name>
              <description>Transmission complete interrupt
              enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RXNEIE</name>
              <description>RXNE interrupt enable</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDLEIE</name>
              <description>IDLE interrupt enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TE</name>
              <description>Transmitter enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RE</name>
              <description>Receiver enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RWU</name>
              <description>Receiver wakeup</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SBK</name>
              <description>Send break</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR2</name>
          <displayName>CR2</displayName>
          <description>Control register 2</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>LINEN</name>
              <description>LIN mode enable</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STOP</name>
              <description>STOP bits</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CLKEN</name>
              <description>Clock enable</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CPOL</name>
              <description>Clock polarity</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CPHA</name>
              <description>Clock phase</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LBCL</name>
              <description>Last bit clock pulse</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LBDIE</name>
              <description>LIN break detection interrupt
              enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LBDL</name>
              <description>lin break detection length</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ADD</name>
              <description>Address of the USART node</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR3</name>
          <displayName>CR3</displayName>
          <description>Control register 3</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>ONEBIT</name>
              <description>One sample bit method
              enable</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTSIE</name>
              <description>CTS interrupt enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTSE</name>
              <description>CTS enable</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RTSE</name>
              <description>RTS enable</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMAT</name>
              <description>DMA enable transmitter</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMAR</name>
              <description>DMA enable receiver</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SCEN</name>
              <description>Smartcard mode enable</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>NACK</name>
              <description>Smartcard NACK enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HDSEL</name>
              <description>Half-duplex selection</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IRLP</name>
              <description>IrDA low-power</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IREN</name>
              <description>IrDA mode enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EIE</name>
              <description>Error interrupt enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>GTPR</name>
          <displayName>GTPR</displayName>
          <description>Guard time and prescaler
          register</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>GT</name>
              <description>Guard time value</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>PSC</name>
              <description>Prescaler value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral derivedFrom="USART1">
      <name>USART2</name>
      <baseAddress>0x40004400</baseAddress>
    </peripheral>
    <peripheral derivedFrom="USART1">
      <name>USART6</name>
      <baseAddress>0x40011400</baseAddress>
    </peripheral>
    <peripheral>
      <name>WWDG</name>
      <description>Window watchdog</description>
      <groupName>WWDG</groupName>
      <baseAddress>0x40002C00</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>Control register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x7F</resetValue>
          <fields>
            <field>
              <name>WDGA</name>
              <description>Activation bit</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>T</name>
              <description>7-bit counter (MSB to LSB)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>7</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CFR</name>
          <displayName>CFR</displayName>
          <description>Configuration register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x7F</resetValue>
          <fields>
            <field>
              <name>EWI</name>
              <description>Early wakeup interrupt</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WDGTB1</name>
              <description>Timer base</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WDGTB0</name>
              <description>Timer base</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>W</name>
              <description>7-bit window value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>7</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>Status register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00</resetValue>
          <fields>
            <field>
              <name>EWIF</name>
              <description>Early wakeup interrupt
              flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>DMA2</name>
      <description>DMA controller</description>
      <groupName>DMA</groupName>
      <baseAddress>0x40026400</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>LISR</name>
          <displayName>LISR</displayName>
          <description>low interrupt status register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>TCIF3</name>
              <description>Stream x transfer complete interrupt
              flag (x = 3..0)</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIF3</name>
              <description>Stream x half transfer interrupt flag
              (x=3..0)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIF3</name>
              <description>Stream x transfer error interrupt flag
              (x=3..0)</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMEIF3</name>
              <description>Stream x direct mode error interrupt
              flag (x=3..0)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>FEIF3</name>
              <description>Stream x FIFO error interrupt flag
              (x=3..0)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIF2</name>
              <description>Stream x transfer complete interrupt
              flag (x = 3..0)</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIF2</name>
              <description>Stream x half transfer interrupt flag
              (x=3..0)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIF2</name>
              <description>Stream x transfer error interrupt flag
              (x=3..0)</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMEIF2</name>
              <description>Stream x direct mode error interrupt
              flag (x=3..0)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>FEIF2</name>
              <description>Stream x FIFO error interrupt flag
              (x=3..0)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIF1</name>
              <description>Stream x transfer complete interrupt
              flag (x = 3..0)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIF1</name>
              <description>Stream x half transfer interrupt flag
              (x=3..0)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIF1</name>
              <description>Stream x transfer error interrupt flag
              (x=3..0)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMEIF1</name>
              <description>Stream x direct mode error interrupt
              flag (x=3..0)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>FEIF1</name>
              <description>Stream x FIFO error interrupt flag
              (x=3..0)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIF0</name>
              <description>Stream x transfer complete interrupt
              flag (x = 3..0)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIF0</name>
              <description>Stream x half transfer interrupt flag
              (x=3..0)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIF0</name>
              <description>Stream x transfer error interrupt flag
              (x=3..0)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMEIF0</name>
              <description>Stream x direct mode error interrupt
              flag (x=3..0)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>FEIF0</name>
              <description>Stream x FIFO error interrupt flag
              (x=3..0)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>HISR</name>
          <displayName>HISR</displayName>
          <description>high interrupt status register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>TCIF7</name>
              <description>Stream x transfer complete interrupt
              flag (x=7..4)</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIF7</name>
              <description>Stream x half transfer interrupt flag
              (x=7..4)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIF7</name>
              <description>Stream x transfer error interrupt flag
              (x=7..4)</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMEIF7</name>
              <description>Stream x direct mode error interrupt
              flag (x=7..4)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>FEIF7</name>
              <description>Stream x FIFO error interrupt flag
              (x=7..4)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIF6</name>
              <description>Stream x transfer complete interrupt
              flag (x=7..4)</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIF6</name>
              <description>Stream x half transfer interrupt flag
              (x=7..4)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIF6</name>
              <description>Stream x transfer error interrupt flag
              (x=7..4)</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMEIF6</name>
              <description>Stream x direct mode error interrupt
              flag (x=7..4)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>FEIF6</name>
              <description>Stream x FIFO error interrupt flag
              (x=7..4)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIF5</name>
              <description>Stream x transfer complete interrupt
              flag (x=7..4)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIF5</name>
              <description>Stream x half transfer interrupt flag
              (x=7..4)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIF5</name>
              <description>Stream x transfer error interrupt flag
              (x=7..4)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMEIF5</name>
              <description>Stream x direct mode error interrupt
              flag (x=7..4)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>FEIF5</name>
              <description>Stream x FIFO error interrupt flag
              (x=7..4)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIF4</name>
              <description>Stream x transfer complete interrupt
              flag (x=7..4)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIF4</name>
              <description>Stream x half transfer interrupt flag
              (x=7..4)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIF4</name>
              <description>Stream x transfer error interrupt flag
              (x=7..4)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMEIF4</name>
              <description>Stream x direct mode error interrupt
              flag (x=7..4)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>FEIF4</name>
              <description>Stream x FIFO error interrupt flag
              (x=7..4)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>LIFCR</name>
          <displayName>LIFCR</displayName>
          <description>low interrupt flag clear
          register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CTCIF3</name>
              <description>Stream x clear transfer complete
              interrupt flag (x = 3..0)</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHTIF3</name>
              <description>Stream x clear half transfer interrupt
              flag (x = 3..0)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTEIF3</name>
              <description>Stream x clear transfer error interrupt
              flag (x = 3..0)</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CDMEIF3</name>
              <description>Stream x clear direct mode error
              interrupt flag (x = 3..0)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CFEIF3</name>
              <description>Stream x clear FIFO error interrupt flag
              (x = 3..0)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTCIF2</name>
              <description>Stream x clear transfer complete
              interrupt flag (x = 3..0)</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHTIF2</name>
              <description>Stream x clear half transfer interrupt
              flag (x = 3..0)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTEIF2</name>
              <description>Stream x clear transfer error interrupt
              flag (x = 3..0)</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CDMEIF2</name>
              <description>Stream x clear direct mode error
              interrupt flag (x = 3..0)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CFEIF2</name>
              <description>Stream x clear FIFO error interrupt flag
              (x = 3..0)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTCIF1</name>
              <description>Stream x clear transfer complete
              interrupt flag (x = 3..0)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHTIF1</name>
              <description>Stream x clear half transfer interrupt
              flag (x = 3..0)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTEIF1</name>
              <description>Stream x clear transfer error interrupt
              flag (x = 3..0)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CDMEIF1</name>
              <description>Stream x clear direct mode error
              interrupt flag (x = 3..0)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CFEIF1</name>
              <description>Stream x clear FIFO error interrupt flag
              (x = 3..0)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTCIF0</name>
              <description>Stream x clear transfer complete
              interrupt flag (x = 3..0)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHTIF0</name>
              <description>Stream x clear half transfer interrupt
              flag (x = 3..0)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTEIF0</name>
              <description>Stream x clear transfer error interrupt
              flag (x = 3..0)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CDMEIF0</name>
              <description>Stream x clear direct mode error
              interrupt flag (x = 3..0)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CFEIF0</name>
              <description>Stream x clear FIFO error interrupt flag
              (x = 3..0)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>HIFCR</name>
          <displayName>HIFCR</displayName>
          <description>high interrupt flag clear
          register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CTCIF7</name>
              <description>Stream x clear transfer complete
              interrupt flag (x = 7..4)</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHTIF7</name>
              <description>Stream x clear half transfer interrupt
              flag (x = 7..4)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTEIF7</name>
              <description>Stream x clear transfer error interrupt
              flag (x = 7..4)</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CDMEIF7</name>
              <description>Stream x clear direct mode error
              interrupt flag (x = 7..4)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CFEIF7</name>
              <description>Stream x clear FIFO error interrupt flag
              (x = 7..4)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTCIF6</name>
              <description>Stream x clear transfer complete
              interrupt flag (x = 7..4)</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHTIF6</name>
              <description>Stream x clear half transfer interrupt
              flag (x = 7..4)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTEIF6</name>
              <description>Stream x clear transfer error interrupt
              flag (x = 7..4)</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CDMEIF6</name>
              <description>Stream x clear direct mode error
              interrupt flag (x = 7..4)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CFEIF6</name>
              <description>Stream x clear FIFO error interrupt flag
              (x = 7..4)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTCIF5</name>
              <description>Stream x clear transfer complete
              interrupt flag (x = 7..4)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHTIF5</name>
              <description>Stream x clear half transfer interrupt
              flag (x = 7..4)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTEIF5</name>
              <description>Stream x clear transfer error interrupt
              flag (x = 7..4)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CDMEIF5</name>
              <description>Stream x clear direct mode error
              interrupt flag (x = 7..4)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CFEIF5</name>
              <description>Stream x clear FIFO error interrupt flag
              (x = 7..4)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTCIF4</name>
              <description>Stream x clear transfer complete
              interrupt flag (x = 7..4)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CHTIF4</name>
              <description>Stream x clear half transfer interrupt
              flag (x = 7..4)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CTEIF4</name>
              <description>Stream x clear transfer error interrupt
              flag (x = 7..4)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CDMEIF4</name>
              <description>Stream x clear direct mode error
              interrupt flag (x = 7..4)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CFEIF4</name>
              <description>Stream x clear FIFO error interrupt flag
              (x = 7..4)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S0CR</name>
          <displayName>S0CR</displayName>
          <description>stream x configuration
          register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CHSEL</name>
              <description>Channel selection</description>
              <bitOffset>25</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>MBURST</name>
              <description>Memory burst transfer
              configuration</description>
              <bitOffset>23</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PBURST</name>
              <description>Peripheral burst transfer
              configuration</description>
              <bitOffset>21</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CT</name>
              <description>Current target (only in double buffer
              mode)</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBM</name>
              <description>Double buffer mode</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PL</name>
              <description>Priority level</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PINCOS</name>
              <description>Peripheral increment offset
              size</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MSIZE</name>
              <description>Memory data size</description>
              <bitOffset>13</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PSIZE</name>
              <description>Peripheral data size</description>
              <bitOffset>11</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MINC</name>
              <description>Memory increment mode</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PINC</name>
              <description>Peripheral increment mode</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CIRC</name>
              <description>Circular mode</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DIR</name>
              <description>Data transfer direction</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PFCTRL</name>
              <description>Peripheral flow controller</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIE</name>
              <description>Transfer complete interrupt
              enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIE</name>
              <description>Half transfer interrupt
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIE</name>
              <description>Transfer error interrupt
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMEIE</name>
              <description>Direct mode error interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EN</name>
              <description>Stream enable / flag stream ready when
              read low</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S0NDTR</name>
          <displayName>S0NDTR</displayName>
          <description>stream x number of data
          register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>NDT</name>
              <description>Number of data items to
              transfer</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S0PAR</name>
          <displayName>S0PAR</displayName>
          <description>stream x peripheral address
          register</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PA</name>
              <description>Peripheral address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S0M0AR</name>
          <displayName>S0M0AR</displayName>
          <description>stream x memory 0 address
          register</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>M0A</name>
              <description>Memory 0 address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S0M1AR</name>
          <displayName>S0M1AR</displayName>
          <description>stream x memory 1 address
          register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>M1A</name>
              <description>Memory 1 address (used in case of Double
              buffer mode)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S0FCR</name>
          <displayName>S0FCR</displayName>
          <description>stream x FIFO control register</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000021</resetValue>
          <fields>
            <field>
              <name>FEIE</name>
              <description>FIFO error interrupt
              enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>FS</name>
              <description>FIFO status</description>
              <bitOffset>3</bitOffset>
              <bitWidth>3</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>DMDIS</name>
              <description>Direct mode disable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>FTH</name>
              <description>FIFO threshold selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
        <register>
          <name>S1CR</name>
          <displayName>S1CR</displayName>
          <description>stream x configuration
          register</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CHSEL</name>
              <description>Channel selection</description>
              <bitOffset>25</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>MBURST</name>
              <description>Memory burst transfer
              configuration</description>
              <bitOffset>23</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PBURST</name>
              <description>Peripheral burst transfer
              configuration</description>
              <bitOffset>21</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>ACK</name>
              <description>ACK</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CT</name>
              <description>Current target (only in double buffer
              mode)</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBM</name>
              <description>Double buffer mode</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PL</name>
              <description>Priority level</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PINCOS</name>
              <description>Peripheral increment offset
              size</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MSIZE</name>
              <description>Memory data size</description>
              <bitOffset>13</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PSIZE</name>
              <description>Peripheral data size</description>
              <bitOffset>11</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MINC</name>
              <description>Memory increment mode</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PINC</name>
              <description>Peripheral increment mode</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CIRC</name>
              <description>Circular mode</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DIR</name>
              <description>Data transfer direction</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PFCTRL</name>
              <description>Peripheral flow controller</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIE</name>
              <description>Transfer complete interrupt
              enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIE</name>
              <description>Half transfer interrupt
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIE</name>
              <description>Transfer error interrupt
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMEIE</name>
              <description>Direct mode error interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EN</name>
              <description>Stream enable / flag stream ready when
              read low</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S1NDTR</name>
          <displayName>S1NDTR</displayName>
          <description>stream x number of data
          register</description>
          <addressOffset>0x2C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>NDT</name>
              <description>Number of data items to
              transfer</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S1PAR</name>
          <displayName>S1PAR</displayName>
          <description>stream x peripheral address
          register</description>
          <addressOffset>0x30</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PA</name>
              <description>Peripheral address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S1M0AR</name>
          <displayName>S1M0AR</displayName>
          <description>stream x memory 0 address
          register</description>
          <addressOffset>0x34</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>M0A</name>
              <description>Memory 0 address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S1M1AR</name>
          <displayName>S1M1AR</displayName>
          <description>stream x memory 1 address
          register</description>
          <addressOffset>0x38</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>M1A</name>
              <description>Memory 1 address (used in case of Double
              buffer mode)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S1FCR</name>
          <displayName>S1FCR</displayName>
          <description>stream x FIFO control register</description>
          <addressOffset>0x3C</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000021</resetValue>
          <fields>
            <field>
              <name>FEIE</name>
              <description>FIFO error interrupt
              enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>FS</name>
              <description>FIFO status</description>
              <bitOffset>3</bitOffset>
              <bitWidth>3</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>DMDIS</name>
              <description>Direct mode disable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>FTH</name>
              <description>FIFO threshold selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
        <register>
          <name>S2CR</name>
          <displayName>S2CR</displayName>
          <description>stream x configuration
          register</description>
          <addressOffset>0x40</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CHSEL</name>
              <description>Channel selection</description>
              <bitOffset>25</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>MBURST</name>
              <description>Memory burst transfer
              configuration</description>
              <bitOffset>23</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PBURST</name>
              <description>Peripheral burst transfer
              configuration</description>
              <bitOffset>21</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>ACK</name>
              <description>ACK</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CT</name>
              <description>Current target (only in double buffer
              mode)</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBM</name>
              <description>Double buffer mode</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PL</name>
              <description>Priority level</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PINCOS</name>
              <description>Peripheral increment offset
              size</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MSIZE</name>
              <description>Memory data size</description>
              <bitOffset>13</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PSIZE</name>
              <description>Peripheral data size</description>
              <bitOffset>11</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MINC</name>
              <description>Memory increment mode</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PINC</name>
              <description>Peripheral increment mode</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CIRC</name>
              <description>Circular mode</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DIR</name>
              <description>Data transfer direction</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PFCTRL</name>
              <description>Peripheral flow controller</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIE</name>
              <description>Transfer complete interrupt
              enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIE</name>
              <description>Half transfer interrupt
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIE</name>
              <description>Transfer error interrupt
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMEIE</name>
              <description>Direct mode error interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EN</name>
              <description>Stream enable / flag stream ready when
              read low</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S2NDTR</name>
          <displayName>S2NDTR</displayName>
          <description>stream x number of data
          register</description>
          <addressOffset>0x44</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>NDT</name>
              <description>Number of data items to
              transfer</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S2PAR</name>
          <displayName>S2PAR</displayName>
          <description>stream x peripheral address
          register</description>
          <addressOffset>0x48</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PA</name>
              <description>Peripheral address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S2M0AR</name>
          <displayName>S2M0AR</displayName>
          <description>stream x memory 0 address
          register</description>
          <addressOffset>0x4C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>M0A</name>
              <description>Memory 0 address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S2M1AR</name>
          <displayName>S2M1AR</displayName>
          <description>stream x memory 1 address
          register</description>
          <addressOffset>0x50</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>M1A</name>
              <description>Memory 1 address (used in case of Double
              buffer mode)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S2FCR</name>
          <displayName>S2FCR</displayName>
          <description>stream x FIFO control register</description>
          <addressOffset>0x54</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000021</resetValue>
          <fields>
            <field>
              <name>FEIE</name>
              <description>FIFO error interrupt
              enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>FS</name>
              <description>FIFO status</description>
              <bitOffset>3</bitOffset>
              <bitWidth>3</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>DMDIS</name>
              <description>Direct mode disable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>FTH</name>
              <description>FIFO threshold selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
        <register>
          <name>S3CR</name>
          <displayName>S3CR</displayName>
          <description>stream x configuration
          register</description>
          <addressOffset>0x58</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CHSEL</name>
              <description>Channel selection</description>
              <bitOffset>25</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>MBURST</name>
              <description>Memory burst transfer
              configuration</description>
              <bitOffset>23</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PBURST</name>
              <description>Peripheral burst transfer
              configuration</description>
              <bitOffset>21</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>ACK</name>
              <description>ACK</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CT</name>
              <description>Current target (only in double buffer
              mode)</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBM</name>
              <description>Double buffer mode</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PL</name>
              <description>Priority level</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PINCOS</name>
              <description>Peripheral increment offset
              size</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MSIZE</name>
              <description>Memory data size</description>
              <bitOffset>13</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PSIZE</name>
              <description>Peripheral data size</description>
              <bitOffset>11</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MINC</name>
              <description>Memory increment mode</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PINC</name>
              <description>Peripheral increment mode</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CIRC</name>
              <description>Circular mode</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DIR</name>
              <description>Data transfer direction</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PFCTRL</name>
              <description>Peripheral flow controller</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIE</name>
              <description>Transfer complete interrupt
              enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIE</name>
              <description>Half transfer interrupt
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIE</name>
              <description>Transfer error interrupt
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMEIE</name>
              <description>Direct mode error interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EN</name>
              <description>Stream enable / flag stream ready when
              read low</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S3NDTR</name>
          <displayName>S3NDTR</displayName>
          <description>stream x number of data
          register</description>
          <addressOffset>0x5C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>NDT</name>
              <description>Number of data items to
              transfer</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S3PAR</name>
          <displayName>S3PAR</displayName>
          <description>stream x peripheral address
          register</description>
          <addressOffset>0x60</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PA</name>
              <description>Peripheral address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S3M0AR</name>
          <displayName>S3M0AR</displayName>
          <description>stream x memory 0 address
          register</description>
          <addressOffset>0x64</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>M0A</name>
              <description>Memory 0 address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S3M1AR</name>
          <displayName>S3M1AR</displayName>
          <description>stream x memory 1 address
          register</description>
          <addressOffset>0x68</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>M1A</name>
              <description>Memory 1 address (used in case of Double
              buffer mode)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S3FCR</name>
          <displayName>S3FCR</displayName>
          <description>stream x FIFO control register</description>
          <addressOffset>0x6C</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000021</resetValue>
          <fields>
            <field>
              <name>FEIE</name>
              <description>FIFO error interrupt
              enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>FS</name>
              <description>FIFO status</description>
              <bitOffset>3</bitOffset>
              <bitWidth>3</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>DMDIS</name>
              <description>Direct mode disable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>FTH</name>
              <description>FIFO threshold selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
        <register>
          <name>S4CR</name>
          <displayName>S4CR</displayName>
          <description>stream x configuration
          register</description>
          <addressOffset>0x70</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CHSEL</name>
              <description>Channel selection</description>
              <bitOffset>25</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>MBURST</name>
              <description>Memory burst transfer
              configuration</description>
              <bitOffset>23</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PBURST</name>
              <description>Peripheral burst transfer
              configuration</description>
              <bitOffset>21</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>ACK</name>
              <description>ACK</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CT</name>
              <description>Current target (only in double buffer
              mode)</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBM</name>
              <description>Double buffer mode</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PL</name>
              <description>Priority level</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PINCOS</name>
              <description>Peripheral increment offset
              size</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MSIZE</name>
              <description>Memory data size</description>
              <bitOffset>13</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PSIZE</name>
              <description>Peripheral data size</description>
              <bitOffset>11</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MINC</name>
              <description>Memory increment mode</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PINC</name>
              <description>Peripheral increment mode</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CIRC</name>
              <description>Circular mode</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DIR</name>
              <description>Data transfer direction</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PFCTRL</name>
              <description>Peripheral flow controller</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIE</name>
              <description>Transfer complete interrupt
              enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIE</name>
              <description>Half transfer interrupt
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIE</name>
              <description>Transfer error interrupt
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMEIE</name>
              <description>Direct mode error interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EN</name>
              <description>Stream enable / flag stream ready when
              read low</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S4NDTR</name>
          <displayName>S4NDTR</displayName>
          <description>stream x number of data
          register</description>
          <addressOffset>0x74</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>NDT</name>
              <description>Number of data items to
              transfer</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S4PAR</name>
          <displayName>S4PAR</displayName>
          <description>stream x peripheral address
          register</description>
          <addressOffset>0x78</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PA</name>
              <description>Peripheral address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S4M0AR</name>
          <displayName>S4M0AR</displayName>
          <description>stream x memory 0 address
          register</description>
          <addressOffset>0x7C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>M0A</name>
              <description>Memory 0 address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S4M1AR</name>
          <displayName>S4M1AR</displayName>
          <description>stream x memory 1 address
          register</description>
          <addressOffset>0x80</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>M1A</name>
              <description>Memory 1 address (used in case of Double
              buffer mode)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S4FCR</name>
          <displayName>S4FCR</displayName>
          <description>stream x FIFO control register</description>
          <addressOffset>0x84</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000021</resetValue>
          <fields>
            <field>
              <name>FEIE</name>
              <description>FIFO error interrupt
              enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>FS</name>
              <description>FIFO status</description>
              <bitOffset>3</bitOffset>
              <bitWidth>3</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>DMDIS</name>
              <description>Direct mode disable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>FTH</name>
              <description>FIFO threshold selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
        <register>
          <name>S5CR</name>
          <displayName>S5CR</displayName>
          <description>stream x configuration
          register</description>
          <addressOffset>0x88</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CHSEL</name>
              <description>Channel selection</description>
              <bitOffset>25</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>MBURST</name>
              <description>Memory burst transfer
              configuration</description>
              <bitOffset>23</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PBURST</name>
              <description>Peripheral burst transfer
              configuration</description>
              <bitOffset>21</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>ACK</name>
              <description>ACK</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CT</name>
              <description>Current target (only in double buffer
              mode)</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBM</name>
              <description>Double buffer mode</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PL</name>
              <description>Priority level</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PINCOS</name>
              <description>Peripheral increment offset
              size</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MSIZE</name>
              <description>Memory data size</description>
              <bitOffset>13</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PSIZE</name>
              <description>Peripheral data size</description>
              <bitOffset>11</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MINC</name>
              <description>Memory increment mode</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PINC</name>
              <description>Peripheral increment mode</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CIRC</name>
              <description>Circular mode</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DIR</name>
              <description>Data transfer direction</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PFCTRL</name>
              <description>Peripheral flow controller</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIE</name>
              <description>Transfer complete interrupt
              enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIE</name>
              <description>Half transfer interrupt
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIE</name>
              <description>Transfer error interrupt
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMEIE</name>
              <description>Direct mode error interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EN</name>
              <description>Stream enable / flag stream ready when
              read low</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S5NDTR</name>
          <displayName>S5NDTR</displayName>
          <description>stream x number of data
          register</description>
          <addressOffset>0x8C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>NDT</name>
              <description>Number of data items to
              transfer</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S5PAR</name>
          <displayName>S5PAR</displayName>
          <description>stream x peripheral address
          register</description>
          <addressOffset>0x90</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PA</name>
              <description>Peripheral address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S5M0AR</name>
          <displayName>S5M0AR</displayName>
          <description>stream x memory 0 address
          register</description>
          <addressOffset>0x94</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>M0A</name>
              <description>Memory 0 address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S5M1AR</name>
          <displayName>S5M1AR</displayName>
          <description>stream x memory 1 address
          register</description>
          <addressOffset>0x98</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>M1A</name>
              <description>Memory 1 address (used in case of Double
              buffer mode)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S5FCR</name>
          <displayName>S5FCR</displayName>
          <description>stream x FIFO control register</description>
          <addressOffset>0x9C</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000021</resetValue>
          <fields>
            <field>
              <name>FEIE</name>
              <description>FIFO error interrupt
              enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>FS</name>
              <description>FIFO status</description>
              <bitOffset>3</bitOffset>
              <bitWidth>3</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>DMDIS</name>
              <description>Direct mode disable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>FTH</name>
              <description>FIFO threshold selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
        <register>
          <name>S6CR</name>
          <displayName>S6CR</displayName>
          <description>stream x configuration
          register</description>
          <addressOffset>0xA0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CHSEL</name>
              <description>Channel selection</description>
              <bitOffset>25</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>MBURST</name>
              <description>Memory burst transfer
              configuration</description>
              <bitOffset>23</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PBURST</name>
              <description>Peripheral burst transfer
              configuration</description>
              <bitOffset>21</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>ACK</name>
              <description>ACK</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CT</name>
              <description>Current target (only in double buffer
              mode)</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBM</name>
              <description>Double buffer mode</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PL</name>
              <description>Priority level</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PINCOS</name>
              <description>Peripheral increment offset
              size</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MSIZE</name>
              <description>Memory data size</description>
              <bitOffset>13</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PSIZE</name>
              <description>Peripheral data size</description>
              <bitOffset>11</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MINC</name>
              <description>Memory increment mode</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PINC</name>
              <description>Peripheral increment mode</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CIRC</name>
              <description>Circular mode</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DIR</name>
              <description>Data transfer direction</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PFCTRL</name>
              <description>Peripheral flow controller</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIE</name>
              <description>Transfer complete interrupt
              enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIE</name>
              <description>Half transfer interrupt
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIE</name>
              <description>Transfer error interrupt
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMEIE</name>
              <description>Direct mode error interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EN</name>
              <description>Stream enable / flag stream ready when
              read low</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S6NDTR</name>
          <displayName>S6NDTR</displayName>
          <description>stream x number of data
          register</description>
          <addressOffset>0xA4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>NDT</name>
              <description>Number of data items to
              transfer</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S6PAR</name>
          <displayName>S6PAR</displayName>
          <description>stream x peripheral address
          register</description>
          <addressOffset>0xA8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PA</name>
              <description>Peripheral address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S6M0AR</name>
          <displayName>S6M0AR</displayName>
          <description>stream x memory 0 address
          register</description>
          <addressOffset>0xAC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>M0A</name>
              <description>Memory 0 address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S6M1AR</name>
          <displayName>S6M1AR</displayName>
          <description>stream x memory 1 address
          register</description>
          <addressOffset>0xB0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>M1A</name>
              <description>Memory 1 address (used in case of Double
              buffer mode)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S6FCR</name>
          <displayName>S6FCR</displayName>
          <description>stream x FIFO control register</description>
          <addressOffset>0xB4</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000021</resetValue>
          <fields>
            <field>
              <name>FEIE</name>
              <description>FIFO error interrupt
              enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>FS</name>
              <description>FIFO status</description>
              <bitOffset>3</bitOffset>
              <bitWidth>3</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>DMDIS</name>
              <description>Direct mode disable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>FTH</name>
              <description>FIFO threshold selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
        <register>
          <name>S7CR</name>
          <displayName>S7CR</displayName>
          <description>stream x configuration
          register</description>
          <addressOffset>0xB8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CHSEL</name>
              <description>Channel selection</description>
              <bitOffset>25</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>MBURST</name>
              <description>Memory burst transfer
              configuration</description>
              <bitOffset>23</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PBURST</name>
              <description>Peripheral burst transfer
              configuration</description>
              <bitOffset>21</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>ACK</name>
              <description>ACK</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CT</name>
              <description>Current target (only in double buffer
              mode)</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DBM</name>
              <description>Double buffer mode</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PL</name>
              <description>Priority level</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PINCOS</name>
              <description>Peripheral increment offset
              size</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MSIZE</name>
              <description>Memory data size</description>
              <bitOffset>13</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PSIZE</name>
              <description>Peripheral data size</description>
              <bitOffset>11</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MINC</name>
              <description>Memory increment mode</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PINC</name>
              <description>Peripheral increment mode</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CIRC</name>
              <description>Circular mode</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DIR</name>
              <description>Data transfer direction</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PFCTRL</name>
              <description>Peripheral flow controller</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIE</name>
              <description>Transfer complete interrupt
              enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HTIE</name>
              <description>Half transfer interrupt
              enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TEIE</name>
              <description>Transfer error interrupt
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMEIE</name>
              <description>Direct mode error interrupt
              enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EN</name>
              <description>Stream enable / flag stream ready when
              read low</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S7NDTR</name>
          <displayName>S7NDTR</displayName>
          <description>stream x number of data
          register</description>
          <addressOffset>0xBC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>NDT</name>
              <description>Number of data items to
              transfer</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S7PAR</name>
          <displayName>S7PAR</displayName>
          <description>stream x peripheral address
          register</description>
          <addressOffset>0xC0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PA</name>
              <description>Peripheral address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S7M0AR</name>
          <displayName>S7M0AR</displayName>
          <description>stream x memory 0 address
          register</description>
          <addressOffset>0xC4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>M0A</name>
              <description>Memory 0 address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S7M1AR</name>
          <displayName>S7M1AR</displayName>
          <description>stream x memory 1 address
          register</description>
          <addressOffset>0xC8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>M1A</name>
              <description>Memory 1 address (used in case of Double
              buffer mode)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>S7FCR</name>
          <displayName>S7FCR</displayName>
          <description>stream x FIFO control register</description>
          <addressOffset>0xCC</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000021</resetValue>
          <fields>
            <field>
              <name>FEIE</name>
              <description>FIFO error interrupt
              enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>FS</name>
              <description>FIFO status</description>
              <bitOffset>3</bitOffset>
              <bitWidth>3</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>DMDIS</name>
              <description>Direct mode disable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>FTH</name>
              <description>FIFO threshold selection</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral derivedFrom="DMA2">
      <name>DMA1</name>
      <baseAddress>0x40026000</baseAddress>
      <interrupt>
        <name>RTC_Alarm</name>
        <description>RTC Alarms (A and B) through EXTI line
        interrupt</description>
        <value>41</value>
      </interrupt>
    </peripheral>
    <peripheral>
      <name>GPIOH</name>
      <description>General-purpose I/Os</description>
      <groupName>GPIO</groupName>
      <baseAddress>0x40021C00</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>MODER</name>
          <displayName>MODER</displayName>
          <description>GPIO port mode register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>MODER15</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>30</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER14</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER13</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER12</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER11</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER10</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER9</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER8</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER7</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER6</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER5</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER4</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER3</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER2</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER1</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER0</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OTYPER</name>
          <displayName>OTYPER</displayName>
          <description>GPIO port output type register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OT15</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT14</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT13</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT12</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT11</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT10</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT9</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT8</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT7</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT6</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT5</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT4</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT3</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT2</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT1</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT0</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OSPEEDR</name>
          <displayName>OSPEEDR</displayName>
          <description>GPIO port output speed
          register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OSPEEDR15</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>30</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR14</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR13</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR12</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR11</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR10</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR9</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR8</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR7</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR6</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR5</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR4</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR3</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR2</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR1</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR0</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>PUPDR</name>
          <displayName>PUPDR</displayName>
          <description>GPIO port pull-up/pull-down
          register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PUPDR15</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>30</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR14</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR13</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR12</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR11</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR10</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR9</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR8</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR7</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR6</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR5</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR4</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR3</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR2</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR1</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR0</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IDR</name>
          <displayName>IDR</displayName>
          <description>GPIO port input data register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IDR15</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR14</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR13</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR12</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR11</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR10</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR9</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR8</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR7</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR6</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR5</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR4</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR3</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR2</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR1</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR0</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ODR</name>
          <displayName>ODR</displayName>
          <description>GPIO port output data register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ODR15</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR14</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR13</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR12</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR11</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR10</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR9</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR8</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR7</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR6</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR5</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR4</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR3</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR2</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR1</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR0</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BSRR</name>
          <displayName>BSRR</displayName>
          <description>GPIO port bit set/reset
          register</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BR15</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR14</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR13</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR12</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR11</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR10</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR9</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR8</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR7</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR6</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR5</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR4</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR3</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR2</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR1</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR0</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS15</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS14</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS13</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS12</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS11</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS10</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS9</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS8</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS7</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS6</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS5</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS4</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS3</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS2</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS1</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS0</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>LCKR</name>
          <displayName>LCKR</displayName>
          <description>GPIO port configuration lock
          register</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>LCKK</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK15</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK14</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK13</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK12</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK11</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK10</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK9</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK8</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK7</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK6</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK5</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK4</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK3</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK2</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK1</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK0</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>AFRL</name>
          <displayName>AFRL</displayName>
          <description>GPIO alternate function low
          register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>AFRL7</name>
              <description>Alternate function selection for port x
              bit y (y = 0..7)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRL6</name>
              <description>Alternate function selection for port x
              bit y (y = 0..7)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRL5</name>
              <description>Alternate function selection for port x
              bit y (y = 0..7)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRL4</name>
              <description>Alternate function selection for port x
              bit y (y = 0..7)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRL3</name>
              <description>Alternate function selection for port x
              bit y (y = 0..7)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRL2</name>
              <description>Alternate function selection for port x
              bit y (y = 0..7)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRL1</name>
              <description>Alternate function selection for port x
              bit y (y = 0..7)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRL0</name>
              <description>Alternate function selection for port x
              bit y (y = 0..7)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>AFRH</name>
          <displayName>AFRH</displayName>
          <description>GPIO alternate function high
          register</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>AFRH15</name>
              <description>Alternate function selection for port x
              bit y (y = 8..15)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRH14</name>
              <description>Alternate function selection for port x
              bit y (y = 8..15)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRH13</name>
              <description>Alternate function selection for port x
              bit y (y = 8..15)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRH12</name>
              <description>Alternate function selection for port x
              bit y (y = 8..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRH11</name>
              <description>Alternate function selection for port x
              bit y (y = 8..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRH10</name>
              <description>Alternate function selection for port x
              bit y (y = 8..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRH9</name>
              <description>Alternate function selection for port x
              bit y (y = 8..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRH8</name>
              <description>Alternate function selection for port x
              bit y (y = 8..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral derivedFrom="GPIOH">
      <name>GPIOC</name>
      <baseAddress>0x40020800</baseAddress>
    </peripheral>
    <peripheral>
      <name>GPIOB</name>
      <description>General-purpose I/Os</description>
      <groupName>GPIO</groupName>
      <baseAddress>0x40020400</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>MODER</name>
          <displayName>MODER</displayName>
          <description>GPIO port mode register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000280</resetValue>
          <fields>
            <field>
              <name>MODER15</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>30</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER14</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER13</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER12</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER11</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER10</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER9</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER8</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER7</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER6</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER5</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER4</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER3</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER2</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER1</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER0</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OTYPER</name>
          <displayName>OTYPER</displayName>
          <description>GPIO port output type register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OT15</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT14</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT13</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT12</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT11</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT10</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT9</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT8</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT7</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT6</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT5</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT4</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT3</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT2</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT1</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT0</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OSPEEDR</name>
          <displayName>OSPEEDR</displayName>
          <description>GPIO port output speed
          register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x000000C0</resetValue>
          <fields>
            <field>
              <name>OSPEEDR15</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>30</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR14</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR13</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR12</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR11</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR10</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR9</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR8</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR7</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR6</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR5</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR4</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR3</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR2</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR1</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR0</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>PUPDR</name>
          <displayName>PUPDR</displayName>
          <description>GPIO port pull-up/pull-down
          register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000100</resetValue>
          <fields>
            <field>
              <name>PUPDR15</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>30</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR14</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR13</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR12</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR11</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR10</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR9</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR8</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR7</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR6</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR5</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR4</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR3</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR2</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR1</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR0</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IDR</name>
          <displayName>IDR</displayName>
          <description>GPIO port input data register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IDR15</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR14</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR13</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR12</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR11</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR10</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR9</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR8</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR7</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR6</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR5</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR4</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR3</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR2</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR1</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR0</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ODR</name>
          <displayName>ODR</displayName>
          <description>GPIO port output data register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ODR15</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR14</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR13</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR12</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR11</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR10</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR9</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR8</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR7</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR6</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR5</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR4</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR3</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR2</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR1</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR0</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BSRR</name>
          <displayName>BSRR</displayName>
          <description>GPIO port bit set/reset
          register</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BR15</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR14</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR13</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR12</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR11</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR10</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR9</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR8</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR7</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR6</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR5</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR4</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR3</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR2</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR1</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR0</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS15</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS14</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS13</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS12</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS11</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS10</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS9</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS8</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS7</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS6</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS5</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS4</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS3</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS2</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS1</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS0</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>LCKR</name>
          <displayName>LCKR</displayName>
          <description>GPIO port configuration lock
          register</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>LCKK</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK15</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK14</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK13</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK12</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK11</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK10</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK9</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK8</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK7</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK6</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK5</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK4</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK3</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK2</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK1</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK0</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>AFRL</name>
          <displayName>AFRL</displayName>
          <description>GPIO alternate function low
          register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>AFRL7</name>
              <description>Alternate function selection for port x
              bit y (y = 0..7)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRL6</name>
              <description>Alternate function selection for port x
              bit y (y = 0..7)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRL5</name>
              <description>Alternate function selection for port x
              bit y (y = 0..7)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRL4</name>
              <description>Alternate function selection for port x
              bit y (y = 0..7)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRL3</name>
              <description>Alternate function selection for port x
              bit y (y = 0..7)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRL2</name>
              <description>Alternate function selection for port x
              bit y (y = 0..7)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRL1</name>
              <description>Alternate function selection for port x
              bit y (y = 0..7)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRL0</name>
              <description>Alternate function selection for port x
              bit y (y = 0..7)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>AFRH</name>
          <displayName>AFRH</displayName>
          <description>GPIO alternate function high
          register</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>AFRH15</name>
              <description>Alternate function selection for port x
              bit y (y = 8..15)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRH14</name>
              <description>Alternate function selection for port x
              bit y (y = 8..15)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRH13</name>
              <description>Alternate function selection for port x
              bit y (y = 8..15)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRH12</name>
              <description>Alternate function selection for port x
              bit y (y = 8..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRH11</name>
              <description>Alternate function selection for port x
              bit y (y = 8..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRH10</name>
              <description>Alternate function selection for port x
              bit y (y = 8..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRH9</name>
              <description>Alternate function selection for port x
              bit y (y = 8..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRH8</name>
              <description>Alternate function selection for port x
              bit y (y = 8..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>GPIOA</name>
      <description>General-purpose I/Os</description>
      <groupName>GPIO</groupName>
      <baseAddress>0x40020000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>MODER</name>
          <displayName>MODER</displayName>
          <description>GPIO port mode register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0xA8000000</resetValue>
          <fields>
            <field>
              <name>MODER15</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>30</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER14</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER13</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER12</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER11</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER10</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER9</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER8</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER7</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER6</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER5</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER4</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER3</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER2</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER1</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>MODER0</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OTYPER</name>
          <displayName>OTYPER</displayName>
          <description>GPIO port output type register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OT15</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT14</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT13</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT12</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT11</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT10</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT9</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT8</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT7</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT6</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT5</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT4</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT3</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT2</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT1</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OT0</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OSPEEDR</name>
          <displayName>OSPEEDR</displayName>
          <description>GPIO port output speed
          register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OSPEEDR15</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>30</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR14</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR13</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR12</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR11</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR10</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR9</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR8</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR7</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR6</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR5</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR4</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR3</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR2</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR1</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>OSPEEDR0</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>PUPDR</name>
          <displayName>PUPDR</displayName>
          <description>GPIO port pull-up/pull-down
          register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x64000000</resetValue>
          <fields>
            <field>
              <name>PUPDR15</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>30</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR14</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR13</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR12</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR11</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR10</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR9</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR8</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR7</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR6</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR5</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR4</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR3</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR2</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR1</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PUPDR0</name>
              <description>Port x configuration bits (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IDR</name>
          <displayName>IDR</displayName>
          <description>GPIO port input data register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IDR15</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR14</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR13</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR12</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR11</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR10</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR9</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR8</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR7</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR6</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR5</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR4</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR3</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR2</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR1</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>IDR0</name>
              <description>Port input data (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ODR</name>
          <displayName>ODR</displayName>
          <description>GPIO port output data register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ODR15</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR14</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR13</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR12</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR11</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR10</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR9</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR8</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR7</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR6</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR5</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR4</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR3</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR2</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR1</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODR0</name>
              <description>Port output data (y =
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>BSRR</name>
          <displayName>BSRR</displayName>
          <description>GPIO port bit set/reset
          register</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>BR15</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR14</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>30</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR13</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR12</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR11</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>27</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR10</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR9</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR8</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR7</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR6</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR5</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR4</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR3</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR2</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR1</name>
              <description>Port x reset bit y (y =
              0..15)</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR0</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS15</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS14</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS13</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS12</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS11</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS10</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS9</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS8</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS7</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS6</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS5</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS4</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS3</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS2</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS1</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BS0</name>
              <description>Port x set bit y (y=
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>LCKR</name>
          <displayName>LCKR</displayName>
          <description>GPIO port configuration lock
          register</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>LCKK</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK15</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK14</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK13</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK12</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK11</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK10</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK9</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK8</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK7</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK6</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK5</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK4</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK3</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK2</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK1</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LCK0</name>
              <description>Port x lock bit y (y=
              0..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>AFRL</name>
          <displayName>AFRL</displayName>
          <description>GPIO alternate function low
          register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>AFRL7</name>
              <description>Alternate function selection for port x
              bit y (y = 0..7)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRL6</name>
              <description>Alternate function selection for port x
              bit y (y = 0..7)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRL5</name>
              <description>Alternate function selection for port x
              bit y (y = 0..7)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRL4</name>
              <description>Alternate function selection for port x
              bit y (y = 0..7)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRL3</name>
              <description>Alternate function selection for port x
              bit y (y = 0..7)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRL2</name>
              <description>Alternate function selection for port x
              bit y (y = 0..7)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRL1</name>
              <description>Alternate function selection for port x
              bit y (y = 0..7)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRL0</name>
              <description>Alternate function selection for port x
              bit y (y = 0..7)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>AFRH</name>
          <displayName>AFRH</displayName>
          <description>GPIO alternate function high
          register</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>AFRH15</name>
              <description>Alternate function selection for port x
              bit y (y = 8..15)</description>
              <bitOffset>28</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRH14</name>
              <description>Alternate function selection for port x
              bit y (y = 8..15)</description>
              <bitOffset>24</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRH13</name>
              <description>Alternate function selection for port x
              bit y (y = 8..15)</description>
              <bitOffset>20</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRH12</name>
              <description>Alternate function selection for port x
              bit y (y = 8..15)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRH11</name>
              <description>Alternate function selection for port x
              bit y (y = 8..15)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRH10</name>
              <description>Alternate function selection for port x
              bit y (y = 8..15)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRH9</name>
              <description>Alternate function selection for port x
              bit y (y = 8..15)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>AFRH8</name>
              <description>Alternate function selection for port x
              bit y (y = 8..15)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>I2C2</name>
      <description>Inter-integrated circuit</description>
      <groupName>I2C</groupName>
      <baseAddress>0x40005800</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>I2C2_EV</name>
        <description>I2C2 event interrupt</description>
        <value>33</value>
      </interrupt>
      <interrupt>
        <name>I2C2_ER</name>
        <description>I2C2 error interrupt</description>
        <value>34</value>
      </interrupt>
      <registers>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>Control register 1</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>SWRST</name>
              <description>Software reset</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ALERT</name>
              <description>SMBus alert</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PEC</name>
              <description>Packet error checking</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>POS</name>
              <description>Acknowledge/PEC Position (for data
              reception)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ACK</name>
              <description>Acknowledge enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STOP</name>
              <description>Stop generation</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>START</name>
              <description>Start generation</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>NOSTRETCH</name>
              <description>Clock stretching disable (Slave
              mode)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ENGC</name>
              <description>General call enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ENPEC</name>
              <description>PEC enable</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ENARP</name>
              <description>ARP enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SMBTYPE</name>
              <description>SMBus type</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SMBUS</name>
              <description>SMBus mode</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PE</name>
              <description>Peripheral enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR2</name>
          <displayName>CR2</displayName>
          <description>Control register 2</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>LAST</name>
              <description>DMA last transfer</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMAEN</name>
              <description>DMA requests enable</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ITBUFEN</name>
              <description>Buffer interrupt enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ITEVTEN</name>
              <description>Event interrupt enable</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ITERREN</name>
              <description>Error interrupt enable</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>FREQ</name>
              <description>Peripheral clock frequency</description>
              <bitOffset>0</bitOffset>
              <bitWidth>6</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OAR1</name>
          <displayName>OAR1</displayName>
          <description>Own address register 1</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>ADDMODE</name>
              <description>Addressing mode (slave
              mode)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ADD10</name>
              <description>Interface address</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>ADD7</name>
              <description>Interface address</description>
              <bitOffset>1</bitOffset>
              <bitWidth>7</bitWidth>
            </field>
            <field>
              <name>ADD0</name>
              <description>Interface address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OAR2</name>
          <displayName>OAR2</displayName>
          <description>Own address register 2</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>ADD2</name>
              <description>Interface address</description>
              <bitOffset>1</bitOffset>
              <bitWidth>7</bitWidth>
            </field>
            <field>
              <name>ENDUAL</name>
              <description>Dual addressing mode
              enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DR</name>
          <displayName>DR</displayName>
          <description>Data register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>DR</name>
              <description>8-bit data register</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SR1</name>
          <displayName>SR1</displayName>
          <description>Status register 1</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>SMBALERT</name>
              <description>SMBus alert</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>TIMEOUT</name>
              <description>Timeout or Tlow error</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>PECERR</name>
              <description>PEC Error in reception</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>OVR</name>
              <description>Overrun/Underrun</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>AF</name>
              <description>Acknowledge failure</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>ARLO</name>
              <description>Arbitration lost (master
              mode)</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>BERR</name>
              <description>Bus error</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>TxE</name>
              <description>Data register empty
              (transmitters)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>RxNE</name>
              <description>Data register not empty
              (receivers)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>STOPF</name>
              <description>Stop detection (slave
              mode)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>ADD10</name>
              <description>10-bit header sent (Master
              mode)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>BTF</name>
              <description>Byte transfer finished</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>ADDR</name>
              <description>Address sent (master mode)/matched
              (slave mode)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>SB</name>
              <description>Start bit (Master mode)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
          </fields>
        </register>
        <register>
          <name>SR2</name>
          <displayName>SR2</displayName>
          <description>Status register 2</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>PEC</name>
              <description>acket error checking
              register</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>DUALF</name>
              <description>Dual flag (Slave mode)</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SMBHOST</name>
              <description>SMBus host header (Slave
              mode)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SMBDEFAULT</name>
              <description>SMBus device default address (Slave
              mode)</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>GENCALL</name>
              <description>General call address (Slave
              mode)</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TRA</name>
              <description>Transmitter/receiver</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BUSY</name>
              <description>Bus busy</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MSL</name>
              <description>Master/slave</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CCR</name>
          <displayName>CCR</displayName>
          <description>Clock control register</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>F_S</name>
              <description>I2C master mode selection</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DUTY</name>
              <description>Fast mode duty cycle</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CCR</name>
              <description>Clock control register in Fast/Standard
              mode (Master mode)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>TRISE</name>
          <displayName>TRISE</displayName>
          <description>TRISE register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0002</resetValue>
          <fields>
            <field>
              <name>TRISE</name>
              <description>Maximum rise time in Fast/Standard mode
              (Master mode)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>6</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral derivedFrom="I2C2">
      <name>I2C1</name>
      <baseAddress>0x40005400</baseAddress>
      <interrupt>
        <name>I2C1_EV</name>
        <description>I2C1 event interrupt</description>
        <value>31</value>
      </interrupt>
      <interrupt>
        <name>I2C1_ER</name>
        <description>I2C1 error interrupt</description>
        <value>32</value>
      </interrupt>
    </peripheral>
    <peripheral>
      <name>SPI1</name>
      <description>Serial peripheral interface</description>
      <groupName>SPI</groupName>
      <baseAddress>0x40013000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>SPI1</name>
        <description>SPI1 global interrupt</description>
        <value>35</value>
      </interrupt>
      <registers>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>control register 1</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>BIDIMODE</name>
              <description>Bidirectional data mode
              enable</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BIDIOE</name>
              <description>Output enable in bidirectional
              mode</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CRCEN</name>
              <description>Hardware CRC calculation
              enable</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CRCNEXT</name>
              <description>CRC transfer next</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DFF</name>
              <description>Data frame format</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RXONLY</name>
              <description>Receive only</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SSM</name>
              <description>Software slave management</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SSI</name>
              <description>Internal slave select</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>LSBFIRST</name>
              <description>Frame format</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SPE</name>
              <description>SPI enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BR</name>
              <description>Baud rate control</description>
              <bitOffset>3</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>MSTR</name>
              <description>Master selection</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CPOL</name>
              <description>Clock polarity</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CPHA</name>
              <description>Clock phase</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR2</name>
          <displayName>CR2</displayName>
          <description>control register 2</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>TXEIE</name>
              <description>Tx buffer empty interrupt
              enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RXNEIE</name>
              <description>RX buffer not empty interrupt
              enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ERRIE</name>
              <description>Error interrupt enable</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>FRF</name>
              <description>Frame format</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SSOE</name>
              <description>SS output enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TXDMAEN</name>
              <description>Tx buffer DMA enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RXDMAEN</name>
              <description>Rx buffer DMA enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>status register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <resetValue>0x0002</resetValue>
          <fields>
            <field>
              <name>TIFRFE</name>
              <description>TI frame format error</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>BSY</name>
              <description>Busy flag</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>OVR</name>
              <description>Overrun flag</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>MODF</name>
              <description>Mode fault</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>CRCERR</name>
              <description>CRC error flag</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>UDR</name>
              <description>Underrun flag</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>CHSIDE</name>
              <description>Channel side</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>TXE</name>
              <description>Transmit buffer empty</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>RXNE</name>
              <description>Receive buffer not empty</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
          </fields>
        </register>
        <register>
          <name>DR</name>
          <displayName>DR</displayName>
          <description>data register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>DR</name>
              <description>Data register</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CRCPR</name>
          <displayName>CRCPR</displayName>
          <description>CRC polynomial register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0007</resetValue>
          <fields>
            <field>
              <name>CRCPOLY</name>
              <description>CRC polynomial register</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>RXCRCR</name>
          <displayName>RXCRCR</displayName>
          <description>RX CRC register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>RxCRC</name>
              <description>Rx CRC register</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>TXCRCR</name>
          <displayName>TXCRCR</displayName>
          <description>TX CRC register</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>TxCRC</name>
              <description>Tx CRC register</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>I2SCFGR</name>
          <displayName>I2SCFGR</displayName>
          <description>I2S configuration register</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>I2SMOD</name>
              <description>I2S mode selection</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2SE</name>
              <description>I2S Enable</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2SCFG</name>
              <description>I2S configuration mode</description>
              <bitOffset>8</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>PCMSYNC</name>
              <description>PCM frame synchronization</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2SSTD</name>
              <description>I2S standard selection</description>
              <bitOffset>4</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CKPOL</name>
              <description>Steady state clock
              polarity</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DATLEN</name>
              <description>Data length to be
              transferred</description>
              <bitOffset>1</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CHLEN</name>
              <description>Channel length (number of bits per audio
              channel)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>I2SPR</name>
          <displayName>I2SPR</displayName>
          <description>I2S prescaler register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>00000010</resetValue>
          <fields>
            <field>
              <name>MCKOE</name>
              <description>Master clock output enable</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ODD</name>
              <description>Odd factor for the
              prescaler</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>I2SDIV</name>
              <description>I2S Linear prescaler</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral derivedFrom="SPI1">
      <name>SPI2</name>
      <baseAddress>0x40003800</baseAddress>
      <interrupt>
        <name>SPI2</name>
        <description>SPI2 global interrupt</description>
        <value>36</value>
      </interrupt>
    </peripheral>
    <peripheral derivedFrom="SPI1">
      <name>SPI5</name>
      <baseAddress>0x40015000</baseAddress>
    </peripheral>
    <peripheral>
      <name>NVIC</name>
      <description>Nested Vectored Interrupt
      Controller</description>
      <groupName>NVIC</groupName>
      <baseAddress>0xE000E000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x1001</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>ICTR</name>
          <displayName>ICTR</displayName>
          <description>Interrupt Controller Type
          Register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>INTLINESNUM</name>
              <description>Total number of interrupt lines in
              groups</description>
              <bitOffset>0</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>STIR</name>
          <displayName>STIR</displayName>
          <description>Software Triggered Interrupt
          Register</description>
          <addressOffset>0xF00</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>INTID</name>
              <description>interrupt to be triggered</description>
              <bitOffset>0</bitOffset>
              <bitWidth>9</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ISER0</name>
          <displayName>ISER0</displayName>
          <description>Interrupt Set-Enable Register</description>
          <addressOffset>0x100</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SETENA</name>
              <description>SETENA</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ISER1</name>
          <displayName>ISER1</displayName>
          <description>Interrupt Set-Enable Register</description>
          <addressOffset>0x104</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SETENA</name>
              <description>SETENA</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ISER2</name>
          <displayName>ISER2</displayName>
          <description>Interrupt Set-Enable Register</description>
          <addressOffset>0x108</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SETENA</name>
              <description>SETENA</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ICER0</name>
          <displayName>ICER0</displayName>
          <description>Interrupt Clear-Enable
          Register</description>
          <addressOffset>0x180</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CLRENA</name>
              <description>CLRENA</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ICER1</name>
          <displayName>ICER1</displayName>
          <description>Interrupt Clear-Enable
          Register</description>
          <addressOffset>0x184</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CLRENA</name>
              <description>CLRENA</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ICER2</name>
          <displayName>ICER2</displayName>
          <description>Interrupt Clear-Enable
          Register</description>
          <addressOffset>0x188</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CLRENA</name>
              <description>CLRENA</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ISPR0</name>
          <displayName>ISPR0</displayName>
          <description>Interrupt Set-Pending Register</description>
          <addressOffset>0x200</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SETPEND</name>
              <description>SETPEND</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ISPR1</name>
          <displayName>ISPR1</displayName>
          <description>Interrupt Set-Pending Register</description>
          <addressOffset>0x204</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SETPEND</name>
              <description>SETPEND</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ISPR2</name>
          <displayName>ISPR2</displayName>
          <description>Interrupt Set-Pending Register</description>
          <addressOffset>0x208</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SETPEND</name>
              <description>SETPEND</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ICPR0</name>
          <displayName>ICPR0</displayName>
          <description>Interrupt Clear-Pending
          Register</description>
          <addressOffset>0x280</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CLRPEND</name>
              <description>CLRPEND</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ICPR1</name>
          <displayName>ICPR1</displayName>
          <description>Interrupt Clear-Pending
          Register</description>
          <addressOffset>0x284</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CLRPEND</name>
              <description>CLRPEND</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ICPR2</name>
          <displayName>ICPR2</displayName>
          <description>Interrupt Clear-Pending
          Register</description>
          <addressOffset>0x288</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CLRPEND</name>
              <description>CLRPEND</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IABR0</name>
          <displayName>IABR0</displayName>
          <description>Interrupt Active Bit Register</description>
          <addressOffset>0x300</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ACTIVE</name>
              <description>ACTIVE</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IABR1</name>
          <displayName>IABR1</displayName>
          <description>Interrupt Active Bit Register</description>
          <addressOffset>0x304</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ACTIVE</name>
              <description>ACTIVE</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IABR2</name>
          <displayName>IABR2</displayName>
          <description>Interrupt Active Bit Register</description>
          <addressOffset>0x308</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ACTIVE</name>
              <description>ACTIVE</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR0</name>
          <displayName>IPR0</displayName>
          <description>Interrupt Priority Register</description>
          <addressOffset>0x400</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IPR_N0</name>
              <description>IPR_N0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N1</name>
              <description>IPR_N1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N2</name>
              <description>IPR_N2</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N3</name>
              <description>IPR_N3</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR1</name>
          <displayName>IPR1</displayName>
          <description>Interrupt Priority Register</description>
          <addressOffset>0x404</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IPR_N0</name>
              <description>IPR_N0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N1</name>
              <description>IPR_N1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N2</name>
              <description>IPR_N2</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N3</name>
              <description>IPR_N3</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR2</name>
          <displayName>IPR2</displayName>
          <description>Interrupt Priority Register</description>
          <addressOffset>0x408</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IPR_N0</name>
              <description>IPR_N0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N1</name>
              <description>IPR_N1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N2</name>
              <description>IPR_N2</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N3</name>
              <description>IPR_N3</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR3</name>
          <displayName>IPR3</displayName>
          <description>Interrupt Priority Register</description>
          <addressOffset>0x40C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IPR_N0</name>
              <description>IPR_N0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N1</name>
              <description>IPR_N1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N2</name>
              <description>IPR_N2</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N3</name>
              <description>IPR_N3</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR4</name>
          <displayName>IPR4</displayName>
          <description>Interrupt Priority Register</description>
          <addressOffset>0x410</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IPR_N0</name>
              <description>IPR_N0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N1</name>
              <description>IPR_N1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N2</name>
              <description>IPR_N2</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N3</name>
              <description>IPR_N3</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR5</name>
          <displayName>IPR5</displayName>
          <description>Interrupt Priority Register</description>
          <addressOffset>0x414</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IPR_N0</name>
              <description>IPR_N0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N1</name>
              <description>IPR_N1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N2</name>
              <description>IPR_N2</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N3</name>
              <description>IPR_N3</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR6</name>
          <displayName>IPR6</displayName>
          <description>Interrupt Priority Register</description>
          <addressOffset>0x418</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IPR_N0</name>
              <description>IPR_N0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N1</name>
              <description>IPR_N1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N2</name>
              <description>IPR_N2</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N3</name>
              <description>IPR_N3</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR7</name>
          <displayName>IPR7</displayName>
          <description>Interrupt Priority Register</description>
          <addressOffset>0x41C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IPR_N0</name>
              <description>IPR_N0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N1</name>
              <description>IPR_N1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N2</name>
              <description>IPR_N2</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N3</name>
              <description>IPR_N3</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR8</name>
          <displayName>IPR8</displayName>
          <description>Interrupt Priority Register</description>
          <addressOffset>0x420</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IPR_N0</name>
              <description>IPR_N0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N1</name>
              <description>IPR_N1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N2</name>
              <description>IPR_N2</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N3</name>
              <description>IPR_N3</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR9</name>
          <displayName>IPR9</displayName>
          <description>Interrupt Priority Register</description>
          <addressOffset>0x424</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IPR_N0</name>
              <description>IPR_N0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N1</name>
              <description>IPR_N1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N2</name>
              <description>IPR_N2</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N3</name>
              <description>IPR_N3</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR10</name>
          <displayName>IPR10</displayName>
          <description>Interrupt Priority Register</description>
          <addressOffset>0x428</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IPR_N0</name>
              <description>IPR_N0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N1</name>
              <description>IPR_N1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N2</name>
              <description>IPR_N2</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N3</name>
              <description>IPR_N3</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR11</name>
          <displayName>IPR11</displayName>
          <description>Interrupt Priority Register</description>
          <addressOffset>0x42C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IPR_N0</name>
              <description>IPR_N0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N1</name>
              <description>IPR_N1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N2</name>
              <description>IPR_N2</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N3</name>
              <description>IPR_N3</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR12</name>
          <displayName>IPR12</displayName>
          <description>Interrupt Priority Register</description>
          <addressOffset>0x430</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IPR_N0</name>
              <description>IPR_N0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N1</name>
              <description>IPR_N1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N2</name>
              <description>IPR_N2</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N3</name>
              <description>IPR_N3</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR13</name>
          <displayName>IPR13</displayName>
          <description>Interrupt Priority Register</description>
          <addressOffset>0x434</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IPR_N0</name>
              <description>IPR_N0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N1</name>
              <description>IPR_N1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N2</name>
              <description>IPR_N2</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N3</name>
              <description>IPR_N3</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR14</name>
          <displayName>IPR14</displayName>
          <description>Interrupt Priority Register</description>
          <addressOffset>0x438</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IPR_N0</name>
              <description>IPR_N0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N1</name>
              <description>IPR_N1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N2</name>
              <description>IPR_N2</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N3</name>
              <description>IPR_N3</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR15</name>
          <displayName>IPR15</displayName>
          <description>Interrupt Priority Register</description>
          <addressOffset>0x43C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IPR_N0</name>
              <description>IPR_N0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N1</name>
              <description>IPR_N1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N2</name>
              <description>IPR_N2</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N3</name>
              <description>IPR_N3</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR16</name>
          <displayName>IPR16</displayName>
          <description>Interrupt Priority Register</description>
          <addressOffset>0x440</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IPR_N0</name>
              <description>IPR_N0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N1</name>
              <description>IPR_N1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N2</name>
              <description>IPR_N2</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N3</name>
              <description>IPR_N3</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR17</name>
          <displayName>IPR17</displayName>
          <description>Interrupt Priority Register</description>
          <addressOffset>0x444</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IPR_N0</name>
              <description>IPR_N0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N1</name>
              <description>IPR_N1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N2</name>
              <description>IPR_N2</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N3</name>
              <description>IPR_N3</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR18</name>
          <displayName>IPR18</displayName>
          <description>Interrupt Priority Register</description>
          <addressOffset>0x448</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IPR_N0</name>
              <description>IPR_N0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N1</name>
              <description>IPR_N1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N2</name>
              <description>IPR_N2</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N3</name>
              <description>IPR_N3</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IPR19</name>
          <displayName>IPR19</displayName>
          <description>Interrupt Priority Register</description>
          <addressOffset>0x44C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IPR_N0</name>
              <description>IPR_N0</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N1</name>
              <description>IPR_N1</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N2</name>
              <description>IPR_N2</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>IPR_N3</name>
              <description>IPR_N3</description>
              <bitOffset>24</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>TIM6</name>
      <description>Basic timers</description>
      <groupName>TIM</groupName>
      <baseAddress>0x40001000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>TIM6_DAC1</name>
        <description>Timer6 and DAC1 global interrupt</description>
        <value>54</value>
      </interrupt>
      <registers>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>control register 1</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>ARPE</name>
              <description>Auto-reload preload enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OPM</name>
              <description>One-pulse mode</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>URS</name>
              <description>Update request source</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UDIS</name>
              <description>Update disable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CEN</name>
              <description>Counter enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR2</name>
          <displayName>CR2</displayName>
          <description>control register 2</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>MMS</name>
              <description>Master mode selection</description>
              <bitOffset>4</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DIER</name>
          <displayName>DIER</displayName>
          <description>DMA/Interrupt enable register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>UDE</name>
              <description>Update DMA request enable</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UIE</name>
              <description>Update interrupt enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>status register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>UIF</name>
              <description>Update interrupt flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>EGR</name>
          <displayName>EGR</displayName>
          <description>event generation register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>UG</name>
              <description>Update generation</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CNT</name>
          <displayName>CNT</displayName>
          <description>counter</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CNT</name>
              <description>Low counter value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>PSC</name>
          <displayName>PSC</displayName>
          <description>prescaler</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x0000</resetValue>
          <fields>
            <field>
              <name>PSC</name>
              <description>Prescaler value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ARR</name>
          <displayName>ARR</displayName>
          <description>auto-reload register</description>
          <addressOffset>0x2C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ARR</name>
              <description>Low Auto-reload value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>RNG</name>
      <description>Random number generator</description>
      <groupName>RNG</groupName>
      <baseAddress>0x40080000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>RNG</name>
        <description>RNG global interrupt</description>
        <value>80</value>
      </interrupt>
      <registers>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>control register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>IE</name>
              <description>Interrupt enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RNGEN</name>
              <description>Random number generator
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>status register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SEIS</name>
              <description>Seed error interrupt
              status</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>CEIS</name>
              <description>Clock error interrupt
              status</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>SECS</name>
              <description>Seed error current status</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>CECS</name>
              <description>Clock error current status</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>DRDY</name>
              <description>Data ready</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
          </fields>
        </register>
        <register>
          <name>DR</name>
          <displayName>DR</displayName>
          <description>data register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>RNDATA</name>
              <description>Random data</description>
              <bitOffset>0</bitOffset>
              <bitWidth>32</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>DAC</name>
      <description>Digital-to-analog converter</description>
      <groupName>DAC</groupName>
      <baseAddress>0x40007400</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <registers>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>control register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DMAUDRIE2</name>
              <description>DAC channel2 DMA underrun interrupt
              enable</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMAEN2</name>
              <description>DAC channel2 DMA enable</description>
              <bitOffset>28</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MAMP2</name>
              <description>DAC channel2 mask/amplitude
              selector</description>
              <bitOffset>24</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>WAVE2</name>
              <description>DAC channel2 noise/triangle wave
              generation enable</description>
              <bitOffset>22</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>TSEL2</name>
              <description>DAC channel2 trigger
              selection</description>
              <bitOffset>19</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>TEN2</name>
              <description>DAC channel2 trigger
              enable</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BOFF2</name>
              <description>DAC channel2 output buffer
              disable</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EN2</name>
              <description>DAC channel2 enable</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMAUDRIE1</name>
              <description>DAC channel1 DMA Underrun Interrupt
              enable</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMAEN1</name>
              <description>DAC channel1 DMA enable</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>MAMP1</name>
              <description>DAC channel1 mask/amplitude
              selector</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>WAVE1</name>
              <description>DAC channel1 noise/triangle wave
              generation enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>TSEL1</name>
              <description>DAC channel1 trigger
              selection</description>
              <bitOffset>3</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>TEN1</name>
              <description>DAC channel1 trigger
              enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BOFF1</name>
              <description>DAC channel1 output buffer
              disable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EN1</name>
              <description>DAC channel1 enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SWTRIGR</name>
          <displayName>SWTRIGR</displayName>
          <description>software trigger register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SWTRIG2</name>
              <description>DAC channel2 software
              trigger</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SWTRIG1</name>
              <description>DAC channel1 software
              trigger</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DHR12R1</name>
          <displayName>DHR12R1</displayName>
          <description>channel1 12-bit right-aligned data holding
          register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DACC1DHR</name>
              <description>DAC channel1 12-bit right-aligned
              data</description>
              <bitOffset>0</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DHR12L1</name>
          <displayName>DHR12L1</displayName>
          <description>channel1 12-bit left aligned data holding
          register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DACC1DHR</name>
              <description>DAC channel1 12-bit left-aligned
              data</description>
              <bitOffset>4</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DHR8R1</name>
          <displayName>DHR8R1</displayName>
          <description>channel1 8-bit right aligned data holding
          register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DACC1DHR</name>
              <description>DAC channel1 8-bit right-aligned
              data</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DHR12R2</name>
          <displayName>DHR12R2</displayName>
          <description>channel2 12-bit right aligned data holding
          register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DACC2DHR</name>
              <description>DAC channel2 12-bit right-aligned
              data</description>
              <bitOffset>0</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DHR12L2</name>
          <displayName>DHR12L2</displayName>
          <description>channel2 12-bit left aligned data holding
          register</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DACC2DHR</name>
              <description>DAC channel2 12-bit left-aligned
              data</description>
              <bitOffset>4</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DHR8R2</name>
          <displayName>DHR8R2</displayName>
          <description>channel2 8-bit right-aligned data holding
          register</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DACC2DHR</name>
              <description>DAC channel2 8-bit right-aligned
              data</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DHR12RD</name>
          <displayName>DHR12RD</displayName>
          <description>Dual DAC 12-bit right-aligned data holding
          register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DACC2DHR</name>
              <description>DAC channel2 12-bit right-aligned
              data</description>
              <bitOffset>16</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
            <field>
              <name>DACC1DHR</name>
              <description>DAC channel1 12-bit right-aligned
              data</description>
              <bitOffset>0</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DHR12LD</name>
          <displayName>DHR12LD</displayName>
          <description>DUAL DAC 12-bit left aligned data holding
          register</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DACC2DHR</name>
              <description>DAC channel2 12-bit left-aligned
              data</description>
              <bitOffset>20</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
            <field>
              <name>DACC1DHR</name>
              <description>DAC channel1 12-bit left-aligned
              data</description>
              <bitOffset>4</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DHR8RD</name>
          <displayName>DHR8RD</displayName>
          <description>DUAL DAC 8-bit right aligned data holding
          register</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DACC2DHR</name>
              <description>DAC channel2 8-bit right-aligned
              data</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>DACC1DHR</name>
              <description>DAC channel1 8-bit right-aligned
              data</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DOR1</name>
          <displayName>DOR1</displayName>
          <description>channel1 data output register</description>
          <addressOffset>0x2C</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DACC1DOR</name>
              <description>DAC channel1 data output</description>
              <bitOffset>0</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>DOR2</name>
          <displayName>DOR2</displayName>
          <description>channel2 data output register</description>
          <addressOffset>0x30</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DACC2DOR</name>
              <description>DAC channel2 data output</description>
              <bitOffset>0</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>SR</name>
          <displayName>SR</displayName>
          <description>status register</description>
          <addressOffset>0x34</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DMAUDR2</name>
              <description>DAC channel2 DMA underrun
              flag</description>
              <bitOffset>29</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DMAUDR1</name>
              <description>DAC channel1 DMA underrun
              flag</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>LPTIM1</name>
      <description>Low power timer</description>
      <groupName>LPTIM</groupName>
      <baseAddress>0x40002400</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>LPTIM1</name>
        <description>LPTimer global interrupt</description>
        <value>97</value>
      </interrupt>
      <registers>
        <register>
          <name>ISR</name>
          <displayName>ISR</displayName>
          <description>Interrupt and Status Register</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DOWN</name>
              <description>Counter direction change up to
              down</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UP</name>
              <description>Counter direction change down to
              up</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ARROK</name>
              <description>Autoreload register update
              OK</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CMPOK</name>
              <description>Compare register update OK</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EXTTRIG</name>
              <description>External trigger edge
              event</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ARRM</name>
              <description>Autoreload match</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CMPM</name>
              <description>Compare match</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ICR</name>
          <displayName>ICR</displayName>
          <description>Interrupt Clear Register</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DOWNCF</name>
              <description>Direction change to down Clear
              Flag</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UPCF</name>
              <description>Direction change to UP Clear
              Flag</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ARROKCF</name>
              <description>Autoreload register update OK Clear
              Flag</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CMPOKCF</name>
              <description>Compare register update OK Clear
              Flag</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EXTTRIGCF</name>
              <description>External trigger valid edge Clear
              Flag</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ARRMCF</name>
              <description>Autoreload match Clear
              Flag</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CMPMCF</name>
              <description>compare match Clear Flag</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>IER</name>
          <displayName>IER</displayName>
          <description>Interrupt Enable Register</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>DOWNIE</name>
              <description>Direction change to down Interrupt
              Enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>UPIE</name>
              <description>Direction change to UP Interrupt
              Enable</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ARROKIE</name>
              <description>Autoreload register update OK Interrupt
              Enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CMPOKIE</name>
              <description>Compare register update OK Interrupt
              Enable</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>EXTTRIGIE</name>
              <description>External trigger valid edge Interrupt
              Enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ARRMIE</name>
              <description>Autoreload match Interrupt
              Enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>CMPMIE</name>
              <description>Compare match Interrupt
              Enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CFGR</name>
          <displayName>CFGR</displayName>
          <description>Configuration Register</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ENC</name>
              <description>Encoder mode enable</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>COUNTMODE</name>
              <description>counter mode enabled</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PRELOAD</name>
              <description>Registers update mode</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WAVPOL</name>
              <description>Waveform shape polarity</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WAVE</name>
              <description>Waveform shape</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIMOUT</name>
              <description>Timeout enable</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TRIGEN</name>
              <description>Trigger enable and
              polarity</description>
              <bitOffset>17</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>TRIGSEL</name>
              <description>Trigger selector</description>
              <bitOffset>13</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>PRESC</name>
              <description>Clock prescaler</description>
              <bitOffset>9</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>TRGFLT</name>
              <description>Configurable digital filter for
              trigger</description>
              <bitOffset>6</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CKFLT</name>
              <description>Configurable digital filter for external
              clock</description>
              <bitOffset>3</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CKPOL</name>
              <description>Clock Polarity</description>
              <bitOffset>1</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
            <field>
              <name>CKSEL</name>
              <description>Clock selector</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR</name>
          <displayName>CR</displayName>
          <description>Control Register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CNTSTRT</name>
              <description>Timer start in continuous
              mode</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SNGSTRT</name>
              <description>LPTIM start in single mode</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ENABLE</name>
              <description>LPTIM Enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CMP</name>
          <displayName>CMP</displayName>
          <description>Compare Register</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CMP</name>
              <description>Compare value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ARR</name>
          <displayName>ARR</displayName>
          <description>Autoreload Register</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000001</resetValue>
          <fields>
            <field>
              <name>ARR</name>
              <description>Auto reload value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CNT</name>
          <displayName>CNT</displayName>
          <description>Counter Register</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>CNT</name>
              <description>Counter value</description>
              <bitOffset>0</bitOffset>
              <bitWidth>16</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OPTR</name>
          <displayName>OPTR</displayName>
          <description>Option Register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OR</name>
              <description>OR</description>
              <bitOffset>0</bitOffset>
              <bitWidth>2</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
    <peripheral>
      <name>I2C4</name>
      <description>Inter-integrated circuit</description>
      <groupName>I2C</groupName>
      <baseAddress>0x40006000</baseAddress>
      <addressBlock>
        <offset>0x0</offset>
        <size>0x400</size>
        <usage>registers</usage>
      </addressBlock>
      <interrupt>
        <name>I2C4_EV</name>
        <description>I2C4 event interrupt</description>
        <value>95</value>
      </interrupt>
      <interrupt>
        <name>I2C4_ER</name>
        <description>I2C2 error interrupt</description>
        <value>96</value>
      </interrupt>
      <registers>
        <register>
          <name>CR1</name>
          <displayName>CR1</displayName>
          <description>Control register 1</description>
          <addressOffset>0x0</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PE</name>
              <description>Peripheral enable</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TXIE</name>
              <description>TX Interrupt enable</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RXIE</name>
              <description>RX Interrupt enable</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ADDRIE</name>
              <description>Address match interrupt enable (slave
              only)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>NACKIE</name>
              <description>Not acknowledge received interrupt
              enable</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STOPIE</name>
              <description>STOP detection Interrupt
              enable</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TCIE</name>
              <description>Transfer Complete interrupt
              enable</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ERRIE</name>
              <description>Error interrupts enable</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>DNF</name>
              <description>Digital noise filter</description>
              <bitOffset>8</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>ANFOFF</name>
              <description>Analog noise filter OFF</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TXDMAEN</name>
              <description>DMA transmission requests
              enable</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RXDMAEN</name>
              <description>DMA reception requests
              enable</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SBC</name>
              <description>Slave byte control</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>NOSTRETCH</name>
              <description>Clock stretching disable</description>
              <bitOffset>17</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>WUPEN</name>
              <description>Wakeup from STOP enable</description>
              <bitOffset>18</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>GCEN</name>
              <description>General call enable</description>
              <bitOffset>19</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SMBHEN</name>
              <description>SMBus Host address enable</description>
              <bitOffset>20</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SMBDEN</name>
              <description>SMBus Device Default address
              enable</description>
              <bitOffset>21</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ALERTEN</name>
              <description>SMBUS alert enable</description>
              <bitOffset>22</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PECEN</name>
              <description>PEC enable</description>
              <bitOffset>23</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>CR2</name>
          <displayName>CR2</displayName>
          <description>Control register 2</description>
          <addressOffset>0x4</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PECBYTE</name>
              <description>Packet error checking byte</description>
              <bitOffset>26</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>AUTOEND</name>
              <description>Automatic end mode (master
              mode)</description>
              <bitOffset>25</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RELOAD</name>
              <description>NBYTES reload mode</description>
              <bitOffset>24</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>NBYTES</name>
              <description>Number of bytes</description>
              <bitOffset>16</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>NACK</name>
              <description>NACK generation (slave
              mode)</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STOP</name>
              <description>Stop generation (master
              mode)</description>
              <bitOffset>14</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>START</name>
              <description>Start generation</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>HEAD10R</name>
              <description>10-bit address header only read
              direction (master receiver mode)</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ADD10</name>
              <description>10-bit addressing mode (master
              mode)</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>RD_WRN</name>
              <description>Transfer direction (master
              mode)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>SADD</name>
              <description>Slave address bit (master
              mode)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>10</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OAR1</name>
          <displayName>OAR1</displayName>
          <description>Own address register 1</description>
          <addressOffset>0x8</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OA1</name>
              <description>Interface address</description>
              <bitOffset>0</bitOffset>
              <bitWidth>10</bitWidth>
            </field>
            <field>
              <name>OA1MODE</name>
              <description>Own Address 1 10-bit mode</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OA1EN</name>
              <description>Own Address 1 enable</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>OAR2</name>
          <displayName>OAR2</displayName>
          <description>Own address register 2</description>
          <addressOffset>0xC</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>OA2</name>
              <description>Interface address</description>
              <bitOffset>1</bitOffset>
              <bitWidth>7</bitWidth>
            </field>
            <field>
              <name>OA2MSK</name>
              <description>Own Address 2 masks</description>
              <bitOffset>8</bitOffset>
              <bitWidth>3</bitWidth>
            </field>
            <field>
              <name>OA2EN</name>
              <description>Own Address 2 enable</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>TIMINGR</name>
          <displayName>TIMINGR</displayName>
          <description>Timing register</description>
          <addressOffset>0x10</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>SCLL</name>
              <description>SCL low period (master
              mode)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>SCLH</name>
              <description>SCL high period (master
              mode)</description>
              <bitOffset>8</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
            <field>
              <name>SDADEL</name>
              <description>Data hold time</description>
              <bitOffset>16</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>SCLDEL</name>
              <description>Data setup time</description>
              <bitOffset>20</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
            <field>
              <name>PRESC</name>
              <description>Timing prescaler</description>
              <bitOffset>28</bitOffset>
              <bitWidth>4</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>TIMEOUTR</name>
          <displayName>TIMEOUTR</displayName>
          <description>Status register 1</description>
          <addressOffset>0x14</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>TIMEOUTA</name>
              <description>Bus timeout A</description>
              <bitOffset>0</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
            <field>
              <name>TIDLE</name>
              <description>Idle clock timeout
              detection</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIMOUTEN</name>
              <description>Clock timeout enable</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIMEOUTB</name>
              <description>Bus timeout B</description>
              <bitOffset>16</bitOffset>
              <bitWidth>12</bitWidth>
            </field>
            <field>
              <name>TEXTEN</name>
              <description>Extended clock timeout
              enable</description>
              <bitOffset>31</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>ISR</name>
          <displayName>ISR</displayName>
          <description>Interrupt and Status register</description>
          <addressOffset>0x18</addressOffset>
          <size>0x20</size>
          <resetValue>0x00000001</resetValue>
          <fields>
            <field>
              <name>ADDCODE</name>
              <description>Address match code (Slave
              mode)</description>
              <bitOffset>17</bitOffset>
              <bitWidth>7</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>DIR</name>
              <description>Transfer direction (Slave
              mode)</description>
              <bitOffset>16</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>BUSY</name>
              <description>Bus busy</description>
              <bitOffset>15</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>ALERT</name>
              <description>SMBus alert</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>TIMEOUT</name>
              <description>Timeout or t_low detection
              flag</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>PECERR</name>
              <description>PEC Error in reception</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>OVR</name>
              <description>Overrun/Underrun (slave
              mode)</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>ARLO</name>
              <description>Arbitration lost</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>BERR</name>
              <description>Bus error</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>TCR</name>
              <description>Transfer Complete Reload</description>
              <bitOffset>7</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>TC</name>
              <description>Transfer Complete (master
              mode)</description>
              <bitOffset>6</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>STOPF</name>
              <description>Stop detection flag</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>NACKF</name>
              <description>Not acknowledge received
              flag</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>ADDR</name>
              <description>Address matched (slave
              mode)</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>RXNE</name>
              <description>Receive data register not empty
              (receivers)</description>
              <bitOffset>2</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-only</access>
            </field>
            <field>
              <name>TXIS</name>
              <description>Transmit interrupt status
              (transmitters)</description>
              <bitOffset>1</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
            <field>
              <name>TXE</name>
              <description>Transmit data register empty
              (transmitters)</description>
              <bitOffset>0</bitOffset>
              <bitWidth>1</bitWidth>
              <access>read-write</access>
            </field>
          </fields>
        </register>
        <register>
          <name>ICR</name>
          <displayName>ICR</displayName>
          <description>Interrupt clear register</description>
          <addressOffset>0x1C</addressOffset>
          <size>0x20</size>
          <access>write-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>ALERTCF</name>
              <description>Alert flag clear</description>
              <bitOffset>13</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>TIMOUTCF</name>
              <description>Timeout detection flag
              clear</description>
              <bitOffset>12</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>PECCF</name>
              <description>PEC Error flag clear</description>
              <bitOffset>11</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>OVRCF</name>
              <description>Overrun/Underrun flag
              clear</description>
              <bitOffset>10</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ARLOCF</name>
              <description>Arbitration lost flag
              clear</description>
              <bitOffset>9</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>BERRCF</name>
              <description>Bus error flag clear</description>
              <bitOffset>8</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>STOPCF</name>
              <description>Stop detection flag clear</description>
              <bitOffset>5</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>NACKCF</name>
              <description>Not Acknowledge flag clear</description>
              <bitOffset>4</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
            <field>
              <name>ADDRCF</name>
              <description>Address Matched flag clear</description>
              <bitOffset>3</bitOffset>
              <bitWidth>1</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>PECR</name>
          <displayName>PECR</displayName>
          <description>PEC register</description>
          <addressOffset>0x20</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>PEC</name>
              <description>Packet error checking
              register</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>RXDR</name>
          <displayName>RXDR</displayName>
          <description>Receive data register</description>
          <addressOffset>0x24</addressOffset>
          <size>0x20</size>
          <access>read-only</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>RXDATA</name>
              <description>8-bit receive data</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
        <register>
          <name>TXDR</name>
          <displayName>TXDR</displayName>
          <description>Transmit data register</description>
          <addressOffset>0x28</addressOffset>
          <size>0x20</size>
          <access>read-write</access>
          <resetValue>0x00000000</resetValue>
          <fields>
            <field>
              <name>TXDATA</name>
              <description>8-bit transmit data</description>
              <bitOffset>0</bitOffset>
              <bitWidth>8</bitWidth>
            </field>
          </fields>
        </register>
      </registers>
    </peripheral>
  </peripherals>
</device>
